* Freescale i.MX Universal Asynchronous Receiver/Transmitter (UART)

Required properties:
- compatible : Should be "fsl,<soc>-uart"
- reg : Address and length of the register set for the device
- interrupts : Should contain uart interrupt

Optional properties:
- fsl,uart-has-rtscts : Indicate the uart has rts and cts
- fsl,irda-mode : Indicate the uart supports irda mode

Example:

serial@73fbc000 {
	compatible = "fsl,imx51-uart", "fsl,imx21-uart";
	reg = <0x73fbc000 0x4000>;
	interrupts = <31>;
	fsl,uart-has-rtscts;
};
