What:		/sys/bus/iio/devices/iio:deviceX
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Hardware chip or device accessed by one communication port.
		Corresponds to a grouping of sensor channels. X is the IIO
		index of the device.

What:		/sys/bus/iio/devices/triggerX
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		An event driven driver of data capture to an in kernel buffer.
		May be provided by a device driver that also has an IIO device
		based on hardware generated events (e.g. data ready) or
		provided by a separate driver for other hardware (e.g.
		periodic timer, GPIO or high resolution timer).
		Contains trigger type specific elements. These do not
		generalize well and hence are not documented in this file.
		X is the IIO index of the trigger.

What:		/sys/bus/iio/devices/iio:deviceX/buffer
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Directory of attributes relating to the buffer for the device.

What:		/sys/bus/iio/devices/iio:deviceX/name
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Description of the physical chip / device for device X.
		Typically a part number.

What:		/sys/bus/iio/devices/iio:deviceX/sampling_frequency
What:		/sys/bus/iio/devices/iio:deviceX/buffer/sampling_frequency
What:		/sys/bus/iio/devices/triggerX/sampling_frequency
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Some devices have internal clocks.  This parameter sets the
		resulting sampling frequency.  In many devices this
		parameter has an effect on input filters etc rather than
		simply controlling when the input is sampled.  As this
		effects datardy triggers, hardware buffers and the sysfs
		direct access interfaces, it may be found in any of the
		relevant directories.  If it effects all of the above
		then it is to be found in the base device directory.

What:		/sys/bus/iio/devices/iio:deviceX/sampling_frequency_available
What:		/sys/.../iio:deviceX/buffer/sampling_frequency_available
What:		/sys/bus/iio/devices/triggerX/sampling_frequency_available
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		When the internal sampling clock can only take a small
		discrete set of values, this file lists those available.

What:		/sys/bus/iio/devices/iio:deviceX/oversampling_ratio
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		Hardware dependent ADC oversampling. Controls the sampling ratio
		of the digital filter if available.

What:		/sys/bus/iio/devices/iio:deviceX/oversampling_ratio_available
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		Hardware dependent values supported by the oversampling filter.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_supply_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Raw (unscaled no bias removal etc) voltage measurement from
		channel Y. In special cases where the channel does not
		correspond to externally available input one of the named
		versions may be used. The number must always be specified and
		unique to allow association with event codes. Units after
		application of scale and offset are microvolts.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY-voltageZ_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Raw (unscaled) differential voltage measurement equivalent to
		channel Y - channel Z where these channel numbers apply to the
		physically equivalent inputs when non differential readings are
		separately available. In differential only parts, then all that
		is required is a consistent labeling.  Units after application
		of scale and offset are microvolts.

What:		/sys/bus/iio/devices/iio:deviceX/in_capacitanceY_raw
KernelVersion:	3.2
Contact:	linux-iio@vger.kernel.org
Description:
		Raw capacitance measurement from channel Y. Units after
		application of scale and offset are nanofarads.

What:		/sys/.../iio:deviceX/in_capacitanceY-in_capacitanceZ_raw
KernelVersion:	3.2
Contact:	linux-iio@vger.kernel.org
Description:
		Raw differential capacitance measurement equivalent to
		channel Y - channel Z where these channel numbers apply to the
		physically equivalent inputs when non differential readings are
		separately available. In differential only parts, then all that
		is required is a consistent labeling.  Units after application
		of scale and offset are nanofarads.

What:		/sys/bus/iio/devices/iio:deviceX/in_temp_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_tempX_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_temp_x_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_temp_y_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_temp_z_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Raw (unscaled no bias removal etc) temperature measurement.
		If an axis is specified it generally means that the temperature
		sensor is associated with one part of a compound device (e.g.
		a gyroscope axis). Units after application of scale and offset
		are milli degrees Celsuis.

What:		/sys/bus/iio/devices/iio:deviceX/in_tempX_input
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		Scaled temperature measurement in milli degrees Celsius.

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_x_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_y_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_z_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Acceleration in direction x, y or z (may be arbitrarily assigned
		but should match other such assignments on device).
		Has all of the equivalent parameters as per voltageY. Units
		after application of scale and offset are m/s^2.

What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_x_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_y_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_z_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Angular velocity about axis x, y or z (may be arbitrarily
		assigned) Data converted by application of offset then scale to
		radians per second. Has all the equivalent parameters as
		per voltageY. Units after application of scale and offset are
		radians per second.

What:		/sys/bus/iio/devices/iio:deviceX/in_incli_x_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_incli_y_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_incli_z_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Inclination raw reading about axis x, y or z (may be
		arbitrarily assigned). Data converted by application of offset
		and scale to Degrees.

What:		/sys/bus/iio/devices/iio:deviceX/in_magn_x_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_magn_y_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_magn_z_raw
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Magnetic field along axis x, y or z (may be arbitrarily
		assigned).  Data converted by application of offset
		then scale to Gauss.

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_x_peak_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_y_peak_raw
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_z_peak_raw
KernelVersion:	2.6.36
Contact:	linux-iio@vger.kernel.org
Description:
		Highest value since some reset condition.  These
		attributes allow access to this and are otherwise
		the direct equivalent of the <type>Y[_name]_raw attributes.

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_xyz_squared_peak_raw
KernelVersion:	2.6.36
Contact:	linux-iio@vger.kernel.org
Description:
		A computed peak value based on the sum squared magnitude of
		the underlying value in the specified directions.

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_x_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_y_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_z_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_voltage_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_tempY_offset
What:		/sys/bus/iio/devices/iio:deviceX/in_temp_offset
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		If known for a device, offset to be added to <type>[Y]_raw prior
		to scaling by <type>[Y]_scale in order to obtain value in the
		<type> units as specified in <type>[y]_raw documentation.
		Not present if the offset is always 0 or unknown. If Y or
		axis <x|y|z> is not present, then the offset applies to all
		in channels of <type>.
		May be writable if a variable offset can be applied on the
		device. Note that this is different to calibbias which
		is for devices (or drivers) that apply offsets to compensate
		for variation between different instances of the part, typically
		adjusted by using some hardware supported calibration procedure.
		Calibbias is applied internally, offset is applied in userspace
		to the _raw output.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_supply_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_voltage_scale
What:		/sys/bus/iio/devices/iio:deviceX/out_voltageY_scale
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_peak_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_magn_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_magn_x_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_magn_y_scale
What:		/sys/bus/iio/devices/iio:deviceX/in_magn_z_scale
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		If known for a device, scale to be applied to <type>Y[_name]_raw
		post addition of <type>[Y][_name]_offset in order to obtain the
		measured value in <type> units as specified in
		<type>[Y][_name]_raw documentation.  If shared across all in
		channels then Y and <x|y|z> are not present and the value is
		called <type>[Y][_name]_scale. The peak modifier means this
		value is applied to <type>Y[_name]_peak_raw values.

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_x_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_y_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_z_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_x_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_y_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_z_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_illuminance0_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_proximity0_calibbias
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Hardware applied calibration offset. (assumed to fix production
		inaccuracies).

What		/sys/bus/iio/devices/iio:deviceX/in_voltageY_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_voltageY_supply_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_voltage_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_accel_x_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_accel_y_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_accel_z_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_anglvel_x_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_anglvel_y_calibscale
What		/sys/bus/iio/devices/iio:deviceX/in_anglvel_z_calibscale
what		/sys/bus/iio/devices/iio:deviceX/in_illuminance0_calibscale
what		/sys/bus/iio/devices/iio:deviceX/in_proximity0_calibscale
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Hardware applied calibration scale factor. (assumed to fix
		production inaccuracies).  If shared across all channels,
		<type>_calibscale is used.

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_scale_available
What:		/sys/.../iio:deviceX/in_voltageX_scale_available
What:		/sys/.../iio:deviceX/in_voltage-voltage_scale_available
What:		/sys/.../iio:deviceX/out_voltageX_scale_available
What:		/sys/.../iio:deviceX/out_altvoltageX_scale_available
What:		/sys/.../iio:deviceX/in_capacitance_scale_available
KernelVersion:	2.635
Contact:	linux-iio@vger.kernel.org
Description:
		If a discrete set of scale values are available, they
		are listed in this attribute.

What		/sys/bus/iio/devices/iio:deviceX/out_voltageY_hardwaregain
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Hardware applied gain factor. If shared across all channels,
		<type>_hardwaregain is used.

What:		/sys/.../in_accel_filter_low_pass_3db_frequency
What:		/sys/.../in_magn_filter_low_pass_3db_frequency
What:		/sys/.../in_anglvel_filter_low_pass_3db_frequency
KernelVersion:	3.2
Contact:	linux-iio@vger.kernel.org
Description:
		If a known or controllable low pass filter is applied
		to the underlying data channel, then this parameter
		gives the 3dB frequency of the filter in Hz.

What:		/sys/bus/iio/devices/iio:deviceX/out_voltageY_raw
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY_raw
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Raw (unscaled, no bias etc.) output voltage for
		channel Y.  The number must always be specified and
		unique if the output corresponds to a single channel.
		While DAC like devices typically use out_voltage,
		a continuous frequency generating device, such as
		a DDS or PLL should use out_altvoltage.

What:		/sys/bus/iio/devices/iio:deviceX/out_voltageY&Z_raw
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY&Z_raw
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Raw (unscaled, no bias etc.) output voltage for an aggregate of
		channel Y, channel Z, etc.  This interface is available in cases
		where a single output sets the value for multiple channels
		simultaneously.

What:		/sys/bus/iio/devices/iio:deviceX/out_voltageY_powerdown_mode
What:		/sys/bus/iio/devices/iio:deviceX/out_voltage_powerdown_mode
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY_powerdown_mode
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltage_powerdown_mode
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		Specifies the output powerdown mode.
		DAC output stage is disconnected from the amplifier and
		1kohm_to_gnd: connected to ground via an 1kOhm resistor
		100kohm_to_gnd: connected to ground via an 100kOhm resistor
		three_state: left floating
		For a list of available output power down options read
		outX_powerdown_mode_available. If Y is not present the
		mode is shared across all outputs.

What:		/sys/.../iio:deviceX/out_votlageY_powerdown_mode_available
What:		/sys/.../iio:deviceX/out_voltage_powerdown_mode_available
What:		/sys/.../iio:deviceX/out_altvotlageY_powerdown_mode_available
What:		/sys/.../iio:deviceX/out_altvoltage_powerdown_mode_available
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		Lists all available output power down modes.
		If Y is not present the mode is shared across all outputs.

What:		/sys/bus/iio/devices/iio:deviceX/out_voltageY_powerdown
What:		/sys/bus/iio/devices/iio:deviceX/out_voltage_powerdown
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY_powerdown
What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltage_powerdown
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		Writing 1 causes output Y to enter the power down mode specified
		by the corresponding outY_powerdown_mode. Clearing returns to
		normal operation. Y may be suppressed if all outputs are
		controlled together.

What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY_frequency
KernelVersion:	3.4.0
Contact:	linux-iio@vger.kernel.org
Description:
		Output frequency for channel Y in Hz. The number must always be
		specified and unique if the output corresponds to a single
		channel.

What:		/sys/bus/iio/devices/iio:deviceX/out_altvoltageY_phase
KernelVersion:	3.4.0
Contact:	linux-iio@vger.kernel.org
Description:
		Phase in radians of one frequency/clock output Y
		(out_altvoltageY) relative to another frequency/clock output
		(out_altvoltageZ) of the device X. The number must always be
		specified and unique if the output corresponds to a single
		channel.

What:		/sys/bus/iio/devices/iio:deviceX/events
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Configuration of which hardware generated events are passed up
		to user-space.

What:		/sys/.../iio:deviceX/events/in_accel_x_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_x_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_y_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_y_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_z_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_z_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_anglvel_x_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_anglvel_x_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_anglvel_y_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_anglvel_y_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_anglvel_z_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_anglvel_z_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_magn_x_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_magn_x_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_magn_y_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_magn_y_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_magn_z_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_magn_z_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_voltageY_supply_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_voltageY_supply_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_voltageY_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_voltageY_thresh_falling_en
What:		/sys/.../iio:deviceX/events/in_tempY_thresh_rising_en
What:		/sys/.../iio:deviceX/events/in_tempY_thresh_falling_en
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Event generated when channel passes a threshold in the specified
		(_rising|_falling) direction. If the direction is not specified,
		then either the device will report an event which ever direction
		a single threshold value is passed in (e.g.
		<type>[Y][_name]_<raw|input>_thresh_value) or
		<type>[Y][_name]_<raw|input>_thresh_rising_value and
		<type>[Y][_name]_<raw|input>_thresh_falling_value may take
		different values, but the device can only enable both thresholds
		or neither.
		Note the driver will assume the last p events requested are
		to be enabled where p is however many it supports (which may
		vary depending on the exact set requested. So if you want to be
		sure you have set what you think you have, check the contents of
		these attributes after everything is configured. Drivers may
		have to buffer any parameters so that they are consistent when
		a given event type is enabled a future point (and not those for
		whatever event was previously enabled).

What:		/sys/.../iio:deviceX/events/in_accel_x_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_x_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_y_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_y_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_z_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_z_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_anglvel_x_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_anglvel_x_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_anglvel_y_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_anglvel_y_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_anglvel_z_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_anglvel_z_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_magn_x_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_magn_x_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_magn_y_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_magn_y_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_magn_z_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_magn_z_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_voltageY_supply_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_voltageY_supply_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_voltageY_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_voltageY_roc_falling_en
What:		/sys/.../iio:deviceX/events/in_tempY_roc_rising_en
What:		/sys/.../iio:deviceX/events/in_tempY_roc_falling_en
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Event generated when channel passes a threshold on the rate of
		change (1st differential) in the specified (_rising|_falling)
		direction. If the direction is not specified, then either the
		device will report an event which ever direction a single
		threshold value is passed in (e.g.
		<type>[Y][_name]_<raw|input>_roc_value) or
		<type>[Y][_name]_<raw|input>_roc_rising_value and
		<type>[Y][_name]_<raw|input>_roc_falling_value may take
		different values, but the device can only enable both rate of
		change thresholds or neither.
		Note the driver will assume the last p events requested are
		to be enabled where p is however many it supports (which may
		vary depending on the exact set requested. So if you want to be
		sure you have set what you think you have, check the contents of
		these attributes after everything is configured. Drivers may
		have to buffer any parameters so that they are consistent when
		a given event type is enabled a future point (and not those for
		whatever event was previously enabled).

What:		/sys/.../events/in_accel_x_raw_thresh_rising_value
What:		/sys/.../events/in_accel_x_raw_thresh_falling_value
What:		/sys/.../events/in_accel_y_raw_thresh_rising_value
What:		/sys/.../events/in_accel_y_raw_thresh_falling_value
What:		/sys/.../events/in_accel_z_raw_thresh_rising_value
What:		/sys/.../events/in_accel_z_raw_thresh_falling_value
What:		/sys/.../events/in_anglvel_x_raw_thresh_rising_value
What:		/sys/.../events/in_anglvel_x_raw_thresh_falling_value
What:		/sys/.../events/in_anglvel_y_raw_thresh_rising_value
What:		/sys/.../events/in_anglvel_y_raw_thresh_falling_value
What:		/sys/.../events/in_anglvel_z_raw_thresh_rising_value
What:		/sys/.../events/in_anglvel_z_raw_thresh_falling_value
What:		/sys/.../events/in_magn_x_raw_thresh_rising_value
What:		/sys/.../events/in_magn_x_raw_thresh_falling_value
What:		/sys/.../events/in_magn_y_raw_thresh_rising_value
What:		/sys/.../events/in_magn_y_raw_thresh_falling_value
What:		/sys/.../events/in_magn_z_raw_thresh_rising_value
What:		/sys/.../events/in_magn_z_raw_thresh_falling_value
What:		/sys/.../events/in_voltageY_supply_raw_thresh_rising_value
What:		/sys/.../events/in_voltageY_supply_raw_thresh_falling_value
What:		/sys/.../events/in_voltageY_raw_thresh_rising_value
What:		/sys/.../events/in_voltageY_raw_thresh_falling_value
What:		/sys/.../events/in_tempY_raw_thresh_rising_value
What:		/sys/.../events/in_tempY_raw_thresh_falling_value
What:		/sys/.../events/in_illuminance0_thresh_falling_value
what:		/sys/.../events/in_illuminance0_thresh_rising_value
what:		/sys/.../events/in_proximity0_thresh_falling_value
what:		/sys/.../events/in_proximity0_thresh_rising_value
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Specifies the value of threshold that the device is comparing
		against for the events enabled by
		<type>Y[_name]_thresh[_rising|falling]_en.
		If separate attributes exist for the two directions, but
		direction is not specified for this attribute, then a single
		threshold value applies to both directions.
		The raw or input element of the name indicates whether the
		value is in raw device units or in processed units (as _raw
		and _input do on sysfs direct channel read attributes).

What:		/sys/.../events/in_accel_x_raw_roc_rising_value
What:		/sys/.../events/in_accel_x_raw_roc_falling_value
What:		/sys/.../events/in_accel_y_raw_roc_rising_value
What:		/sys/.../events/in_accel_y_raw_roc_falling_value
What:		/sys/.../events/in_accel_z_raw_roc_rising_value
What:		/sys/.../events/in_accel_z_raw_roc_falling_value
What:		/sys/.../events/in_anglvel_x_raw_roc_rising_value
What:		/sys/.../events/in_anglvel_x_raw_roc_falling_value
What:		/sys/.../events/in_anglvel_y_raw_roc_rising_value
What:		/sys/.../events/in_anglvel_y_raw_roc_falling_value
What:		/sys/.../events/in_anglvel_z_raw_roc_rising_value
What:		/sys/.../events/in_anglvel_z_raw_roc_falling_value
What:		/sys/.../events/in_magn_x_raw_roc_rising_value
What:		/sys/.../events/in_magn_x_raw_roc_falling_value
What:		/sys/.../events/in_magn_y_raw_roc_rising_value
What:		/sys/.../events/in_magn_y_raw_roc_falling_value
What:		/sys/.../events/in_magn_z_raw_roc_rising_value
What:		/sys/.../events/in_magn_z_raw_roc_falling_value
What:		/sys/.../events/in_voltageY_supply_raw_roc_rising_value
What:		/sys/.../events/in_voltageY_supply_raw_roc_falling_value
What:		/sys/.../events/in_voltageY_raw_roc_rising_value
What:		/sys/.../events/in_voltageY_raw_roc_falling_value
What:		/sys/.../events/in_tempY_raw_roc_rising_value
What:		/sys/.../events/in_tempY_raw_roc_falling_value
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Specifies the value of rate of change threshold that the
		device is comparing against for the events enabled by
		<type>[Y][_name]_roc[_rising|falling]_en.
		If separate attributes exist for the two directions,
		but direction is not specified for this attribute,
		then a single threshold value applies to both directions.
		The raw or input element of the name indicates whether the
		value is in raw device units or in processed units (as _raw
		and _input do on sysfs direct channel read attributes).

What:		/sys/.../events/in_accel_x_thresh_rising_period
What:		/sys/.../events/in_accel_x_thresh_falling_period
hat:		/sys/.../events/in_accel_x_roc_rising_period
What:		/sys/.../events/in_accel_x_roc_falling_period
What:		/sys/.../events/in_accel_y_thresh_rising_period
What:		/sys/.../events/in_accel_y_thresh_falling_period
What:		/sys/.../events/in_accel_y_roc_rising_period
What:		/sys/.../events/in_accel_y_roc_falling_period
What:		/sys/.../events/in_accel_z_thresh_rising_period
What:		/sys/.../events/in_accel_z_thresh_falling_period
What:		/sys/.../events/in_accel_z_roc_rising_period
What:		/sys/.../events/in_accel_z_roc_falling_period
What:		/sys/.../events/in_anglvel_x_thresh_rising_period
What:		/sys/.../events/in_anglvel_x_thresh_falling_period
What:		/sys/.../events/in_anglvel_x_roc_rising_period
What:		/sys/.../events/in_anglvel_x_roc_falling_period
What:		/sys/.../events/in_anglvel_y_thresh_rising_period
What:		/sys/.../events/in_anglvel_y_thresh_falling_period
What:		/sys/.../events/in_anglvel_y_roc_rising_period
What:		/sys/.../events/in_anglvel_y_roc_falling_period
What:		/sys/.../events/in_anglvel_z_thresh_rising_period
What:		/sys/.../events/in_anglvel_z_thresh_falling_period
What:		/sys/.../events/in_anglvel_z_roc_rising_period
What:		/sys/.../events/in_anglvel_z_roc_falling_period
What:		/sys/.../events/in_magn_x_thresh_rising_period
What:		/sys/.../events/in_magn_x_thresh_falling_period
What:		/sys/.../events/in_magn_x_roc_rising_period
What:		/sys/.../events/in_magn_x_roc_falling_period
What:		/sys/.../events/in_magn_y_thresh_rising_period
What:		/sys/.../events/in_magn_y_thresh_falling_period
What:		/sys/.../events/in_magn_y_roc_rising_period
What:		/sys/.../events/in_magn_y_roc_falling_period
What:		/sys/.../events/in_magn_z_thresh_rising_period
What:		/sys/.../events/in_magn_z_thresh_falling_period
What:		/sys/.../events/in_magn_z_roc_rising_period
What:		/sys/.../events/in_magn_z_roc_falling_period
What:		/sys/.../events/in_voltageY_supply_thresh_rising_period
What:		/sys/.../events/in_voltageY_supply_thresh_falling_period
What:		/sys/.../events/in_voltageY_supply_roc_rising_period
What:		/sys/.../events/in_voltageY_supply_roc_falling_period
What:		/sys/.../events/in_voltageY_thresh_rising_period
What:		/sys/.../events/in_voltageY_thresh_falling_period
What:		/sys/.../events/in_voltageY_roc_rising_period
What:		/sys/.../events/in_voltageY_roc_falling_period
What:		/sys/.../events/in_tempY_thresh_rising_period
What:		/sys/.../events/in_tempY_thresh_falling_period
What:		/sys/.../events/in_tempY_roc_rising_period
What:		/sys/.../events/in_tempY_roc_falling_period
What:		/sys/.../events/in_accel_x&y&z_mag_falling_period
What:		/sys/.../events/in_intensity0_thresh_period
What:		/sys/.../events/in_proximity0_thresh_period
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Period of time (in seconds) for which the condition must be
		met before an event is generated. If direction is not
		specified then this period applies to both directions.

What:		/sys/.../iio:deviceX/events/in_accel_mag_en
What:		/sys/.../iio:deviceX/events/in_accel_mag_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_mag_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_x_mag_en
What:		/sys/.../iio:deviceX/events/in_accel_x_mag_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_x_mag_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_y_mag_en
What:		/sys/.../iio:deviceX/events/in_accel_y_mag_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_y_mag_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_z_mag_en
What:		/sys/.../iio:deviceX/events/in_accel_z_mag_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_z_mag_falling_en
What:		/sys/.../iio:deviceX/events/in_accel_x&y&z_mag_rising_en
What:		/sys/.../iio:deviceX/events/in_accel_x&y&z_mag_falling_en
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Similar to in_accel_x_thresh[_rising|_falling]_en, but here the
		magnitude of the channel is compared to the threshold, not its
		signed value.

What:		/sys/.../events/in_accel_raw_mag_value
What:		/sys/.../events/in_accel_x_raw_mag_rising_value
What:		/sys/.../events/in_accel_y_raw_mag_rising_value
What:		/sys/.../events/in_accel_z_raw_mag_rising_value
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		The value to which the magnitude of the channel is compared. If
		number or direction is not specified, applies to all channels of
		this type.

What:		/sys/bus/iio/devices/iio:deviceX/trigger/current_trigger
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		The name of the trigger source being used, as per string given
		in /sys/class/iio/triggerY/name.

What:		/sys/bus/iio/devices/iio:deviceX/buffer/length
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Number of scans contained by the buffer.

What:		/sys/bus/iio/devices/iio:deviceX/buffer/bytes_per_datum
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Bytes per scan.  Due to alignment fun, the scan may be larger
		than implied directly by the scan_element parameters.

What:		/sys/bus/iio/devices/iio:deviceX/buffer/enable
KernelVersion:	2.6.35
Contact:	linux-iio@vger.kernel.org
Description:
		Actually start the buffer capture up.  Will start trigger
		if first device and appropriate.

What:		/sys/bus/iio/devices/iio:deviceX/buffer/scan_elements
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Directory containing interfaces for elements that will be
		captured for a single triggered sample set in the buffer.

What:		/sys/.../buffer/scan_elements/in_accel_x_en
What:		/sys/.../buffer/scan_elements/in_accel_y_en
What:		/sys/.../buffer/scan_elements/in_accel_z_en
What:		/sys/.../buffer/scan_elements/in_anglvel_x_en
What:		/sys/.../buffer/scan_elements/in_anglvel_y_en
What:		/sys/.../buffer/scan_elements/in_anglvel_z_en
What:		/sys/.../buffer/scan_elements/in_magn_x_en
What:		/sys/.../buffer/scan_elements/in_magn_y_en
What:		/sys/.../buffer/scan_elements/in_magn_z_en
What:		/sys/.../buffer/scan_elements/in_timestamp_en
What:		/sys/.../buffer/scan_elements/in_voltageY_supply_en
What:		/sys/.../buffer/scan_elements/in_voltageY_en
What:		/sys/.../buffer/scan_elements/in_voltageY-voltageZ_en
What:		/sys/.../buffer/scan_elements/in_incli_x_en
What:		/sys/.../buffer/scan_elements/in_incli_y_en
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Scan element control for triggered data capture.

What:		/sys/.../buffer/scan_elements/in_accel_type
What:		/sys/.../buffer/scan_elements/in_anglvel_type
What:		/sys/.../buffer/scan_elements/in_magn_type
What:		/sys/.../buffer/scan_elements/in_incli_type
What:		/sys/.../buffer/scan_elements/in_voltageY_type
What:		/sys/.../buffer/scan_elements/in_voltage-in_type
What:		/sys/.../buffer/scan_elements/in_voltageY_supply_type
What:		/sys/.../buffer/scan_elements/in_timestamp_type
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		Description of the scan element data storage within the buffer
		and hence the form in which it is read from user-space.
		Form is [be|le]:[s|u]bits/storagebits[>>shift].
		be or le specifies big or little endian. s or u specifies if
		signed (2's complement) or unsigned. bits is the number of bits
		of data and storagebits is the space (after padding) that it
		occupies in the buffer. shift if specified, is the shift that
		needs to be applied prior to masking out unused bits. Some
		devices put their data in the middle of the transferred elements
		with additional information on both sides.  Note that some
		devices will have additional information in the unused bits
		so to get a clean value, the bits value must be used to mask
		the buffer output value appropriately.  The storagebits value
		also specifies the data alignment.  So s48/64>>2 will be a
		signed 48 bit integer stored in a 64 bit location aligned to
		a a64 bit boundary. To obtain the clean value, shift right 2
		and apply a mask to zero the top 16 bits of the result.
		For other storage combinations this attribute will be extended
		appropriately.

What:		/sys/.../buffer/scan_elements/in_accel_type_available
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		If the type parameter can take one of a small set of values,
		this attribute lists them.

What:		/sys/.../buffer/scan_elements/in_voltageY_index
What:		/sys/.../buffer/scan_elements/in_voltageY_supply_index
What:		/sys/.../buffer/scan_elements/in_accel_x_index
What:		/sys/.../buffer/scan_elements/in_accel_y_index
What:		/sys/.../buffer/scan_elements/in_accel_z_index
What:		/sys/.../buffer/scan_elements/in_anglvel_x_index
What:		/sys/.../buffer/scan_elements/in_anglvel_y_index
What:		/sys/.../buffer/scan_elements/in_anglvel_z_index
What:		/sys/.../buffer/scan_elements/in_magn_x_index
What:		/sys/.../buffer/scan_elements/in_magn_y_index
What:		/sys/.../buffer/scan_elements/in_magn_z_index
What:		/sys/.../buffer/scan_elements/in_incli_x_index
What:		/sys/.../buffer/scan_elements/in_incli_y_index
What:		/sys/.../buffer/scan_elements/in_timestamp_index
KernelVersion:	2.6.37
Contact:	linux-iio@vger.kernel.org
Description:
		A single positive integer specifying the position of this
		scan element in the buffer. Note these are not dependent on
		what is enabled and may not be contiguous. Thus for user-space
		to establish the full layout these must be used in conjunction
		with all _en attributes to establish which channels are present,
		and the relevant _type attributes to establish the data storage
		format.

What:		/sys/.../iio:deviceX/in_anglvel_z_quadrature_correction_raw
KernelVersion:	2.6.38
Contact:	linux-iio@vger.kernel.org
Description:
		This attribute is used to read the amount of quadrature error
		present in the device at a given time.
