* TI - L3 Network On Chip (NoC)

This version is an implementation of the generic NoC IP
provided by Arteris.

Required properties:
- compatible : Should be "ti,omap3-l3-smx" for OMAP3 family
               Should be "ti,omap4-l3-noc" for OMAP4 family
- ti,hwmods: "l3_main_1", ... One hwmod for each noc domain.

Examples:

ocp {
	compatible = "ti,omap4-l3-noc", "simple-bus";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges;
	ti,hwmods = "l3_main_1", "l3_main_2", "l3_main_3";
};
