Kernel driver ina2xx
====================

Supported chips:
  * Texas Instruments INA219
    Prefix: 'ina219'
    Addresses: I2C 0x40 - 0x4f
    Datasheet: Publicly available at the Texas Instruments website
               http://www.ti.com/

  * Texas Instruments INA220
    Prefix: 'ina220'
    Addresses: I2C 0x40 - 0x4f
    Datasheet: Publicly available at the Texas Instruments website
               http://www.ti.com/

  * Texas Instruments INA226
    Prefix: 'ina226'
    Addresses: I2C 0x40 - 0x4f
    Datasheet: Publicly available at the Texas Instruments website
               http://www.ti.com/

  * Texas Instruments INA230
    Prefix: 'ina230'
    Addresses: I2C 0x40 - 0x4f
    Datasheet: Publicly available at the Texas Instruments website
               http://www.ti.com/

Author: Lothar Felten <l-felten@ti.com>

Description
-----------

The INA219 is a high-side current shunt and power monitor with an I2C
interface. The INA219 monitors both shunt drop and supply voltage, with
programmable conversion times and filtering.

The INA220 is a high or low side current shunt and power monitor with an I2C
interface. The INA220 monitors both shunt drop and supply voltage.

The INA226 is a current shunt and power monitor with an I2C interface.
The INA226 monitors both a shunt voltage drop and bus supply voltage.

The INA230 is a high or low side current shunt and power monitor with an I2C
interface. The INA230 monitors both a shunt voltage drop and bus supply voltage.

The shunt value in micro-ohms can be set via platform data.
