* Freescale MXS Pin Controller

The pins controlled by mxs pin controller are organized in banks, each bank
has 32 pins.  Each pin has 4 multiplexing functions, and generally, the 4th
function is GPIO.  The configuration on the pins includes drive strength,
voltage and pull-up.

Required properties:
- compatible: "fsl,imx23-pinctrl" or "fsl,imx28-pinctrl"
- reg: Should contain the register physical address and length for the
  pin controller.

Please refer to pinctrl-bindings.txt in this directory for details of the
common pinctrl bindings used by client devices.

The node of mxs pin controller acts as a container for an arbitrary number of
subnodes.  Each of these subnodes represents some desired configuration for
a group of pins, and only affects those parameters that are explicitly listed.
In other words, a subnode that describes a drive strength parameter implies no
information about pull-up. For this reason, even seemingly boolean values are
actually tristates in this binding: unspecified, off, or on. Unspecified is
represented as an absent property, and off/on are represented as integer
values 0 and 1.

Those subnodes under mxs pin controller node will fall into two categories.
One is to set up a group of pins for a function, both mux selection and pin
configurations, and it's called group node in the binding document.   The other
one is to adjust the pin configuration for some particular pins that need a
different configuration than what is defined in group node.  The binding
document calls this type of node config node.

On mxs, there is no hardware pin group. The pin group in this binding only
means a group of pins put together for particular peripheral to work in
particular function, like SSP0 functioning as mmc0-8bit.  That said, the
group node should include all the pins needed for one function rather than
having these pins defined in several group nodes.  It also means each of
"pinctrl-*" phandle in client device node should only have one group node
pointed in there, while the phandle can have multiple config node referenced
there to adjust configurations for some pins in the group.

Required subnode-properties:
- fsl,pinmux-ids: An integer array.  Each integer in the array specify a pin
  with given mux function, with bank, pin and mux packed as below.

    [15..12] : bank number
    [11..4]  : pin number
    [3..0]   : mux selection

  This integer with mux selection packed is used as an entity by both group
  and config nodes to identify a pin.  The mux selection in the integer takes
  effects only on group node, and will get ignored by driver with config node,
  since config node is only meant to set up pin configurations.

  Valid values for these integers are listed below.

- reg: Should be the index of the group nodes for same function.  This property
  is required only for group nodes, and should not be present in any config
  nodes.

Optional subnode-properties:
- fsl,drive-strength: Integer.
    0: 4 mA
    1: 8 mA
    2: 12 mA
    3: 16 mA
- fsl,voltage: Integer.
    0: 1.8 V
    1: 3.3 V
- fsl,pull-up: Integer.
    0: Disable the internal pull-up
    1: Enable the internal pull-up

Examples:

pinctrl@80018000 {
	#address-cells = <1>;
	#size-cells = <0>;
	compatible = "fsl,imx28-pinctrl";
	reg = <0x80018000 2000>;

	mmc0_8bit_pins_a: mmc0-8bit@0 {
		reg = <0>;
		fsl,pinmux-ids = <
			0x2000 0x2010 0x2020 0x2030
			0x2040 0x2050 0x2060 0x2070
			0x2080 0x2090 0x20a0>;
		fsl,drive-strength = <1>;
		fsl,voltage = <1>;
		fsl,pull-up = <1>;
	};

	mmc_cd_cfg: mmc-cd-cfg {
		fsl,pinmux-ids = <0x2090>;
		fsl,pull-up = <0>;
	};

	mmc_sck_cfg: mmc-sck-cfg {
		fsl,pinmux-ids = <0x20a0>;
		fsl,drive-strength = <2>;
		fsl,pull-up = <0>;
	};
};

In this example, group node mmc0-8bit defines a group of pins for mxs SSP0
to function as a 8-bit mmc device, with 8mA, 3.3V and pull-up configurations
applied on all these pins.  And config nodes mmc-cd-cfg and mmc-sck-cfg are
adjusting the configuration for pins card-detection and clock from what group
node mmc0-8bit defines.  Only the configuration properties to be adjusted need
to be listed in the config nodes.

Valid values for i.MX28 pinmux-id:

pinmux						id
------						--
MX28_PAD_GPMI_D00__GPMI_D0			0x0000
MX28_PAD_GPMI_D01__GPMI_D1			0x0010
MX28_PAD_GPMI_D02__GPMI_D2			0x0020
MX28_PAD_GPMI_D03__GPMI_D3			0x0030
MX28_PAD_GPMI_D04__GPMI_D4			0x0040
MX28_PAD_GPMI_D05__GPMI_D5			0x0050
MX28_PAD_GPMI_D06__GPMI_D6			0x0060
MX28_PAD_GPMI_D07__GPMI_D7			0x0070
MX28_PAD_GPMI_CE0N__GPMI_CE0N			0x0100
MX28_PAD_GPMI_CE1N__GPMI_CE1N			0x0110
MX28_PAD_GPMI_CE2N__GPMI_CE2N			0x0120
MX28_PAD_GPMI_CE3N__GPMI_CE3N			0x0130
MX28_PAD_GPMI_RDY0__GPMI_READY0			0x0140
MX28_PAD_GPMI_RDY1__GPMI_READY1			0x0150
MX28_PAD_GPMI_RDY2__GPMI_READY2			0x0160
MX28_PAD_GPMI_RDY3__GPMI_READY3			0x0170
MX28_PAD_GPMI_RDN__GPMI_RDN			0x0180
MX28_PAD_GPMI_WRN__GPMI_WRN			0x0190
MX28_PAD_GPMI_ALE__GPMI_ALE			0x01a0
MX28_PAD_GPMI_CLE__GPMI_CLE			0x01b0
MX28_PAD_GPMI_RESETN__GPMI_RESETN		0x01c0
MX28_PAD_LCD_D00__LCD_D0			0x1000
MX28_PAD_LCD_D01__LCD_D1			0x1010
MX28_PAD_LCD_D02__LCD_D2			0x1020
MX28_PAD_LCD_D03__LCD_D3			0x1030
MX28_PAD_LCD_D04__LCD_D4			0x1040
MX28_PAD_LCD_D05__LCD_D5			0x1050
MX28_PAD_LCD_D06__LCD_D6			0x1060
MX28_PAD_LCD_D07__LCD_D7			0x1070
MX28_PAD_LCD_D08__LCD_D8			0x1080
MX28_PAD_LCD_D09__LCD_D9			0x1090
MX28_PAD_LCD_D10__LCD_D10			0x10a0
MX28_PAD_LCD_D11__LCD_D11			0x10b0
MX28_PAD_LCD_D12__LCD_D12			0x10c0
MX28_PAD_LCD_D13__LCD_D13			0x10d0
MX28_PAD_LCD_D14__LCD_D14			0x10e0
MX28_PAD_LCD_D15__LCD_D15			0x10f0
MX28_PAD_LCD_D16__LCD_D16			0x1100
MX28_PAD_LCD_D17__LCD_D17			0x1110
MX28_PAD_LCD_D18__LCD_D18			0x1120
MX28_PAD_LCD_D19__LCD_D19			0x1130
MX28_PAD_LCD_D20__LCD_D20			0x1140
MX28_PAD_LCD_D21__LCD_D21			0x1150
MX28_PAD_LCD_D22__LCD_D22			0x1160
MX28_PAD_LCD_D23__LCD_D23			0x1170
MX28_PAD_LCD_RD_E__LCD_RD_E			0x1180
MX28_PAD_LCD_WR_RWN__LCD_WR_RWN			0x1190
MX28_PAD_LCD_RS__LCD_RS				0x11a0
MX28_PAD_LCD_CS__LCD_CS				0x11b0
MX28_PAD_LCD_VSYNC__LCD_VSYNC			0x11c0
MX28_PAD_LCD_HSYNC__LCD_HSYNC			0x11d0
MX28_PAD_LCD_DOTCLK__LCD_DOTCLK			0x11e0
MX28_PAD_LCD_ENABLE__LCD_ENABLE			0x11f0
MX28_PAD_SSP0_DATA0__SSP0_D0			0x2000
MX28_PAD_SSP0_DATA1__SSP0_D1			0x2010
MX28_PAD_SSP0_DATA2__SSP0_D2			0x2020
MX28_PAD_SSP0_DATA3__SSP0_D3			0x2030
MX28_PAD_SSP0_DATA4__SSP0_D4			0x2040
MX28_PAD_SSP0_DATA5__SSP0_D5			0x2050
MX28_PAD_SSP0_DATA6__SSP0_D6			0x2060
MX28_PAD_SSP0_DATA7__SSP0_D7			0x2070
MX28_PAD_SSP0_CMD__SSP0_CMD			0x2080
MX28_PAD_SSP0_DETECT__SSP0_CARD_DETECT		0x2090
MX28_PAD_SSP0_SCK__SSP0_SCK			0x20a0
MX28_PAD_SSP1_SCK__SSP1_SCK			0x20c0
MX28_PAD_SSP1_CMD__SSP1_CMD			0x20d0
MX28_PAD_SSP1_DATA0__SSP1_D0			0x20e0
MX28_PAD_SSP1_DATA3__SSP1_D3			0x20f0
MX28_PAD_SSP2_SCK__SSP2_SCK			0x2100
MX28_PAD_SSP2_MOSI__SSP2_CMD			0x2110
MX28_PAD_SSP2_MISO__SSP2_D0			0x2120
MX28_PAD_SSP2_SS0__SSP2_D3			0x2130
MX28_PAD_SSP2_SS1__SSP2_D4			0x2140
MX28_PAD_SSP2_SS2__SSP2_D5			0x2150
MX28_PAD_SSP3_SCK__SSP3_SCK			0x2180
MX28_PAD_SSP3_MOSI__SSP3_CMD			0x2190
MX28_PAD_SSP3_MISO__SSP3_D0			0x21a0
MX28_PAD_SSP3_SS0__SSP3_D3			0x21b0
MX28_PAD_AUART0_RX__AUART0_RX			0x3000
MX28_PAD_AUART0_TX__AUART0_TX			0x3010
MX28_PAD_AUART0_CTS__AUART0_CTS			0x3020
MX28_PAD_AUART0_RTS__AUART0_RTS			0x3030
MX28_PAD_AUART1_RX__AUART1_RX			0x3040
MX28_PAD_AUART1_TX__AUART1_TX			0x3050
MX28_PAD_AUART1_CTS__AUART1_CTS			0x3060
MX28_PAD_AUART1_RTS__AUART1_RTS			0x3070
MX28_PAD_AUART2_RX__AUART2_RX			0x3080
MX28_PAD_AUART2_TX__AUART2_TX			0x3090
MX28_PAD_AUART2_CTS__AUART2_CTS			0x30a0
MX28_PAD_AUART2_RTS__AUART2_RTS			0x30b0
MX28_PAD_AUART3_RX__AUART3_RX			0x30c0
MX28_PAD_AUART3_TX__AUART3_TX			0x30d0
MX28_PAD_AUART3_CTS__AUART3_CTS			0x30e0
MX28_PAD_AUART3_RTS__AUART3_RTS			0x30f0
MX28_PAD_PWM0__PWM_0				0x3100
MX28_PAD_PWM1__PWM_1				0x3110
MX28_PAD_PWM2__PWM_2				0x3120
MX28_PAD_SAIF0_MCLK__SAIF0_MCLK			0x3140
MX28_PAD_SAIF0_LRCLK__SAIF0_LRCLK		0x3150
MX28_PAD_SAIF0_BITCLK__SAIF0_BITCLK		0x3160
MX28_PAD_SAIF0_SDATA0__SAIF0_SDATA0		0x3170
MX28_PAD_I2C0_SCL__I2C0_SCL			0x3180
MX28_PAD_I2C0_SDA__I2C0_SDA			0x3190
MX28_PAD_SAIF1_SDATA0__SAIF1_SDATA0		0x31a0
MX28_PAD_SPDIF__SPDIF_TX			0x31b0
MX28_PAD_PWM3__PWM_3				0x31c0
MX28_PAD_PWM4__PWM_4				0x31d0
MX28_PAD_LCD_RESET__LCD_RESET			0x31e0
MX28_PAD_ENET0_MDC__ENET0_MDC			0x4000
MX28_PAD_ENET0_MDIO__ENET0_MDIO			0x4010
MX28_PAD_ENET0_RX_EN__ENET0_RX_EN		0x4020
MX28_PAD_ENET0_RXD0__ENET0_RXD0			0x4030
MX28_PAD_ENET0_RXD1__ENET0_RXD1			0x4040
MX28_PAD_ENET0_TX_CLK__ENET0_TX_CLK		0x4050
MX28_PAD_ENET0_TX_EN__ENET0_TX_EN		0x4060
MX28_PAD_ENET0_TXD0__ENET0_TXD0			0x4070
MX28_PAD_ENET0_TXD1__ENET0_TXD1			0x4080
MX28_PAD_ENET0_RXD2__ENET0_RXD2			0x4090
MX28_PAD_ENET0_RXD3__ENET0_RXD3			0x40a0
MX28_PAD_ENET0_TXD2__ENET0_TXD2			0x40b0
MX28_PAD_ENET0_TXD3__ENET0_TXD3			0x40c0
MX28_PAD_ENET0_RX_CLK__ENET0_RX_CLK		0x40d0
MX28_PAD_ENET0_COL__ENET0_COL			0x40e0
MX28_PAD_ENET0_CRS__ENET0_CRS			0x40f0
MX28_PAD_ENET_CLK__CLKCTRL_ENET			0x4100
MX28_PAD_JTAG_RTCK__JTAG_RTCK			0x4140
MX28_PAD_EMI_D00__EMI_DATA0			0x5000
MX28_PAD_EMI_D01__EMI_DATA1			0x5010
MX28_PAD_EMI_D02__EMI_DATA2			0x5020
MX28_PAD_EMI_D03__EMI_DATA3			0x5030
MX28_PAD_EMI_D04__EMI_DATA4			0x5040
MX28_PAD_EMI_D05__EMI_DATA5			0x5050
MX28_PAD_EMI_D06__EMI_DATA6			0x5060
MX28_PAD_EMI_D07__EMI_DATA7			0x5070
MX28_PAD_EMI_D08__EMI_DATA8			0x5080
MX28_PAD_EMI_D09__EMI_DATA9			0x5090
MX28_PAD_EMI_D10__EMI_DATA10			0x50a0
MX28_PAD_EMI_D11__EMI_DATA11			0x50b0
MX28_PAD_EMI_D12__EMI_DATA12			0x50c0
MX28_PAD_EMI_D13__EMI_DATA13			0x50d0
MX28_PAD_EMI_D14__EMI_DATA14			0x50e0
MX28_PAD_EMI_D15__EMI_DATA15			0x50f0
MX28_PAD_EMI_ODT0__EMI_ODT0			0x5100
MX28_PAD_EMI_DQM0__EMI_DQM0			0x5110
MX28_PAD_EMI_ODT1__EMI_ODT1			0x5120
MX28_PAD_EMI_DQM1__EMI_DQM1			0x5130
MX28_PAD_EMI_DDR_OPEN_FB__EMI_DDR_OPEN_FEEDBACK	0x5140
MX28_PAD_EMI_CLK__EMI_CLK			0x5150
MX28_PAD_EMI_DQS0__EMI_DQS0			0x5160
MX28_PAD_EMI_DQS1__EMI_DQS1			0x5170
MX28_PAD_EMI_DDR_OPEN__EMI_DDR_OPEN		0x51a0
MX28_PAD_EMI_A00__EMI_ADDR0			0x6000
MX28_PAD_EMI_A01__EMI_ADDR1			0x6010
MX28_PAD_EMI_A02__EMI_ADDR2			0x6020
MX28_PAD_EMI_A03__EMI_ADDR3			0x6030
MX28_PAD_EMI_A04__EMI_ADDR4			0x6040
MX28_PAD_EMI_A05__EMI_ADDR5			0x6050
MX28_PAD_EMI_A06__EMI_ADDR6			0x6060
MX28_PAD_EMI_A07__EMI_ADDR7			0x6070
MX28_PAD_EMI_A08__EMI_ADDR8			0x6080
MX28_PAD_EMI_A09__EMI_ADDR9			0x6090
MX28_PAD_EMI_A10__EMI_ADDR10			0x60a0
MX28_PAD_EMI_A11__EMI_ADDR11			0x60b0
MX28_PAD_EMI_A12__EMI_ADDR12			0x60c0
MX28_PAD_EMI_A13__EMI_ADDR13			0x60d0
MX28_PAD_EMI_A14__EMI_ADDR14			0x60e0
MX28_PAD_EMI_BA0__EMI_BA0			0x6100
MX28_PAD_EMI_BA1__EMI_BA1			0x6110
MX28_PAD_EMI_BA2__EMI_BA2			0x6120
MX28_PAD_EMI_CASN__EMI_CASN			0x6130
MX28_PAD_EMI_RASN__EMI_RASN			0x6140
MX28_PAD_EMI_WEN__EMI_WEN			0x6150
MX28_PAD_EMI_CE0N__EMI_CE0N			0x6160
MX28_PAD_EMI_CE1N__EMI_CE1N			0x6170
MX28_PAD_EMI_CKE__EMI_CKE			0x6180
MX28_PAD_GPMI_D00__SSP1_D0			0x0001
MX28_PAD_GPMI_D01__SSP1_D1			0x0011
MX28_PAD_GPMI_D02__SSP1_D2			0x0021
MX28_PAD_GPMI_D03__SSP1_D3			0x0031
MX28_PAD_GPMI_D04__SSP1_D4			0x0041
MX28_PAD_GPMI_D05__SSP1_D5			0x0051
MX28_PAD_GPMI_D06__SSP1_D6			0x0061
MX28_PAD_GPMI_D07__SSP1_D7			0x0071
MX28_PAD_GPMI_CE0N__SSP3_D0			0x0101
MX28_PAD_GPMI_CE1N__SSP3_D3			0x0111
MX28_PAD_GPMI_CE2N__CAN1_TX			0x0121
MX28_PAD_GPMI_CE3N__CAN1_RX			0x0131
MX28_PAD_GPMI_RDY0__SSP1_CARD_DETECT		0x0141
MX28_PAD_GPMI_RDY1__SSP1_CMD			0x0151
MX28_PAD_GPMI_RDY2__CAN0_TX			0x0161
MX28_PAD_GPMI_RDY3__CAN0_RX			0x0171
MX28_PAD_GPMI_RDN__SSP3_SCK			0x0181
MX28_PAD_GPMI_WRN__SSP1_SCK			0x0191
MX28_PAD_GPMI_ALE__SSP3_D1			0x01a1
MX28_PAD_GPMI_CLE__SSP3_D2			0x01b1
MX28_PAD_GPMI_RESETN__SSP3_CMD			0x01c1
MX28_PAD_LCD_D03__ETM_DA8			0x1031
MX28_PAD_LCD_D04__ETM_DA9			0x1041
MX28_PAD_LCD_D08__ETM_DA3			0x1081
MX28_PAD_LCD_D09__ETM_DA4			0x1091
MX28_PAD_LCD_D20__ENET1_1588_EVENT2_OUT		0x1141
MX28_PAD_LCD_D21__ENET1_1588_EVENT2_IN		0x1151
MX28_PAD_LCD_D22__ENET1_1588_EVENT3_OUT		0x1161
MX28_PAD_LCD_D23__ENET1_1588_EVENT3_IN		0x1171
MX28_PAD_LCD_RD_E__LCD_VSYNC			0x1181
MX28_PAD_LCD_WR_RWN__LCD_HSYNC			0x1191
MX28_PAD_LCD_RS__LCD_DOTCLK			0x11a1
MX28_PAD_LCD_CS__LCD_ENABLE			0x11b1
MX28_PAD_LCD_VSYNC__SAIF1_SDATA0		0x11c1
MX28_PAD_LCD_HSYNC__SAIF1_SDATA1		0x11d1
MX28_PAD_LCD_DOTCLK__SAIF1_MCLK			0x11e1
MX28_PAD_SSP0_DATA4__SSP2_D0			0x2041
MX28_PAD_SSP0_DATA5__SSP2_D3			0x2051
MX28_PAD_SSP0_DATA6__SSP2_CMD			0x2061
MX28_PAD_SSP0_DATA7__SSP2_SCK			0x2071
MX28_PAD_SSP1_SCK__SSP2_D1			0x20c1
MX28_PAD_SSP1_CMD__SSP2_D2			0x20d1
MX28_PAD_SSP1_DATA0__SSP2_D6			0x20e1
MX28_PAD_SSP1_DATA3__SSP2_D7			0x20f1
MX28_PAD_SSP2_SCK__AUART2_RX			0x2101
MX28_PAD_SSP2_MOSI__AUART2_TX			0x2111
MX28_PAD_SSP2_MISO__AUART3_RX			0x2121
MX28_PAD_SSP2_SS0__AUART3_TX			0x2131
MX28_PAD_SSP2_SS1__SSP2_D1			0x2141
MX28_PAD_SSP2_SS2__SSP2_D2			0x2151
MX28_PAD_SSP3_SCK__AUART4_TX			0x2181
MX28_PAD_SSP3_MOSI__AUART4_RX			0x2191
MX28_PAD_SSP3_MISO__AUART4_RTS			0x21a1
MX28_PAD_SSP3_SS0__AUART4_CTS			0x21b1
MX28_PAD_AUART0_RX__I2C0_SCL			0x3001
MX28_PAD_AUART0_TX__I2C0_SDA			0x3011
MX28_PAD_AUART0_CTS__AUART4_RX			0x3021
MX28_PAD_AUART0_RTS__AUART4_TX			0x3031
MX28_PAD_AUART1_RX__SSP2_CARD_DETECT		0x3041
MX28_PAD_AUART1_TX__SSP3_CARD_DETECT		0x3051
MX28_PAD_AUART1_CTS__USB0_OVERCURRENT		0x3061
MX28_PAD_AUART1_RTS__USB0_ID			0x3071
MX28_PAD_AUART2_RX__SSP3_D1			0x3081
MX28_PAD_AUART2_TX__SSP3_D2			0x3091
MX28_PAD_AUART2_CTS__I2C1_SCL			0x30a1
MX28_PAD_AUART2_RTS__I2C1_SDA			0x30b1
MX28_PAD_AUART3_RX__CAN0_TX			0x30c1
MX28_PAD_AUART3_TX__CAN0_RX			0x30d1
MX28_PAD_AUART3_CTS__CAN1_TX			0x30e1
MX28_PAD_AUART3_RTS__CAN1_RX			0x30f1
MX28_PAD_PWM0__I2C1_SCL				0x3101
MX28_PAD_PWM1__I2C1_SDA				0x3111
MX28_PAD_PWM2__USB0_ID				0x3121
MX28_PAD_SAIF0_MCLK__PWM_3			0x3141
MX28_PAD_SAIF0_LRCLK__PWM_4			0x3151
MX28_PAD_SAIF0_BITCLK__PWM_5			0x3161
MX28_PAD_SAIF0_SDATA0__PWM_6			0x3171
MX28_PAD_I2C0_SCL__TIMROT_ROTARYA		0x3181
MX28_PAD_I2C0_SDA__TIMROT_ROTARYB		0x3191
MX28_PAD_SAIF1_SDATA0__PWM_7			0x31a1
MX28_PAD_LCD_RESET__LCD_VSYNC			0x31e1
MX28_PAD_ENET0_MDC__GPMI_CE4N			0x4001
MX28_PAD_ENET0_MDIO__GPMI_CE5N			0x4011
MX28_PAD_ENET0_RX_EN__GPMI_CE6N			0x4021
MX28_PAD_ENET0_RXD0__GPMI_CE7N			0x4031
MX28_PAD_ENET0_RXD1__GPMI_READY4		0x4041
MX28_PAD_ENET0_TX_CLK__HSADC_TRIGGER		0x4051
MX28_PAD_ENET0_TX_EN__GPMI_READY5		0x4061
MX28_PAD_ENET0_TXD0__GPMI_READY6		0x4071
MX28_PAD_ENET0_TXD1__GPMI_READY7		0x4081
MX28_PAD_ENET0_RXD2__ENET1_RXD0			0x4091
MX28_PAD_ENET0_RXD3__ENET1_RXD1			0x40a1
MX28_PAD_ENET0_TXD2__ENET1_TXD0			0x40b1
MX28_PAD_ENET0_TXD3__ENET1_TXD1			0x40c1
MX28_PAD_ENET0_RX_CLK__ENET0_RX_ER		0x40d1
MX28_PAD_ENET0_COL__ENET1_TX_EN			0x40e1
MX28_PAD_ENET0_CRS__ENET1_RX_EN			0x40f1
MX28_PAD_GPMI_CE2N__ENET0_RX_ER			0x0122
MX28_PAD_GPMI_CE3N__SAIF1_MCLK			0x0132
MX28_PAD_GPMI_RDY0__USB0_ID			0x0142
MX28_PAD_GPMI_RDY2__ENET0_TX_ER			0x0162
MX28_PAD_GPMI_RDY3__HSADC_TRIGGER		0x0172
MX28_PAD_GPMI_ALE__SSP3_D4			0x01a2
MX28_PAD_GPMI_CLE__SSP3_D5			0x01b2
MX28_PAD_LCD_D00__ETM_DA0			0x1002
MX28_PAD_LCD_D01__ETM_DA1			0x1012
MX28_PAD_LCD_D02__ETM_DA2			0x1022
MX28_PAD_LCD_D03__ETM_DA3			0x1032
MX28_PAD_LCD_D04__ETM_DA4			0x1042
MX28_PAD_LCD_D05__ETM_DA5			0x1052
MX28_PAD_LCD_D06__ETM_DA6			0x1062
MX28_PAD_LCD_D07__ETM_DA7			0x1072
MX28_PAD_LCD_D08__ETM_DA8			0x1082
MX28_PAD_LCD_D09__ETM_DA9			0x1092
MX28_PAD_LCD_D10__ETM_DA10			0x10a2
MX28_PAD_LCD_D11__ETM_DA11			0x10b2
MX28_PAD_LCD_D12__ETM_DA12			0x10c2
MX28_PAD_LCD_D13__ETM_DA13			0x10d2
MX28_PAD_LCD_D14__ETM_DA14			0x10e2
MX28_PAD_LCD_D15__ETM_DA15			0x10f2
MX28_PAD_LCD_D16__ETM_DA7			0x1102
MX28_PAD_LCD_D17__ETM_DA6			0x1112
MX28_PAD_LCD_D18__ETM_DA5			0x1122
MX28_PAD_LCD_D19__ETM_DA4			0x1132
MX28_PAD_LCD_D20__ETM_DA3			0x1142
MX28_PAD_LCD_D21__ETM_DA2			0x1152
MX28_PAD_LCD_D22__ETM_DA1			0x1162
MX28_PAD_LCD_D23__ETM_DA0			0x1172
MX28_PAD_LCD_RD_E__ETM_TCTL			0x1182
MX28_PAD_LCD_WR_RWN__ETM_TCLK			0x1192
MX28_PAD_LCD_HSYNC__ETM_TCTL			0x11d2
MX28_PAD_LCD_DOTCLK__ETM_TCLK			0x11e2
MX28_PAD_SSP1_SCK__ENET0_1588_EVENT2_OUT	0x20c2
MX28_PAD_SSP1_CMD__ENET0_1588_EVENT2_IN		0x20d2
MX28_PAD_SSP1_DATA0__ENET0_1588_EVENT3_OUT	0x20e2
MX28_PAD_SSP1_DATA3__ENET0_1588_EVENT3_IN	0x20f2
MX28_PAD_SSP2_SCK__SAIF0_SDATA1			0x2102
MX28_PAD_SSP2_MOSI__SAIF0_SDATA2		0x2112
MX28_PAD_SSP2_MISO__SAIF1_SDATA1		0x2122
MX28_PAD_SSP2_SS0__SAIF1_SDATA2			0x2132
MX28_PAD_SSP2_SS1__USB1_OVERCURRENT		0x2142
MX28_PAD_SSP2_SS2__USB0_OVERCURRENT		0x2152
MX28_PAD_SSP3_SCK__ENET1_1588_EVENT0_OUT	0x2182
MX28_PAD_SSP3_MOSI__ENET1_1588_EVENT0_IN	0x2192
MX28_PAD_SSP3_MISO__ENET1_1588_EVENT1_OUT	0x21a2
MX28_PAD_SSP3_SS0__ENET1_1588_EVENT1_IN		0x21b2
MX28_PAD_AUART0_RX__DUART_CTS			0x3002
MX28_PAD_AUART0_TX__DUART_RTS			0x3012
MX28_PAD_AUART0_CTS__DUART_RX			0x3022
MX28_PAD_AUART0_RTS__DUART_TX			0x3032
MX28_PAD_AUART1_RX__PWM_0			0x3042
MX28_PAD_AUART1_TX__PWM_1			0x3052
MX28_PAD_AUART1_CTS__TIMROT_ROTARYA		0x3062
MX28_PAD_AUART1_RTS__TIMROT_ROTARYB		0x3072
MX28_PAD_AUART2_RX__SSP3_D4			0x3082
MX28_PAD_AUART2_TX__SSP3_D5			0x3092
MX28_PAD_AUART2_CTS__SAIF1_BITCLK		0x30a2
MX28_PAD_AUART2_RTS__SAIF1_LRCLK		0x30b2
MX28_PAD_AUART3_RX__ENET0_1588_EVENT0_OUT	0x30c2
MX28_PAD_AUART3_TX__ENET0_1588_EVENT0_IN	0x30d2
MX28_PAD_AUART3_CTS__ENET0_1588_EVENT1_OUT	0x30e2
MX28_PAD_AUART3_RTS__ENET0_1588_EVENT1_IN	0x30f2
MX28_PAD_PWM0__DUART_RX				0x3102
MX28_PAD_PWM1__DUART_TX				0x3112
MX28_PAD_PWM2__USB1_OVERCURRENT			0x3122
MX28_PAD_SAIF0_MCLK__AUART4_CTS			0x3142
MX28_PAD_SAIF0_LRCLK__AUART4_RTS		0x3152
MX28_PAD_SAIF0_BITCLK__AUART4_RX		0x3162
MX28_PAD_SAIF0_SDATA0__AUART4_TX		0x3172
MX28_PAD_I2C0_SCL__DUART_RX			0x3182
MX28_PAD_I2C0_SDA__DUART_TX			0x3192
MX28_PAD_SAIF1_SDATA0__SAIF0_SDATA1		0x31a2
MX28_PAD_SPDIF__ENET1_RX_ER			0x31b2
MX28_PAD_ENET0_MDC__SAIF0_SDATA1		0x4002
MX28_PAD_ENET0_MDIO__SAIF0_SDATA2		0x4012
MX28_PAD_ENET0_RX_EN__SAIF1_SDATA1		0x4022
MX28_PAD_ENET0_RXD0__SAIF1_SDATA2		0x4032
MX28_PAD_ENET0_TX_CLK__ENET0_1588_EVENT2_OUT	0x4052
MX28_PAD_ENET0_RXD2__ENET0_1588_EVENT0_OUT	0x4092
MX28_PAD_ENET0_RXD3__ENET0_1588_EVENT0_IN	0x40a2
MX28_PAD_ENET0_TXD2__ENET0_1588_EVENT1_OUT	0x40b2
MX28_PAD_ENET0_TXD3__ENET0_1588_EVENT1_IN	0x40c2
MX28_PAD_ENET0_RX_CLK__ENET0_1588_EVENT2_IN	0x40d2
MX28_PAD_ENET0_COL__ENET0_1588_EVENT3_OUT	0x40e2
MX28_PAD_ENET0_CRS__ENET0_1588_EVENT3_IN	0x40f2
MX28_PAD_GPMI_D00__GPIO_0_0			0x0003
MX28_PAD_GPMI_D01__GPIO_0_1			0x0013
MX28_PAD_GPMI_D02__GPIO_0_2			0x0023
MX28_PAD_GPMI_D03__GPIO_0_3			0x0033
MX28_PAD_GPMI_D04__GPIO_0_4			0x0043
MX28_PAD_GPMI_D05__GPIO_0_5			0x0053
MX28_PAD_GPMI_D06__GPIO_0_6			0x0063
MX28_PAD_GPMI_D07__GPIO_0_7			0x0073
MX28_PAD_GPMI_CE0N__GPIO_0_16			0x0103
MX28_PAD_GPMI_CE1N__GPIO_0_17			0x0113
MX28_PAD_GPMI_CE2N__GPIO_0_18			0x0123
MX28_PAD_GPMI_CE3N__GPIO_0_19			0x0133
MX28_PAD_GPMI_RDY0__GPIO_0_20			0x0143
MX28_PAD_GPMI_RDY1__GPIO_0_21			0x0153
MX28_PAD_GPMI_RDY2__GPIO_0_22			0x0163
MX28_PAD_GPMI_RDY3__GPIO_0_23			0x0173
MX28_PAD_GPMI_RDN__GPIO_0_24			0x0183
MX28_PAD_GPMI_WRN__GPIO_0_25			0x0193
MX28_PAD_GPMI_ALE__GPIO_0_26			0x01a3
MX28_PAD_GPMI_CLE__GPIO_0_27			0x01b3
MX28_PAD_GPMI_RESETN__GPIO_0_28			0x01c3
MX28_PAD_LCD_D00__GPIO_1_0			0x1003
MX28_PAD_LCD_D01__GPIO_1_1			0x1013
MX28_PAD_LCD_D02__GPIO_1_2			0x1023
MX28_PAD_LCD_D03__GPIO_1_3			0x1033
MX28_PAD_LCD_D04__GPIO_1_4			0x1043
MX28_PAD_LCD_D05__GPIO_1_5			0x1053
MX28_PAD_LCD_D06__GPIO_1_6			0x1063
MX28_PAD_LCD_D07__GPIO_1_7			0x1073
MX28_PAD_LCD_D08__GPIO_1_8			0x1083
MX28_PAD_LCD_D09__GPIO_1_9			0x1093
MX28_PAD_LCD_D10__GPIO_1_10			0x10a3
MX28_PAD_LCD_D11__GPIO_1_11			0x10b3
MX28_PAD_LCD_D12__GPIO_1_12			0x10c3
MX28_PAD_LCD_D13__GPIO_1_13			0x10d3
MX28_PAD_LCD_D14__GPIO_1_14			0x10e3
MX28_PAD_LCD_D15__GPIO_1_15			0x10f3
MX28_PAD_LCD_D16__GPIO_1_16			0x1103
MX28_PAD_LCD_D17__GPIO_1_17			0x1113
MX28_PAD_LCD_D18__GPIO_1_18			0x1123
MX28_PAD_LCD_D19__GPIO_1_19			0x1133
MX28_PAD_LCD_D20__GPIO_1_20			0x1143
MX28_PAD_LCD_D21__GPIO_1_21			0x1153
MX28_PAD_LCD_D22__GPIO_1_22			0x1163
MX28_PAD_LCD_D23__GPIO_1_23			0x1173
MX28_PAD_LCD_RD_E__GPIO_1_24			0x1183
MX28_PAD_LCD_WR_RWN__GPIO_1_25			0x1193
MX28_PAD_LCD_RS__GPIO_1_26			0x11a3
MX28_PAD_LCD_CS__GPIO_1_27			0x11b3
MX28_PAD_LCD_VSYNC__GPIO_1_28			0x11c3
MX28_PAD_LCD_HSYNC__GPIO_1_29			0x11d3
MX28_PAD_LCD_DOTCLK__GPIO_1_30			0x11e3
MX28_PAD_LCD_ENABLE__GPIO_1_31			0x11f3
MX28_PAD_SSP0_DATA0__GPIO_2_0			0x2003
MX28_PAD_SSP0_DATA1__GPIO_2_1			0x2013
MX28_PAD_SSP0_DATA2__GPIO_2_2			0x2023
MX28_PAD_SSP0_DATA3__GPIO_2_3			0x2033
MX28_PAD_SSP0_DATA4__GPIO_2_4			0x2043
MX28_PAD_SSP0_DATA5__GPIO_2_5			0x2053
MX28_PAD_SSP0_DATA6__GPIO_2_6			0x2063
MX28_PAD_SSP0_DATA7__GPIO_2_7			0x2073
MX28_PAD_SSP0_CMD__GPIO_2_8			0x2083
MX28_PAD_SSP0_DETECT__GPIO_2_9			0x2093
MX28_PAD_SSP0_SCK__GPIO_2_10			0x20a3
MX28_PAD_SSP1_SCK__GPIO_2_12			0x20c3
MX28_PAD_SSP1_CMD__GPIO_2_13			0x20d3
MX28_PAD_SSP1_DATA0__GPIO_2_14			0x20e3
MX28_PAD_SSP1_DATA3__GPIO_2_15			0x20f3
MX28_PAD_SSP2_SCK__GPIO_2_16			0x2103
MX28_PAD_SSP2_MOSI__GPIO_2_17			0x2113
MX28_PAD_SSP2_MISO__GPIO_2_18			0x2123
MX28_PAD_SSP2_SS0__GPIO_2_19			0x2133
MX28_PAD_SSP2_SS1__GPIO_2_20			0x2143
MX28_PAD_SSP2_SS2__GPIO_2_21			0x2153
MX28_PAD_SSP3_SCK__GPIO_2_24			0x2183
MX28_PAD_SSP3_MOSI__GPIO_2_25			0x2193
MX28_PAD_SSP3_MISO__GPIO_2_26			0x21a3
MX28_PAD_SSP3_SS0__GPIO_2_27			0x21b3
MX28_PAD_AUART0_RX__GPIO_3_0			0x3003
MX28_PAD_AUART0_TX__GPIO_3_1			0x3013
MX28_PAD_AUART0_CTS__GPIO_3_2			0x3023
MX28_PAD_AUART0_RTS__GPIO_3_3			0x3033
MX28_PAD_AUART1_RX__GPIO_3_4			0x3043
MX28_PAD_AUART1_TX__GPIO_3_5			0x3053
MX28_PAD_AUART1_CTS__GPIO_3_6			0x3063
MX28_PAD_AUART1_RTS__GPIO_3_7			0x3073
MX28_PAD_AUART2_RX__GPIO_3_8			0x3083
MX28_PAD_AUART2_TX__GPIO_3_9			0x3093
MX28_PAD_AUART2_CTS__GPIO_3_10			0x30a3
MX28_PAD_AUART2_RTS__GPIO_3_11			0x30b3
MX28_PAD_AUART3_RX__GPIO_3_12			0x30c3
MX28_PAD_AUART3_TX__GPIO_3_13			0x30d3
MX28_PAD_AUART3_CTS__GPIO_3_14			0x30e3
MX28_PAD_AUART3_RTS__GPIO_3_15			0x30f3
MX28_PAD_PWM0__GPIO_3_16			0x3103
MX28_PAD_PWM1__GPIO_3_17			0x3113
MX28_PAD_PWM2__GPIO_3_18			0x3123
MX28_PAD_SAIF0_MCLK__GPIO_3_20			0x3143
MX28_PAD_SAIF0_LRCLK__GPIO_3_21			0x3153
MX28_PAD_SAIF0_BITCLK__GPIO_3_22		0x3163
MX28_PAD_SAIF0_SDATA0__GPIO_3_23		0x3173
MX28_PAD_I2C0_SCL__GPIO_3_24			0x3183
MX28_PAD_I2C0_SDA__GPIO_3_25			0x3193
MX28_PAD_SAIF1_SDATA0__GPIO_3_26		0x31a3
MX28_PAD_SPDIF__GPIO_3_27			0x31b3
MX28_PAD_PWM3__GPIO_3_28			0x31c3
MX28_PAD_PWM4__GPIO_3_29			0x31d3
MX28_PAD_LCD_RESET__GPIO_3_30			0x31e3
MX28_PAD_ENET0_MDC__GPIO_4_0			0x4003
MX28_PAD_ENET0_MDIO__GPIO_4_1			0x4013
MX28_PAD_ENET0_RX_EN__GPIO_4_2			0x4023
MX28_PAD_ENET0_RXD0__GPIO_4_3			0x4033
MX28_PAD_ENET0_RXD1__GPIO_4_4			0x4043
MX28_PAD_ENET0_TX_CLK__GPIO_4_5			0x4053
MX28_PAD_ENET0_TX_EN__GPIO_4_6			0x4063
MX28_PAD_ENET0_TXD0__GPIO_4_7			0x4073
MX28_PAD_ENET0_TXD1__GPIO_4_8			0x4083
MX28_PAD_ENET0_RXD2__GPIO_4_9			0x4093
MX28_PAD_ENET0_RXD3__GPIO_4_10			0x40a3
MX28_PAD_ENET0_TXD2__GPIO_4_11			0x40b3
MX28_PAD_ENET0_TXD3__GPIO_4_12			0x40c3
MX28_PAD_ENET0_RX_CLK__GPIO_4_13		0x40d3
MX28_PAD_ENET0_COL__GPIO_4_14			0x40e3
MX28_PAD_ENET0_CRS__GPIO_4_15			0x40f3
MX28_PAD_ENET_CLK__GPIO_4_16			0x4103
MX28_PAD_JTAG_RTCK__GPIO_4_20			0x4143

Valid values for i.MX23 pinmux-id:

pinmux						id
------						--
MX23_PAD_GPMI_D00__GPMI_D00			0x0000
MX23_PAD_GPMI_D01__GPMI_D01			0x0010
MX23_PAD_GPMI_D02__GPMI_D02			0x0020
MX23_PAD_GPMI_D03__GPMI_D03			0x0030
MX23_PAD_GPMI_D04__GPMI_D04			0x0040
MX23_PAD_GPMI_D05__GPMI_D05			0x0050
MX23_PAD_GPMI_D06__GPMI_D06			0x0060
MX23_PAD_GPMI_D07__GPMI_D07			0x0070
MX23_PAD_GPMI_D08__GPMI_D08			0x0080
MX23_PAD_GPMI_D09__GPMI_D09			0x0090
MX23_PAD_GPMI_D10__GPMI_D10			0x00a0
MX23_PAD_GPMI_D11__GPMI_D11			0x00b0
MX23_PAD_GPMI_D12__GPMI_D12			0x00c0
MX23_PAD_GPMI_D13__GPMI_D13			0x00d0
MX23_PAD_GPMI_D14__GPMI_D14			0x00e0
MX23_PAD_GPMI_D15__GPMI_D15			0x00f0
MX23_PAD_GPMI_CLE__GPMI_CLE			0x0100
MX23_PAD_GPMI_ALE__GPMI_ALE			0x0110
MX23_PAD_GPMI_CE2N__GPMI_CE2N			0x0120
MX23_PAD_GPMI_RDY0__GPMI_RDY0			0x0130
MX23_PAD_GPMI_RDY1__GPMI_RDY1			0x0140
MX23_PAD_GPMI_RDY2__GPMI_RDY2			0x0150
MX23_PAD_GPMI_RDY3__GPMI_RDY3			0x0160
MX23_PAD_GPMI_WPN__GPMI_WPN			0x0170
MX23_PAD_GPMI_WRN__GPMI_WRN			0x0180
MX23_PAD_GPMI_RDN__GPMI_RDN			0x0190
MX23_PAD_AUART1_CTS__AUART1_CTS			0x01a0
MX23_PAD_AUART1_RTS__AUART1_RTS			0x01b0
MX23_PAD_AUART1_RX__AUART1_RX			0x01c0
MX23_PAD_AUART1_TX__AUART1_TX			0x01d0
MX23_PAD_I2C_SCL__I2C_SCL			0x01e0
MX23_PAD_I2C_SDA__I2C_SDA			0x01f0
MX23_PAD_LCD_D00__LCD_D00			0x1000
MX23_PAD_LCD_D01__LCD_D01			0x1010
MX23_PAD_LCD_D02__LCD_D02			0x1020
MX23_PAD_LCD_D03__LCD_D03			0x1030
MX23_PAD_LCD_D04__LCD_D04			0x1040
MX23_PAD_LCD_D05__LCD_D05			0x1050
MX23_PAD_LCD_D06__LCD_D06			0x1060
MX23_PAD_LCD_D07__LCD_D07			0x1070
MX23_PAD_LCD_D08__LCD_D08			0x1080
MX23_PAD_LCD_D09__LCD_D09			0x1090
MX23_PAD_LCD_D10__LCD_D10			0x10a0
MX23_PAD_LCD_D11__LCD_D11			0x10b0
MX23_PAD_LCD_D12__LCD_D12			0x10c0
MX23_PAD_LCD_D13__LCD_D13			0x10d0
MX23_PAD_LCD_D14__LCD_D14			0x10e0
MX23_PAD_LCD_D15__LCD_D15			0x10f0
MX23_PAD_LCD_D16__LCD_D16			0x1100
MX23_PAD_LCD_D17__LCD_D17			0x1110
MX23_PAD_LCD_RESET__LCD_RESET			0x1120
MX23_PAD_LCD_RS__LCD_RS				0x1130
MX23_PAD_LCD_WR__LCD_WR				0x1140
MX23_PAD_LCD_CS__LCD_CS				0x1150
MX23_PAD_LCD_DOTCK__LCD_DOTCK			0x1160
MX23_PAD_LCD_ENABLE__LCD_ENABLE			0x1170
MX23_PAD_LCD_HSYNC__LCD_HSYNC			0x1180
MX23_PAD_LCD_VSYNC__LCD_VSYNC			0x1190
MX23_PAD_PWM0__PWM0				0x11a0
MX23_PAD_PWM1__PWM1				0x11b0
MX23_PAD_PWM2__PWM2				0x11c0
MX23_PAD_PWM3__PWM3				0x11d0
MX23_PAD_PWM4__PWM4				0x11e0
MX23_PAD_SSP1_CMD__SSP1_CMD			0x2000
MX23_PAD_SSP1_DETECT__SSP1_DETECT		0x2010
MX23_PAD_SSP1_DATA0__SSP1_DATA0			0x2020
MX23_PAD_SSP1_DATA1__SSP1_DATA1			0x2030
MX23_PAD_SSP1_DATA2__SSP1_DATA2			0x2040
MX23_PAD_SSP1_DATA3__SSP1_DATA3			0x2050
MX23_PAD_SSP1_SCK__SSP1_SCK			0x2060
MX23_PAD_ROTARYA__ROTARYA			0x2070
MX23_PAD_ROTARYB__ROTARYB			0x2080
MX23_PAD_EMI_A00__EMI_A00			0x2090
MX23_PAD_EMI_A01__EMI_A01			0x20a0
MX23_PAD_EMI_A02__EMI_A02			0x20b0
MX23_PAD_EMI_A03__EMI_A03			0x20c0
MX23_PAD_EMI_A04__EMI_A04			0x20d0
MX23_PAD_EMI_A05__EMI_A05			0x20e0
MX23_PAD_EMI_A06__EMI_A06			0x20f0
MX23_PAD_EMI_A07__EMI_A07			0x2100
MX23_PAD_EMI_A08__EMI_A08			0x2110
MX23_PAD_EMI_A09__EMI_A09			0x2120
MX23_PAD_EMI_A10__EMI_A10			0x2130
MX23_PAD_EMI_A11__EMI_A11			0x2140
MX23_PAD_EMI_A12__EMI_A12			0x2150
MX23_PAD_EMI_BA0__EMI_BA0			0x2160
MX23_PAD_EMI_BA1__EMI_BA1			0x2170
MX23_PAD_EMI_CASN__EMI_CASN			0x2180
MX23_PAD_EMI_CE0N__EMI_CE0N			0x2190
MX23_PAD_EMI_CE1N__EMI_CE1N			0x21a0
MX23_PAD_GPMI_CE1N__GPMI_CE1N			0x21b0
MX23_PAD_GPMI_CE0N__GPMI_CE0N			0x21c0
MX23_PAD_EMI_CKE__EMI_CKE			0x21d0
MX23_PAD_EMI_RASN__EMI_RASN			0x21e0
MX23_PAD_EMI_WEN__EMI_WEN			0x21f0
MX23_PAD_EMI_D00__EMI_D00			0x3000
MX23_PAD_EMI_D01__EMI_D01			0x3010
MX23_PAD_EMI_D02__EMI_D02			0x3020
MX23_PAD_EMI_D03__EMI_D03			0x3030
MX23_PAD_EMI_D04__EMI_D04			0x3040
MX23_PAD_EMI_D05__EMI_D05			0x3050
MX23_PAD_EMI_D06__EMI_D06			0x3060
MX23_PAD_EMI_D07__EMI_D07			0x3070
MX23_PAD_EMI_D08__EMI_D08			0x3080
MX23_PAD_EMI_D09__EMI_D09			0x3090
MX23_PAD_EMI_D10__EMI_D10			0x30a0
MX23_PAD_EMI_D11__EMI_D11			0x30b0
MX23_PAD_EMI_D12__EMI_D12			0x30c0
MX23_PAD_EMI_D13__EMI_D13			0x30d0
MX23_PAD_EMI_D14__EMI_D14			0x30e0
MX23_PAD_EMI_D15__EMI_D15			0x30f0
MX23_PAD_EMI_DQM0__EMI_DQM0			0x3100
MX23_PAD_EMI_DQM1__EMI_DQM1			0x3110
MX23_PAD_EMI_DQS0__EMI_DQS0			0x3120
MX23_PAD_EMI_DQS1__EMI_DQS1			0x3130
MX23_PAD_EMI_CLK__EMI_CLK			0x3140
MX23_PAD_EMI_CLKN__EMI_CLKN			0x3150
MX23_PAD_GPMI_D00__LCD_D8			0x0001
MX23_PAD_GPMI_D01__LCD_D9			0x0011
MX23_PAD_GPMI_D02__LCD_D10			0x0021
MX23_PAD_GPMI_D03__LCD_D11			0x0031
MX23_PAD_GPMI_D04__LCD_D12			0x0041
MX23_PAD_GPMI_D05__LCD_D13			0x0051
MX23_PAD_GPMI_D06__LCD_D14			0x0061
MX23_PAD_GPMI_D07__LCD_D15			0x0071
MX23_PAD_GPMI_D08__LCD_D18			0x0081
MX23_PAD_GPMI_D09__LCD_D19			0x0091
MX23_PAD_GPMI_D10__LCD_D20			0x00a1
MX23_PAD_GPMI_D11__LCD_D21			0x00b1
MX23_PAD_GPMI_D12__LCD_D22			0x00c1
MX23_PAD_GPMI_D13__LCD_D23			0x00d1
MX23_PAD_GPMI_D14__AUART2_RX			0x00e1
MX23_PAD_GPMI_D15__AUART2_TX			0x00f1
MX23_PAD_GPMI_CLE__LCD_D16			0x0101
MX23_PAD_GPMI_ALE__LCD_D17			0x0111
MX23_PAD_GPMI_CE2N__ATA_A2			0x0121
MX23_PAD_AUART1_RTS__IR_CLK			0x01b1
MX23_PAD_AUART1_RX__IR_RX			0x01c1
MX23_PAD_AUART1_TX__IR_TX			0x01d1
MX23_PAD_I2C_SCL__GPMI_RDY2			0x01e1
MX23_PAD_I2C_SDA__GPMI_CE2N			0x01f1
MX23_PAD_LCD_D00__ETM_DA8			0x1001
MX23_PAD_LCD_D01__ETM_DA9			0x1011
MX23_PAD_LCD_D02__ETM_DA10			0x1021
MX23_PAD_LCD_D03__ETM_DA11			0x1031
MX23_PAD_LCD_D04__ETM_DA12			0x1041
MX23_PAD_LCD_D05__ETM_DA13			0x1051
MX23_PAD_LCD_D06__ETM_DA14			0x1061
MX23_PAD_LCD_D07__ETM_DA15			0x1071
MX23_PAD_LCD_D08__ETM_DA0			0x1081
MX23_PAD_LCD_D09__ETM_DA1			0x1091
MX23_PAD_LCD_D10__ETM_DA2			0x10a1
MX23_PAD_LCD_D11__ETM_DA3			0x10b1
MX23_PAD_LCD_D12__ETM_DA4			0x10c1
MX23_PAD_LCD_D13__ETM_DA5			0x10d1
MX23_PAD_LCD_D14__ETM_DA6			0x10e1
MX23_PAD_LCD_D15__ETM_DA7			0x10f1
MX23_PAD_LCD_RESET__ETM_TCTL			0x1121
MX23_PAD_LCD_RS__ETM_TCLK			0x1131
MX23_PAD_LCD_DOTCK__GPMI_RDY3			0x1161
MX23_PAD_LCD_ENABLE__I2C_SCL			0x1171
MX23_PAD_LCD_HSYNC__I2C_SDA			0x1181
MX23_PAD_LCD_VSYNC__LCD_BUSY			0x1191
MX23_PAD_PWM0__ROTARYA				0x11a1
MX23_PAD_PWM1__ROTARYB				0x11b1
MX23_PAD_PWM2__GPMI_RDY3			0x11c1
MX23_PAD_PWM3__ETM_TCTL				0x11d1
MX23_PAD_PWM4__ETM_TCLK				0x11e1
MX23_PAD_SSP1_DETECT__GPMI_CE3N			0x2011
MX23_PAD_SSP1_DATA1__I2C_SCL			0x2031
MX23_PAD_SSP1_DATA2__I2C_SDA			0x2041
MX23_PAD_ROTARYA__AUART2_RTS			0x2071
MX23_PAD_ROTARYB__AUART2_CTS			0x2081
MX23_PAD_GPMI_D00__SSP2_DATA0			0x0002
MX23_PAD_GPMI_D01__SSP2_DATA1			0x0012
MX23_PAD_GPMI_D02__SSP2_DATA2			0x0022
MX23_PAD_GPMI_D03__SSP2_DATA3			0x0032
MX23_PAD_GPMI_D04__SSP2_DATA4			0x0042
MX23_PAD_GPMI_D05__SSP2_DATA5			0x0052
MX23_PAD_GPMI_D06__SSP2_DATA6			0x0062
MX23_PAD_GPMI_D07__SSP2_DATA7			0x0072
MX23_PAD_GPMI_D08__SSP1_DATA4			0x0082
MX23_PAD_GPMI_D09__SSP1_DATA5			0x0092
MX23_PAD_GPMI_D10__SSP1_DATA6			0x00a2
MX23_PAD_GPMI_D11__SSP1_DATA7			0x00b2
MX23_PAD_GPMI_D15__GPMI_CE3N			0x00f2
MX23_PAD_GPMI_RDY0__SSP2_DETECT			0x0132
MX23_PAD_GPMI_RDY1__SSP2_CMD			0x0142
MX23_PAD_GPMI_WRN__SSP2_SCK			0x0182
MX23_PAD_AUART1_CTS__SSP1_DATA4			0x01a2
MX23_PAD_AUART1_RTS__SSP1_DATA5			0x01b2
MX23_PAD_AUART1_RX__SSP1_DATA6			0x01c2
MX23_PAD_AUART1_TX__SSP1_DATA7			0x01d2
MX23_PAD_I2C_SCL__AUART1_TX			0x01e2
MX23_PAD_I2C_SDA__AUART1_RX			0x01f2
MX23_PAD_LCD_D08__SAIF2_SDATA0			0x1082
MX23_PAD_LCD_D09__SAIF1_SDATA0			0x1092
MX23_PAD_LCD_D10__SAIF_MCLK_BITCLK		0x10a2
MX23_PAD_LCD_D11__SAIF_LRCLK			0x10b2
MX23_PAD_LCD_D12__SAIF2_SDATA1			0x10c2
MX23_PAD_LCD_D13__SAIF2_SDATA2			0x10d2
MX23_PAD_LCD_D14__SAIF1_SDATA2			0x10e2
MX23_PAD_LCD_D15__SAIF1_SDATA1			0x10f2
MX23_PAD_LCD_D16__SAIF_ALT_BITCLK		0x1102
MX23_PAD_LCD_RESET__GPMI_CE3N			0x1122
MX23_PAD_PWM0__DUART_RX				0x11a2
MX23_PAD_PWM1__DUART_TX				0x11b2
MX23_PAD_PWM3__AUART1_CTS			0x11d2
MX23_PAD_PWM4__AUART1_RTS			0x11e2
MX23_PAD_SSP1_CMD__JTAG_TDO			0x2002
MX23_PAD_SSP1_DETECT__USB_OTG_ID		0x2012
MX23_PAD_SSP1_DATA0__JTAG_TDI			0x2022
MX23_PAD_SSP1_DATA1__JTAG_TCLK			0x2032
MX23_PAD_SSP1_DATA2__JTAG_RTCK			0x2042
MX23_PAD_SSP1_DATA3__JTAG_TMS			0x2052
MX23_PAD_SSP1_SCK__JTAG_TRST			0x2062
MX23_PAD_ROTARYA__SPDIF				0x2072
MX23_PAD_ROTARYB__GPMI_CE3N			0x2082
MX23_PAD_GPMI_D00__GPIO_0_0			0x0003
MX23_PAD_GPMI_D01__GPIO_0_1			0x0013
MX23_PAD_GPMI_D02__GPIO_0_2			0x0023
MX23_PAD_GPMI_D03__GPIO_0_3			0x0033
MX23_PAD_GPMI_D04__GPIO_0_4			0x0043
MX23_PAD_GPMI_D05__GPIO_0_5			0x0053
MX23_PAD_GPMI_D06__GPIO_0_6			0x0063
MX23_PAD_GPMI_D07__GPIO_0_7			0x0073
MX23_PAD_GPMI_D08__GPIO_0_8			0x0083
MX23_PAD_GPMI_D09__GPIO_0_9			0x0093
MX23_PAD_GPMI_D10__GPIO_0_10			0x00a3
MX23_PAD_GPMI_D11__GPIO_0_11			0x00b3
MX23_PAD_GPMI_D12__GPIO_0_12			0x00c3
MX23_PAD_GPMI_D13__GPIO_0_13			0x00d3
MX23_PAD_GPMI_D14__GPIO_0_14			0x00e3
MX23_PAD_GPMI_D15__GPIO_0_15			0x00f3
MX23_PAD_GPMI_CLE__GPIO_0_16			0x0103
MX23_PAD_GPMI_ALE__GPIO_0_17			0x0113
MX23_PAD_GPMI_CE2N__GPIO_0_18			0x0123
MX23_PAD_GPMI_RDY0__GPIO_0_19			0x0133
MX23_PAD_GPMI_RDY1__GPIO_0_20			0x0143
MX23_PAD_GPMI_RDY2__GPIO_0_21			0x0153
MX23_PAD_GPMI_RDY3__GPIO_0_22			0x0163
MX23_PAD_GPMI_WPN__GPIO_0_23			0x0173
MX23_PAD_GPMI_WRN__GPIO_0_24			0x0183
MX23_PAD_GPMI_RDN__GPIO_0_25			0x0193
MX23_PAD_AUART1_CTS__GPIO_0_26			0x01a3
MX23_PAD_AUART1_RTS__GPIO_0_27			0x01b3
MX23_PAD_AUART1_RX__GPIO_0_28			0x01c3
MX23_PAD_AUART1_TX__GPIO_0_29			0x01d3
MX23_PAD_I2C_SCL__GPIO_0_30			0x01e3
MX23_PAD_I2C_SDA__GPIO_0_31			0x01f3
MX23_PAD_LCD_D00__GPIO_1_0			0x1003
MX23_PAD_LCD_D01__GPIO_1_1			0x1013
MX23_PAD_LCD_D02__GPIO_1_2			0x1023
MX23_PAD_LCD_D03__GPIO_1_3			0x1033
MX23_PAD_LCD_D04__GPIO_1_4			0x1043
MX23_PAD_LCD_D05__GPIO_1_5			0x1053
MX23_PAD_LCD_D06__GPIO_1_6			0x1063
MX23_PAD_LCD_D07__GPIO_1_7			0x1073
MX23_PAD_LCD_D08__GPIO_1_8			0x1083
MX23_PAD_LCD_D09__GPIO_1_9			0x1093
MX23_PAD_LCD_D10__GPIO_1_10			0x10a3
MX23_PAD_LCD_D11__GPIO_1_11			0x10b3
MX23_PAD_LCD_D12__GPIO_1_12			0x10c3
MX23_PAD_LCD_D13__GPIO_1_13			0x10d3
MX23_PAD_LCD_D14__GPIO_1_14			0x10e3
MX23_PAD_LCD_D15__GPIO_1_15			0x10f3
MX23_PAD_LCD_D16__GPIO_1_16			0x1103
MX23_PAD_LCD_D17__GPIO_1_17			0x1113
MX23_PAD_LCD_RESET__GPIO_1_18			0x1123
MX23_PAD_LCD_RS__GPIO_1_19			0x1133
MX23_PAD_LCD_WR__GPIO_1_20			0x1143
MX23_PAD_LCD_CS__GPIO_1_21			0x1153
MX23_PAD_LCD_DOTCK__GPIO_1_22			0x1163
MX23_PAD_LCD_ENABLE__GPIO_1_23			0x1173
MX23_PAD_LCD_HSYNC__GPIO_1_24			0x1183
MX23_PAD_LCD_VSYNC__GPIO_1_25			0x1193
MX23_PAD_PWM0__GPIO_1_26			0x11a3
MX23_PAD_PWM1__GPIO_1_27			0x11b3
MX23_PAD_PWM2__GPIO_1_28			0x11c3
MX23_PAD_PWM3__GPIO_1_29			0x11d3
MX23_PAD_PWM4__GPIO_1_30			0x11e3
MX23_PAD_SSP1_CMD__GPIO_2_0			0x2003
MX23_PAD_SSP1_DETECT__GPIO_2_1			0x2013
MX23_PAD_SSP1_DATA0__GPIO_2_2			0x2023
MX23_PAD_SSP1_DATA1__GPIO_2_3			0x2033
MX23_PAD_SSP1_DATA2__GPIO_2_4			0x2043
MX23_PAD_SSP1_DATA3__GPIO_2_5			0x2053
MX23_PAD_SSP1_SCK__GPIO_2_6			0x2063
MX23_PAD_ROTARYA__GPIO_2_7			0x2073
MX23_PAD_ROTARYB__GPIO_2_8			0x2083
MX23_PAD_EMI_A00__GPIO_2_9			0x2093
MX23_PAD_EMI_A01__GPIO_2_10			0x20a3
MX23_PAD_EMI_A02__GPIO_2_11			0x20b3
MX23_PAD_EMI_A03__GPIO_2_12			0x20c3
MX23_PAD_EMI_A04__GPIO_2_13			0x20d3
MX23_PAD_EMI_A05__GPIO_2_14			0x20e3
MX23_PAD_EMI_A06__GPIO_2_15			0x20f3
MX23_PAD_EMI_A07__GPIO_2_16			0x2103
MX23_PAD_EMI_A08__GPIO_2_17			0x2113
MX23_PAD_EMI_A09__GPIO_2_18			0x2123
MX23_PAD_EMI_A10__GPIO_2_19			0x2133
MX23_PAD_EMI_A11__GPIO_2_20			0x2143
MX23_PAD_EMI_A12__GPIO_2_21			0x2153
MX23_PAD_EMI_BA0__GPIO_2_22			0x2163
MX23_PAD_EMI_BA1__GPIO_2_23			0x2173
MX23_PAD_EMI_CASN__GPIO_2_24			0x2183
MX23_PAD_EMI_CE0N__GPIO_2_25			0x2193
MX23_PAD_EMI_CE1N__GPIO_2_26			0x21a3
MX23_PAD_GPMI_CE1N__GPIO_2_27			0x21b3
MX23_PAD_GPMI_CE0N__GPIO_2_28			0x21c3
MX23_PAD_EMI_CKE__GPIO_2_29			0x21d3
MX23_PAD_EMI_RASN__GPIO_2_30			0x21e3
MX23_PAD_EMI_WEN__GPIO_2_31			0x21f3
