Freescale Localbus UPM programmed to work with NAND flash

Required properties:
- compatible : "fsl,upm-nand".
- reg : should specify localbus chip select and size used for the chip.
- fsl,upm-addr-offset : UPM pattern offset for the address latch.
- fsl,upm-cmd-offset : UPM pattern offset for the command latch.

Optional properties:
- fsl,upm-wait-flags : add chip-dependent short delays after running the
	UPM pattern (0x1), after writing a data byte (0x2) or after
	writing out a buffer (0x4).
- fsl,upm-addr-line-cs-offsets : address offsets for multi-chip support.
	The corresponding address lines are used to select the chip.
- gpios : may specify optional GPIOs connected to the Ready-Not-Busy pins
	(R/B#). For multi-chip devices, "n" GPIO definitions are required
	according to the number of chips.
- chip-delay : chip dependent delay for transferring data from array to
	read registers (tR). Required if property "gpios" is not used
	(R/B# pins not connected).

Examples:

upm@1,0 {
	compatible = "fsl,upm-nand";
	reg = <1 0 1>;
	fsl,upm-addr-offset = <16>;
	fsl,upm-cmd-offset = <8>;
	gpios = <&qe_pio_e 18 0>;

	flash {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "...";

		partition@0 {
			...
		};
	};
};

upm@3,0 {
	#address-cells = <0>;
	#size-cells = <0>;
	compatible = "tqc,tqm8548-upm-nand", "fsl,upm-nand";
	reg = <3 0x0 0x800>;
	fsl,upm-addr-offset = <0x10>;
	fsl,upm-cmd-offset = <0x08>;
	/* Multi-chip NAND device */
	fsl,upm-addr-line-cs-offsets = <0x0 0x200>;
	fsl,upm-wait-flags = <0x5>;
	chip-delay = <25>; // in micro-seconds

	nand@0 {
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			    label = "fs";
			    reg = <0x00000000 0x10000000>;
		};
	};
};
