ALC5632 audio CODEC

This device supports I2C only.

Required properties:

  - compatible : "realtek,alc5632"

  - reg : the I2C address of the device.

  - gpio-controller : Indicates this device is a GPIO controller.

  - #gpio-cells : Should be two. The first cell is the pin number and the
    second cell is used to specify optional parameters (currently unused).

Example:

alc5632: alc5632@1e {
	compatible = "realtek,alc5632";
	reg = <0x1a>;

	gpio-controller;
	#gpio-cells = <2>;
};
