NVIDIA Tegra30 AHUB (Audio Hub)

Required properties:
- compatible : "nvidia,tegra30-ahub"
- reg : Should contain the register physical address and length for each of
  the AHUB's APBIF registers and the AHUB's own registers.
- interrupts : Should contain AHUB interrupt
- nvidia,dma-request-selector : The Tegra DMA controller's phandle and
  request selector for the first APBIF channel.
- ranges : The bus address mapping for the configlink register bus.
  Can be empty since the mapping is 1:1.
- #address-cells : For the configlink bus. Should be <1>;
- #size-cells : For the configlink bus. Should be <1>.

AHUB client modules need to specify the IDs of their CIFs (Client InterFaces).
For RX CIFs, the numbers indicate the register number within AHUB routing
register space (APBIF 0..3 RX, I2S 0..5 RX, DAM 0..2 RX 0..1, SPDIF RX 0..1).
For TX CIFs, the numbers indicate the bit position within the AHUB routing
registers (APBIF 0..3 TX, I2S 0..5 TX, DAM 0..2 TX, SPDIF TX 0..1).

Example:

ahub@70080000 {
	compatible = "nvidia,tegra30-ahub";
	reg = <0x70080000 0x200 0x70080200 0x100>;
	interrupts = < 0 103 0x04 >;
	nvidia,dma-request-selector = <&apbdma 1>;

	ranges;
	#address-cells = <1>;
	#size-cells = <1>;
};
