PHY nodes

Required properties:

 - device_type : Should be "ethernet-phy"
 - interrupts : <a b> where a is the interrupt number and b is a
   field that represents an encoding of the sense and level
   information for the interrupt.  This should be encoded based on
   the information in section 2) depending on the type of interrupt
   controller you have.
 - interrupt-parent : the phandle for the interrupt controller that
   services interrupts for this device.
 - reg : The ID number for the phy, usually a small integer
 - linux,phandle :  phandle for this node; likely referenced by an
   ethernet controller node.

Optional Properties:

- compatible: Compatible list, may contain
  "ethernet-phy-ieee802.3-c22" or "ethernet-phy-ieee802.3-c45" for
  PHYs that implement IEEE802.3 clause 22 or IEEE802.3 clause 45
  specifications. If neither of these are specified, the default is to
  assume clause 22. The compatible list may also contain other
  elements.

Example:

ethernet-phy@0 {
	compatible = "ethernet-phy-ieee802.3-c22";
	linux,phandle = <2452000>;
	interrupt-parent = <40000>;
	interrupts = <35 1>;
	reg = <0>;
	device_type = "ethernet-phy";
};
