* Freescale MXS LCD Interface (LCDIF)

Required properties:
- compatible: Should be "fsl,<chip>-lcdif".  Supported chips include
  imx23 and imx28.
- reg: Address and length of the register set for lcdif
- interrupts: Should contain lcdif interrupts

Optional properties:
- panel-enable-gpios : Should specify the gpio for panel enable

Examples:

lcdif@80030000 {
	compatible = "fsl,imx28-lcdif";
	reg = <0x80030000 2000>;
	interrupts = <38 86>;
	panel-enable-gpios = <&gpio3 30 0>;
};
