What:		/sys/bus/i2c/devices/.../output_hvled[n]
Date:		April 2012
KernelVersion:	3.5
Contact:	Johan Hovold <jhovold@gmail.com>
Description:
		Set the controlling backlight device for high-voltage current
		sink HVLED[n] (n = 1, 2) (0, 1).

What:		/sys/bus/i2c/devices/.../output_lvled[n]
Date:		April 2012
KernelVersion:	3.5
Contact:	Johan Hovold <jhovold@gmail.com>
Description:
		Set the controlling led device for low-voltage current sink
		LVLED[n] (n = 1..5) (0..3).
