NVIDIA compliant embedded controller

Required properties:
- compatible : should be "nvidia,nvec".
- reg : the iomem of the i2c slave controller
- interrupts : the interrupt line of the i2c slave controller
- clock-frequency : the frequency of the i2c bus
- gpios : the gpio used for ec request
- slave-addr: the i2c address of the slave controller
