# reset<a name="EN-US_TOPIC_0000001053359638"></a>

-   [Command Function](#section366714216619)
-   [Syntax](#section8833164614615)
-   [Parameter Description](#section12809111019453)
-   [Usage](#section15935131220717)
-   [Example](#section79281818476)
-   [Output](#section12742311179)

## Command Function<a name="section366714216619"></a>

This command is used to restart a device.

## Syntax<a name="section8833164614615"></a>

reset

## Parameter Description<a name="section12809111019453"></a>

None

## Usage<a name="section15935131220717"></a>

After the  **reset**  command is executed, the device restarts immediately.

## Example<a name="section79281818476"></a>

Enter  **reset**.

## Output<a name="section12742311179"></a>

None

