# Introduction to the Hi3518 Development Board<a name="EN-US_TOPIC_0000001054261054"></a>

-   [Hi3518](#section14862341445)
-   [Development Board Specifications](#section765112478446)

## Hi3518<a name="section14862341445"></a>

Hi3518E V300 is a next-generation system on chip \(SoC\) designed for the industry-dedicated smart HD IP camera. It introduces a next-generation image signal processor \(ISP\), the H.265 video compression encoder, and the advanced low-power process and architecture design, leading the industry in terms of low bit rate, high image quality, and low power consumption.

**Figure  1**  Front view of the Hi3518E V300 board<a name="fig1187174485310"></a>  
![](figures/front-view-of-the-hi3518e-v300-board.png "front-view-of-the-hi3518e-v300-board")

**Figure  2**  Rear view of the Hi3518E V300 board<a name="fig73195258113"></a>  


![](figures/hi3518正背面.png)

## Development Board Specifications<a name="section765112478446"></a>

**Table  1**  Specifications of the Hi3518 development board

<a name="t88739bdd7be845fab34087af8ab692f7"></a>
<table><thead align="left"><tr id="r7d87cdc7a09d445c824000228ae4a3b0"><th class="cellrowborder" valign="top" width="28.749999999999996%" id="mcps1.2.3.1.1"><p id="a8ea7b45c00a54e7abd826c3b2bc934dc"><a name="a8ea7b45c00a54e7abd826c3b2bc934dc"></a><a name="a8ea7b45c00a54e7abd826c3b2bc934dc"></a><strong id="b18619196194114"><a name="b18619196194114"></a><a name="b18619196194114"></a>Type</strong></p>
</th>
<th class="cellrowborder" valign="top" width="71.25%" id="mcps1.2.3.1.2"><p id="aac42bd02e83846b187c02d3e976c0b09"><a name="aac42bd02e83846b187c02d3e976c0b09"></a><a name="aac42bd02e83846b187c02d3e976c0b09"></a><strong id="b591334418397"><a name="b591334418397"></a><a name="b591334418397"></a>Description</strong></p>
</th>
</tr>
</thead>
<tbody><tr id="r9c0a0b643fd7495ab799c1eab9fbe1ec"><td class="cellrowborder" valign="top" width="28.749999999999996%" headers="mcps1.2.3.1.1 "><p id="a1a129c845a45444f9d0b7dcc3aabf4c3"><a name="a1a129c845a45444f9d0b7dcc3aabf4c3"></a><a name="a1a129c845a45444f9d0b7dcc3aabf4c3"></a>Processor core</p>
</td>
<td class="cellrowborder" valign="top" width="71.25%" headers="mcps1.2.3.1.2 "><a name="ul12459548104218"></a><a name="ul12459548104218"></a><ul id="ul12459548104218"><li>Hi3518E V300</li></ul>
</td>
</tr>
<tr id="row1527851224210"><td class="cellrowborder" valign="top" width="28.749999999999996%" headers="mcps1.2.3.1.1 "><p id="p1327911123424"><a name="p1327911123424"></a><a name="p1327911123424"></a>Imaging device</p>
</td>
<td class="cellrowborder" valign="top" width="71.25%" headers="mcps1.2.3.1.2 "><a name="ul49841342134210"></a><a name="ul49841342134210"></a><ul id="ul49841342134210"><li>1/2.9 F23</li></ul>
</td>
</tr>
<tr id="r79097125b7f64c189f67ac280cdacae9"><td class="cellrowborder" valign="top" width="28.749999999999996%" headers="mcps1.2.3.1.1 "><p id="a2bf783139e304d0f9bfeefc56a55dc66"><a name="a2bf783139e304d0f9bfeefc56a55dc66"></a><a name="a2bf783139e304d0f9bfeefc56a55dc66"></a>External interfaces</p>
</td>
<td class="cellrowborder" valign="top" width="71.25%" headers="mcps1.2.3.1.2 "><a name="u6a04d9aa22f6410f91bbcdaf902d0e5f"></a><a name="u6a04d9aa22f6410f91bbcdaf902d0e5f"></a><ul id="u6a04d9aa22f6410f91bbcdaf902d0e5f"><li>External microphone</li><li>External 8 Ω/1.5 W speaker</li></ul>
</td>
</tr>
<tr id="r785d104d71f6426aa9aab25d14a7581b"><td class="cellrowborder" valign="top" width="28.749999999999996%" headers="mcps1.2.3.1.1 "><p id="a59fb5f9ca2004dd2abeb636b2d4c04fa"><a name="a59fb5f9ca2004dd2abeb636b2d4c04fa"></a><a name="a59fb5f9ca2004dd2abeb636b2d4c04fa"></a>External memory interface</p>
</td>
<td class="cellrowborder" valign="top" width="71.25%" headers="mcps1.2.3.1.2 "><a name="u8f323b7322a14e109e2937b9660af0c4"></a><a name="u8f323b7322a14e109e2937b9660af0c4"></a><ul id="u8f323b7322a14e109e2937b9660af0c4"><li>TF card<p id="p167481654192716"><a name="p167481654192716"></a><a name="p167481654192716"></a>A maximum file size of 128 GB is allowed (FAT32 format).</p>
</li></ul>
</td>
</tr>
<tr id="rae3f8ef812894db3951e01b4a1b85438"><td class="cellrowborder" valign="top" width="28.749999999999996%" headers="mcps1.2.3.1.1 "><p id="a81cd5d5655a44c4cbfc0a35b9f65450a"><a name="a81cd5d5655a44c4cbfc0a35b9f65450a"></a><a name="a81cd5d5655a44c4cbfc0a35b9f65450a"></a>WLAN protocol</p>
</td>
<td class="cellrowborder" valign="top" width="71.25%" headers="mcps1.2.3.1.2 "><a name="ul1311935314215"></a><a name="ul1311935314215"></a><ul id="ul1311935314215"><li>802.11 b/g/n</li></ul>
</td>
</tr>
</tbody>
</table>

