# Initializing the Input Chip Driver and Registering the Driver with the HDF<a name="EN-US_TOPIC_0000001111682042"></a>

For details, see step  [Initialize the input chip driver and register the driver with the HDF](adapting-to-the-private-drivers-of-the-touchscreen.md).

