* TI - MPU (Main Processor Unit) subsystem

The MPU subsystem contain one or several ARM cores
depending of the version.
The MPU contain CPUs, GIC, L2 cache and a local PRCM.

Required properties:
- compatible : Should be "ti,omap3-mpu" for OMAP3
               Should be "ti,omap4-mpu" for OMAP4
- ti,hwmods: "mpu"

Examples:

- For an OMAP4 SMP system:

mpu {
    compatible = "ti,omap4-mpu";
    ti,hwmods = "mpu";
};


- For an OMAP3 monocore system:

mpu {
    compatible = "ti,omap3-mpu";
    ti,hwmods = "mpu";
};
