SMSC LAN91c111 Ethernet mac

Required properties:
- compatible = "smsc,lan91c111";
- reg : physical address and size of registers
- interrupts : interrupt connection

Optional properties:
- phy-device : phandle to Ethernet phy
- local-mac-address : Ethernet mac address to use
