Marvell Platforms Device Tree Bindings
----------------------------------------------------

PXA168 Aspenite Board
Required root node properties:
	- compatible = "mrvl,pxa168-aspenite", "mrvl,pxa168";
