Flash device on ARM Versatile board

Required properties:
- compatible : must be "arm,versatile-flash";
- bank-width : width in bytes of flash interface.

The device tree may optionally contain sub-nodes describing partitions of the
address space. See partition.txt for more detail.
