Flash device on ARM Versatile board

Required properties:
- compatible : must be "arm,versatile-flash";
- bank-width : width in bytes of flash interface.

Optional properties:
- Subnode partition map from mtd flash binding
