  Model name	Description
  ----------    -----------
ALC880
======
  3stack	3-jack in back and a headphone out
  3stack-digout	3-jack in back, a HP out and a SPDIF out
  5stack	5-jack in back, 2-jack in front
  5stack-digout	5-jack in back, 2-jack in front, a SPDIF out
  6stack	6-jack in back, 2-jack in front
  6stack-digout	6-jack with a SPDIF out
  w810		3-jack
  z71v		3-jack (HP shared SPDIF)
  asus		3-jack (ASUS Mobo)
  asus-w1v	ASUS W1V
  asus-dig	ASUS with SPDIF out
  asus-dig2	ASUS with SPDIF out (using GPIO2)
  uniwill	3-jack
  fujitsu	Fujitsu Laptops (Pi1536)
  F1734		2-jack
  lg		LG laptop (m1 express dual)
  lg-lw		LG LW20/LW25 laptop
  tcl		TCL S700
  clevo		Clevo laptops (m520G, m665n)
  medion	Medion Rim 2150
  test		for testing/debugging purpose, almost all controls can be
		adjusted.  Appearing only when compiled with
		$CONFIG_SND_DEBUG=y
  auto		auto-config reading BIOS (default)

ALC260
======
  hp		HP machines
  hp-3013	HP machines (3013-variant)
  hp-dc7600	HP DC7600
  fujitsu	Fujitsu S7020
  acer		Acer TravelMate
  will		Will laptops (PB V7900)
  replacer	Replacer 672V
  basic		fixed pin assignment (old default model)
  test		for testing/debugging purpose, almost all controls can
		adjusted.  Appearing only when compiled with
		$CONFIG_SND_DEBUG=y
  auto		auto-config reading BIOS (default)

ALC262
======
  fujitsu	Fujitsu Laptop
  hp-bpc	HP xw4400/6400/8400/9400 laptops
  hp-bpc-d7000	HP BPC D7000
  hp-tc-t5735	HP Thin Client T5735
  hp-rp5700	HP RP5700
  benq		Benq ED8
  benq-t31	Benq T31
  hippo		Hippo (ATI) with jack detection, Sony UX-90s
  hippo_1	Hippo (Benq) with jack detection
  sony-assamd	Sony ASSAMD
  toshiba-s06	Toshiba S06
  toshiba-rx1	Toshiba RX1
  tyan		Tyan Thunder n6650W (S2915-E)
  ultra		Samsung Q1 Ultra Vista model
  lenovo-3000	Lenovo 3000 y410
  nec		NEC Versa S9100
  basic		fixed pin assignment w/o SPDIF
  auto		auto-config reading BIOS (default)

ALC267/268
==========
  quanta-il1	Quanta IL1 mini-notebook
  3stack	3-stack model
  toshiba	Toshiba A205
  acer		Acer laptops
  acer-dmic	Acer laptops with digital-mic
  acer-aspire	Acer Aspire One
  dell		Dell OEM laptops (Vostro 1200)
  zepto		Zepto laptops
  test		for testing/debugging purpose, almost all controls can
		adjusted.  Appearing only when compiled with
		$CONFIG_SND_DEBUG=y
  auto		auto-config reading BIOS (default)

ALC269
======
  basic		Basic preset
  quanta	Quanta FL1
  eeepc-p703	ASUS Eeepc P703 P900A
  eeepc-p901	ASUS Eeepc P901 S101
  fujitsu	FSC Amilo
  auto		auto-config reading BIOS (default)

ALC662/663
==========
  3stack-dig	3-stack (2-channel) with SPDIF
  3stack-6ch	 3-stack (6-channel)
  3stack-6ch-dig 3-stack (6-channel) with SPDIF
  6stack-dig	 6-stack with SPDIF
  lenovo-101e	 Lenovo laptop
  eeepc-p701	ASUS Eeepc P701
  eeepc-ep20	ASUS Eeepc EP20
  ecs		ECS/Foxconn mobo
  m51va		ASUS M51VA
  g71v		ASUS G71V
  h13		ASUS H13
  g50v		ASUS G50V
  asus-mode1	ASUS
  asus-mode2	ASUS
  asus-mode3	ASUS
  asus-mode4	ASUS
  asus-mode5	ASUS
  asus-mode6	ASUS
  auto		auto-config reading BIOS (default)

ALC882/885
==========
  3stack-dig	3-jack with SPDIF I/O
  6stack-dig	6-jack digital with SPDIF I/O
  arima		Arima W820Di1
  targa		Targa T8, MSI-1049 T8
  asus-a7j	ASUS A7J
  asus-a7m	ASUS A7M
  macpro	MacPro support
  mbp3		Macbook Pro rev3
  imac24	iMac 24'' with jack detection
  w2jc		ASUS W2JC
  auto		auto-config reading BIOS (default)

ALC883/888
==========
  3stack-dig	3-jack with SPDIF I/O
  6stack-dig	6-jack digital with SPDIF I/O
  3stack-6ch    3-jack 6-channel
  3stack-6ch-dig 3-jack 6-channel with SPDIF I/O
  6stack-dig-demo  6-jack digital for Intel demo board
  acer		Acer laptops (Travelmate 3012WTMi, Aspire 5600, etc)
  acer-aspire	Acer Aspire 9810
  acer-aspire-4930g Acer Aspire 4930G
  medion	Medion Laptops
  medion-md2	Medion MD2
  targa-dig	Targa/MSI
  targa-2ch-dig	Targs/MSI with 2-channel
  laptop-eapd   3-jack with SPDIF I/O and EAPD (Clevo M540JE, M550JE)
  lenovo-101e	Lenovo 101E
  lenovo-nb0763	Lenovo NB0763
  lenovo-ms7195-dig Lenovo MS7195
  lenovo-sky	Lenovo Sky
  haier-w66	Haier W66
  3stack-hp	HP machines with 3stack (Lucknow, Samba boards)
  6stack-dell	Dell machines with 6stack (Inspiron 530)
  mitac		Mitac 8252D
  clevo-m720	Clevo M720 laptop series
  fujitsu-pi2515 Fujitsu AMILO Pi2515
  fujitsu-xa3530 Fujitsu AMILO XA3530
  3stack-6ch-intel Intel DG33* boards
  auto		auto-config reading BIOS (default)

ALC861/660
==========
  3stack	3-jack
  3stack-dig	3-jack with SPDIF I/O
  6stack-dig	6-jack with SPDIF I/O
  3stack-660	3-jack (for ALC660)
  uniwill-m31	Uniwill M31 laptop
  toshiba	Toshiba laptop support
  asus		Asus laptop support
  asus-laptop	ASUS F2/F3 laptops
  auto		auto-config reading BIOS (default)

ALC861VD/660VD
==============
  3stack	3-jack
  3stack-dig	3-jack with SPDIF OUT
  6stack-dig	6-jack with SPDIF OUT
  3stack-660	3-jack (for ALC660VD)
  3stack-660-digout 3-jack with SPDIF OUT (for ALC660VD)
  lenovo	Lenovo 3000 C200
  dallas	Dallas laptops
  hp		HP TX1000
  asus-v1s	ASUS V1Sn
  auto		auto-config reading BIOS (default)

CMI9880
=======
  minimal	3-jack in back
  min_fp	3-jack in back, 2-jack in front
  full		6-jack in back, 2-jack in front
  full_dig	6-jack in back, 2-jack in front, SPDIF I/O
  allout	5-jack in back, 2-jack in front, SPDIF out
  auto		auto-config reading BIOS (default)

AD1882 / AD1882A
================
  3stack	3-stack mode (default)
  6stack	6-stack mode

AD1884A / AD1883 / AD1984A / AD1984B
====================================
  desktop	3-stack desktop (default)
  laptop	laptop with HP jack sensing
  mobile	mobile devices with HP jack sensing
  thinkpad	Lenovo Thinkpad X300

AD1884
======
  N/A

AD1981
======
  basic		3-jack (default)
  hp		HP nx6320
  thinkpad	Lenovo Thinkpad T60/X60/Z60
  toshiba	Toshiba U205

AD1983
======
  N/A

AD1984
======
  basic		default configuration
  thinkpad	Lenovo Thinkpad T61/X61
  dell		Dell T3400

AD1986A
=======
  6stack	6-jack, separate surrounds (default)
  3stack	3-stack, shared surrounds
  laptop	2-channel only (FSC V2060, Samsung M50)
  laptop-eapd	2-channel with EAPD (ASUS A6J)
  laptop-automute 2-channel with EAPD and HP-automute (Lenovo N100)
  ultra		2-channel with EAPD (Samsung Ultra tablet PC)
  samsung	2-channel with EAPD (Samsung R65)

AD1988/AD1988B/AD1989A/AD1989B
==============================
  6stack	6-jack
  6stack-dig	ditto with SPDIF
  3stack	3-jack
  3stack-dig	ditto with SPDIF
  laptop	3-jack with hp-jack automute
  laptop-dig	ditto with SPDIF
  auto		auto-config reading BIOS (default)

Conexant 5045
=============
  laptop-hpsense    Laptop with HP sense (old model laptop)
  laptop-micsense   Laptop with Mic sense (old model fujitsu)
  laptop-hpmicsense Laptop with HP and Mic senses
  benq		Benq R55E
  test		for testing/debugging purpose, almost all controls
		can be adjusted.  Appearing only when compiled with
		$CONFIG_SND_DEBUG=y

Conexant 5047
=============
  laptop	Basic Laptop config 
  laptop-hp	Laptop config for some HP models (subdevice 30A5)
  laptop-eapd	Laptop config with EAPD support
  test		for testing/debugging purpose, almost all controls
		can be adjusted.  Appearing only when compiled with
		$CONFIG_SND_DEBUG=y

Conexant 5051
=============
  laptop	Basic Laptop config (default)
  hp		HP Spartan laptop
  hp-dv6736	HP dv6736
  lenovo-x200	Lenovo X200 laptop

STAC9200
========
  ref		Reference board
  dell-d21	Dell (unknown)
  dell-d22	Dell (unknown)
  dell-d23	Dell (unknown)
  dell-m21	Dell Inspiron 630m, Dell Inspiron 640m
  dell-m22	Dell Latitude D620, Dell Latitude D820
  dell-m23	Dell XPS M1710, Dell Precision M90
  dell-m24	Dell Latitude 120L
  dell-m25	Dell Inspiron E1505n
  dell-m26	Dell Inspiron 1501
  dell-m27	Dell Inspiron E1705/9400
  gateway-m4	Gateway laptops with EAPD control
  gateway-m4-2	Gateway laptops with EAPD control
  panasonic	Panasonic CF-74
  auto		BIOS setup (default)

STAC9205/9254
=============
  ref		Reference board
  dell-m42	Dell (unknown)
  dell-m43	Dell Precision
  dell-m44	Dell Inspiron
  eapd		Keep EAPD on (e.g. Gateway T1616)
  auto		BIOS setup (default)

STAC9220/9221
=============
  ref		Reference board
  3stack	D945 3stack
  5stack	D945 5stack + SPDIF
  intel-mac-v1	Intel Mac Type 1
  intel-mac-v2	Intel Mac Type 2
  intel-mac-v3	Intel Mac Type 3
  intel-mac-v4	Intel Mac Type 4
  intel-mac-v5	Intel Mac Type 5
  intel-mac-auto Intel Mac (detect type according to subsystem id)
  macmini	Intel Mac Mini (equivalent with type 3)
  macbook	Intel Mac Book (eq. type 5)
  macbook-pro-v1 Intel Mac Book Pro 1st generation (eq. type 3)
  macbook-pro	Intel Mac Book Pro 2nd generation (eq. type 3)
  imac-intel	Intel iMac (eq. type 2)
  imac-intel-20	Intel iMac (newer version) (eq. type 3)
  ecs202	ECS/PC chips
  dell-d81	Dell (unknown)
  dell-d82	Dell (unknown)
  dell-m81	Dell (unknown)
  dell-m82	Dell XPS M1210
  auto		BIOS setup (default)

STAC9202/9250/9251
==================
  ref		Reference board, base config
  m1		Some Gateway MX series laptops (NX560XL)
  m1-2		Some Gateway MX series laptops (MX6453)
  m2		Some Gateway MX series laptops (M255)
  m2-2		Some Gateway MX series laptops
  m3		Some Gateway MX series laptops
  m5		Some Gateway MX series laptops (MP6954)
  m6		Some Gateway NX series laptops
  auto		BIOS setup (default)

STAC9227/9228/9229/927x
=======================
  ref		Reference board
  ref-no-jd	Reference board without HP/Mic jack detection
  3stack	D965 3stack
  5stack	D965 5stack + SPDIF
  dell-3stack	Dell Dimension E520
  dell-bios	Fixes with Dell BIOS setup
  auto		BIOS setup (default)

STAC92HD71B*
============
  ref		Reference board
  dell-m4-1	Dell desktops
  dell-m4-2	Dell desktops
  dell-m4-3	Dell desktops
  hp-m4		HP mini 1000
  hp-dv5	HP dv series
  hp-hdx	HP HDX series
  auto		BIOS setup (default)

STAC92HD73*
===========
  ref		Reference board
  no-jd		BIOS setup but without jack-detection
  dell-m6-amic	Dell desktops/laptops with analog mics
  dell-m6-dmic	Dell desktops/laptops with digital mics
  dell-m6	Dell desktops/laptops with both type of mics
  dell-eq	Dell desktops/laptops
  auto		BIOS setup (default)

STAC92HD83*
===========
  ref		Reference board
  mic-ref	Reference board with power managment for ports
  dell-s14	Dell laptop
  auto		BIOS setup (default)

STAC9872
========
  vaio		VAIO laptop without SPDIF
  auto		BIOS setup (default)
