                          OSS Kernel Parameters
                          ~~~~~~~~~~~~~~~~~~~~~

See Documentation/kernel-parameters.txt for general information on
specifying module parameters.

This document may not be entirely up to date and comprehensive. The command
"modinfo -p ${modulename}" shows a current list of all parameters of a loadable
module. Loadable modules, after being loaded into the running kernel, also
reveal their parameters in /sys/module/${modulename}/parameters/. Some of these
parameters may be changed at runtime by the command
"echo -n ${value} > /sys/module/${modulename}/parameters/${parm}".


	ad1848=		[HW,OSS]
			Format: <io>,<irq>,<dma>,<dma2>,<type>

	aedsp16=	[HW,OSS] Audio Excel DSP 16
			Format: <io>,<irq>,<dma>,<mss_io>,<mpu_io>,<mpu_irq>
			See also header of sound/oss/aedsp16.c.

	dmasound=	[HW,OSS] Sound subsystem buffers

	mpu401=		[HW,OSS]
			Format: <io>,<irq>

	opl3=		[HW,OSS]
			Format: <io>

	pas2=		[HW,OSS] Format:
			<io>,<irq>,<dma>,<dma16>,<sb_io>,<sb_irq>,<sb_dma>,<sb_dma16>

	pss=		[HW,OSS] Personal Sound System (ECHO ESC614)
			Format:
			<io>,<mss_io>,<mss_irq>,<mss_dma>,<mpu_io>,<mpu_irq>

	sscape=		[HW,OSS]
			Format: <io>,<irq>,<dma>,<mpu_io>,<mpu_irq>

	trix=		[HW,OSS] MediaTrix AudioTrix Pro
			Format:
			<io>,<irq>,<dma>,<dma2>,<sb_io>,<sb_irq>,<sb_dma>,<mpu_io>,<mpu_irq>

	uart401=	[HW,OSS]
			Format: <io>,<irq>

	uart6850=	[HW,OSS]
			Format: <io>,<irq>

	waveartist=	[HW,OSS]
			Format: <io>,<irq>,<dma>,<dma2>
