<refentry id="vidioc-g-sliced-vbi-cap">
  <refmeta>
    <refentrytitle>ioctl VIDIOC_G_SLICED_VBI_CAP</refentrytitle>
    &manvol;
  </refmeta>

  <refnamediv>
    <refname>VIDIOC_G_SLICED_VBI_CAP</refname>
    <refpurpose>Query sliced VBI capabilities</refpurpose>
  </refnamediv>

  <refsynopsisdiv>
    <funcsynopsis>
      <funcprototype>
	<funcdef>int <function>ioctl</function></funcdef>
	<paramdef>int <parameter>fd</parameter></paramdef>
	<paramdef>int <parameter>request</parameter></paramdef>
	<paramdef>struct v4l2_sliced_vbi_cap *<parameter>argp</parameter></paramdef>
      </funcprototype>
    </funcsynopsis>
  </refsynopsisdiv>

  <refsect1>
    <title>Arguments</title>

    <variablelist>
      <varlistentry>
	<term><parameter>fd</parameter></term>
	<listitem>
	  <para>&fd;</para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><parameter>request</parameter></term>
	<listitem>
	  <para>VIDIOC_G_SLICED_VBI_CAP</para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><parameter>argp</parameter></term>
	<listitem>
	  <para></para>
	</listitem>
      </varlistentry>
    </variablelist>
  </refsect1>

  <refsect1>
    <title>Description</title>

    <para>To find out which data services are supported by a sliced
VBI capture or output device, applications initialize the
<structfield>type</structfield> field of a &v4l2-sliced-vbi-cap;,
clear the <structfield>reserved</structfield> array and
call the <constant>VIDIOC_G_SLICED_VBI_CAP</constant> ioctl. The
driver fills in the remaining fields or returns an &EINVAL; if the
sliced VBI API is unsupported or <structfield>type</structfield>
is invalid.</para>

    <para>Note the <structfield>type</structfield> field was added,
and the ioctl changed from read-only to write-read, in Linux 2.6.19.</para>

    <table pgwide="1" frame="none" id="v4l2-sliced-vbi-cap">
      <title>struct <structname>v4l2_sliced_vbi_cap</structname></title>
      <tgroup cols="5">
	<colspec colname="c1" colwidth="3*" />
	<colspec colname="c2" colwidth="3*" />
	<colspec colname="c3" colwidth="2*" />
	<colspec colname="c4" colwidth="2*" />
	<colspec colname="c5" colwidth="2*" />
	<spanspec spanname="hspan" namest="c3" nameend="c5" />
	<tbody valign="top">
	  <row>
	    <entry>__u16</entry>
	    <entry><structfield>service_set</structfield></entry>
	    <entry spanname="hspan">A set of all data services
supported by the driver. Equal to the union of all elements of the
<structfield>service_lines </structfield> array.</entry>
	  </row>
	  <row>
	    <entry>__u16</entry>
	    <entry><structfield>service_lines</structfield>[2][24]</entry>
	    <entry spanname="hspan">Each element of this array
contains a set of data services the hardware can look for or insert
into a particular scan line. Data services are defined in <xref
		linkend="vbi-services" />. Array indices map to ITU-R
line numbers (see also <xref
		linkend="vbi-525" /> and <xref
linkend="vbi-625" />) as follows:</entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry>Element</entry>
	    <entry>525 line systems</entry>
	    <entry>625 line systems</entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry><structfield>service_lines</structfield>[0][1]</entry>
	    <entry align="center">1</entry>
	    <entry align="center">1</entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry><structfield>service_lines</structfield>[0][23]</entry>
	    <entry align="center">23</entry>
	    <entry align="center">23</entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry><structfield>service_lines</structfield>[1][1]</entry>
	    <entry align="center">264</entry>
	    <entry align="center">314</entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry><structfield>service_lines</structfield>[1][23]</entry>
	    <entry align="center">286</entry>
	    <entry align="center">336</entry>
	  </row>
	  <row>
	    <entry></entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry spanname="hspan">The number of VBI lines the
hardware can capture or output per frame, or the number of services it
can identify on a given line may be limited. For example on PAL line
16 the hardware may be able to look for a VPS or Teletext signal, but
not both at the same time. Applications can learn about these limits
using the &VIDIOC-S-FMT; ioctl as described in <xref
		linkend="sliced" />.</entry>
	  </row>
	  <row>
	    <entry></entry>
	  </row>
	  <row>
	    <entry></entry>
	    <entry></entry>
	    <entry spanname="hspan">Drivers must set
<structfield>service_lines</structfield>[0][0] and
<structfield>service_lines</structfield>[1][0] to zero.</entry>
	  </row>
	  <row>
	    <entry>__u32</entry>
	    <entry><structfield>type</structfield></entry>
	    <entry>Type of the data stream, see <xref
		  linkend="v4l2-buf-type" />. Should be
<constant>V4L2_BUF_TYPE_SLICED_VBI_CAPTURE</constant> or
<constant>V4L2_BUF_TYPE_SLICED_VBI_OUTPUT</constant>.</entry>
	  </row>
	  <row>
	    <entry>__u32</entry>
	    <entry><structfield>reserved</structfield>[3]</entry>
	    <entry spanname="hspan">This array is reserved for future
extensions. Applications and drivers must set it to zero.</entry>
	  </row>
	</tbody>
      </tgroup>
    </table>

    <!-- See also dev-sliced-vbi.sgml -->
    <table pgwide="1" frame="none" id="vbi-services">
      <title>Sliced VBI services</title>
      <tgroup cols="5">
	<colspec colname="c1" colwidth="2*" />
	<colspec colname="c2" colwidth="1*" />
	<colspec colname="c3" colwidth="1*" />
	<colspec colname="c4" colwidth="2*" />
	<colspec colname="c5" colwidth="2*" />
	<spanspec spanname='rlp' namest='c3' nameend='c5' />
	<thead>
	  <row>
	    <entry>Symbol</entry>
	    <entry>Value</entry>
	    <entry>Reference</entry>
	    <entry>Lines, usually</entry>
	    <entry>Payload</entry>
	  </row>
	</thead>
	<tbody valign="top">
	  <row>
	    <entry><constant>V4L2_SLICED_TELETEXT_B</constant> (Teletext
System B)</entry>
	    <entry>0x0001</entry>
	    <entry><xref linkend="ets300706" />, <xref linkend="itu653" /></entry>
	    <entry>PAL/SECAM line 7-22, 320-335 (second field 7-22)</entry>
	    <entry>Last 42 of the 45 byte Teletext packet, that is
without clock run-in and framing code, lsb first transmitted.</entry>
	  </row>
	  <row>
	    <entry><constant>V4L2_SLICED_VPS</constant></entry>
	    <entry>0x0400</entry>
	    <entry><xref linkend="ets300231" /></entry>
	    <entry>PAL line 16</entry>
	    <entry>Byte number 3 to 15 according to Figure 9 of
ETS&nbsp;300&nbsp;231, lsb first transmitted.</entry>
	  </row>
	  <row>
	    <entry><constant>V4L2_SLICED_CAPTION_525</constant></entry>
	    <entry>0x1000</entry>
	    <entry><xref linkend="eia608" /></entry>
	    <entry>NTSC line 21, 284 (second field 21)</entry>
	    <entry>Two bytes in transmission order, including parity
bit, lsb first transmitted.</entry>
	  </row>
	  <row>
	    <entry><constant>V4L2_SLICED_WSS_625</constant></entry>
	    <entry>0x4000</entry>
	    <entry><xref linkend="en300294" />, <xref linkend="itu1119" /></entry>
	    <entry>PAL/SECAM line 23</entry>
	    <entry><screen>
Byte        0                 1
     msb         lsb  msb           lsb
Bit  7 6 5 4 3 2 1 0  x x 13 12 11 10 9
</screen></entry>
	  </row>
	  <row>
	    <entry><constant>V4L2_SLICED_VBI_525</constant></entry>
	    <entry>0x1000</entry>
	    <entry spanname="rlp">Set of services applicable to 525
line systems.</entry>
	  </row>
	  <row>
	    <entry><constant>V4L2_SLICED_VBI_625</constant></entry>
	    <entry>0x4401</entry>
	    <entry spanname="rlp">Set of services applicable to 625
line systems.</entry>
	  </row>
	</tbody>
      </tgroup>
    </table>

  </refsect1>

  <refsect1>
    &return-value;

    <variablelist>
      <varlistentry>
	<term><errorcode>EINVAL</errorcode></term>
	<listitem>
	  <para>The value in the <structfield>type</structfield> field is
wrong.</para>
	</listitem>
      </varlistentry>
    </variablelist>
  </refsect1>
</refentry>
