<!--- Licensed to the Apache Software Foundation (ASF) under one -->
<!--- or more contributor license agreements.  See the NOTICE file -->
<!--- distributed with this work for additional information -->
<!--- regarding copyright ownership.  The ASF licenses this file -->
<!--- to you under the Apache License, Version 2.0 (the -->
<!--- "License"); you may not use this file except in compliance -->
<!--- with the License.  You may obtain a copy of the License at -->

<!---   http://www.apache.org/licenses/LICENSE-2.0 -->

<!--- Unless required by applicable law or agreed to in writing, -->
<!--- software distributed under the License is distributed on an -->
<!--- "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY -->
<!--- KIND, either express or implied.  See the License for the -->
<!--- specific language governing permissions and limitations -->
<!--- under the License. -->

Running PaddleOCR text recognition model via TVM on bare metal Arm(R) Cortex(R)-M55 CPU and CMSIS-NN
===============================================================

This folder contains an example of how to use TVM to run a PaddleOCR model
on bare metal Cortex(R)-M55 CPU and CMSIS-NN.

Prerequisites
-------------
If the demo is run in the ci_cpu Docker container provided with TVM, then the following
software will already be installed.

If the demo is not run in the ci_cpu Docker container, then you will need the following:
- Software required to build and run the demo (These can all be installed by running 
  https://github.com/apache/tvm/blob/main/docker/install/ubuntu_install_ethosu_driver_stack.sh .)
  - [Fixed Virtual Platform (FVP) based on Arm(R) Corstone(TM)-300 software](https://developer.arm.com/tools-and-software/open-source-software/arm-platforms-software/arm-ecosystem-fvps)
  - [cmake 3.19.5](https://github.com/Kitware/CMake/releases/)
  - [GCC toolchain from Arm(R)](https://developer.arm.com/-/media/Files/downloads/gnu-rm/10-2020q4/gcc-arm-none-eabi-10-2020-q4-major-x86_64-linux.tar.bz2)
  - [Arm(R) Ethos(TM)-U NPU driver stack](https://review.mlplatform.org)
  - [CMSIS](https://github.com/ARM-software/CMSIS_5)
- The python libraries listed in the requirements.txt of this directory
  - These can be installed by running the following from the current directory:
    ```bash
    pip install -r ./requirements.txt
    ```

You will also need TVM which can either be:
  - Built from source (see [Install from Source](https://tvm.apache.org/docs/install/from_source.html))
    - When building from source, the following need to be set in config.cmake:
      - set(USE_CMSISNN ON)
      - set(USE_MICRO ON)
      - set(USE_LLVM ON)
  - Installed from TLCPack nightly(see [TLCPack](https://tlcpack.ai/))

You will need to update your PATH environment variable to include the path to cmake 3.19.5 and the FVP.
For example if you've installed these in ```/opt/arm``` , then you would do the following:
```bash
export PATH=/opt/arm/FVP_Corstone_SSE-300/models/Linux64_GCC-6.4:/opt/arm/cmake/bin:$PATH
```

Running the demo application
----------------------------
Type the following command to run the bare metal text recognition application ([src/demo_bare_metal.c](./src/demo_bare_metal.c)):

```bash
./run_demo.sh
```

If the Ethos(TM)-U platform and/or CMSIS have not been installed in /opt/arm/ethosu then
the locations for these can be specified as arguments to run_demo.sh, for example:

```bash
./run_demo.sh --cmsis_path /home/tvm-user/cmsis \
--ethosu_platform_path /home/tvm-user/ethosu/core_platform
```

This will:
- Download a PaddleOCR text recognition model
- Use tvmc to compile the text recognition model for Cortex(R)-M55 CPU and CMSIS-NN
- Create a C header file inputs.c containing the image data as a C array
- Create a C header file outputs.c containing a C array where the output of inference will be stored
- Build the demo application
- Run the demo application on a Fixed Virtual Platform (FVP) based on Arm(R) Corstone(TM)-300 software
- The application will report the text on the image and the corresponding score.

Using your own image
--------------------
The create_image.py script takes a single argument on the command line which is the path of the
image to be converted into an array of bytes for consumption by the model.

The demo can be modified to use an image of your choice by changing the following line in run_demo.sh

```bash
python3 ./convert_image.py path/to/image
```

Model description
-----------------
In this demo, the model we use is an English recognition model based on [PP-OCRv3](https://github.com/PaddlePaddle/PaddleOCR/blob/dygraph/doc/doc_ch/PP-OCRv3_introduction.md). PP-OCRv3 is the third version of the PP-OCR series model released by [PaddleOCR](https://github.com/PaddlePaddle/PaddleOCR). This series of models has the following features:
  - PP-OCRv3: ultra-lightweight OCR system: detection (3.6M) + direction classifier (1.4M) + recognition (12M) = 17.0M
  - Support more than 80 kinds of multi-language recognition models, including English, Chinese, French, German, Arabic, Korean, Japanese and so on. For details
  - Support vertical text recognition, and long text recognition

The text recognition model in PP-OCRv3 supports more than 80 languages. In the process of model development, since Arm(R) Cortex(R)-M55 CPU does not support rnn operator, we delete the unsupported operator based on the PP-OCRv3 text recognition model to obtain the current model.