* Freescale IMX6Q IOMUX Controller

Please refer to fsl,imx-pinctrl.txt in this directory for common binding part
and usage.

Required properties:
- compatible: "fsl,imx6q-iomuxc"
- fsl,pins: two integers array, represents a group of pins mux and config
  setting. The format is fsl,pins = <PIN_FUNC_ID CONFIG>, PIN_FUNC_ID is a
  pin working on a specific function, CONFIG is the pad setting value like
  pull-up for this pin. Please refer to imx6q datasheet for the valid pad
  config settings.

CONFIG bits definition:
PAD_CTL_HYS                     (1 << 16)
PAD_CTL_PUS_100K_DOWN           (0 << 14)
PAD_CTL_PUS_47K_UP              (1 << 14)
PAD_CTL_PUS_100K_UP             (2 << 14)
PAD_CTL_PUS_22K_UP              (3 << 14)
PAD_CTL_PUE                     (1 << 13)
PAD_CTL_PKE                     (1 << 12)
PAD_CTL_ODE                     (1 << 11)
PAD_CTL_SPEED_LOW               (1 << 6)
PAD_CTL_SPEED_MED               (2 << 6)
PAD_CTL_SPEED_HIGH              (3 << 6)
PAD_CTL_DSE_DISABLE             (0 << 3)
PAD_CTL_DSE_240ohm              (1 << 3)
PAD_CTL_DSE_120ohm              (2 << 3)
PAD_CTL_DSE_80ohm               (3 << 3)
PAD_CTL_DSE_60ohm               (4 << 3)
PAD_CTL_DSE_48ohm               (5 << 3)
PAD_CTL_DSE_40ohm               (6 << 3)
PAD_CTL_DSE_34ohm               (7 << 3)
PAD_CTL_SRE_FAST                (1 << 0)
PAD_CTL_SRE_SLOW                (0 << 0)

See below for available PIN_FUNC_ID for imx6q:
MX6Q_PAD_SD2_DAT1__USDHC2_DAT1			0
MX6Q_PAD_SD2_DAT1__ECSPI5_SS0			1
MX6Q_PAD_SD2_DAT1__WEIM_WEIM_CS_2		2
MX6Q_PAD_SD2_DAT1__AUDMUX_AUD4_TXFS		3
MX6Q_PAD_SD2_DAT1__KPP_COL_7			4
MX6Q_PAD_SD2_DAT1__GPIO_1_14			5
MX6Q_PAD_SD2_DAT1__CCM_WAIT			6
MX6Q_PAD_SD2_DAT1__ANATOP_TESTO_0		7
MX6Q_PAD_SD2_DAT2__USDHC2_DAT2			8
MX6Q_PAD_SD2_DAT2__ECSPI5_SS1			9
MX6Q_PAD_SD2_DAT2__WEIM_WEIM_CS_3		10
MX6Q_PAD_SD2_DAT2__AUDMUX_AUD4_TXD		11
MX6Q_PAD_SD2_DAT2__KPP_ROW_6			12
MX6Q_PAD_SD2_DAT2__GPIO_1_13			13
MX6Q_PAD_SD2_DAT2__CCM_STOP			14
MX6Q_PAD_SD2_DAT2__ANATOP_TESTO_1		15
MX6Q_PAD_SD2_DAT0__USDHC2_DAT0			16
MX6Q_PAD_SD2_DAT0__ECSPI5_MISO			17
MX6Q_PAD_SD2_DAT0__AUDMUX_AUD4_RXD		18
MX6Q_PAD_SD2_DAT0__KPP_ROW_7			19
MX6Q_PAD_SD2_DAT0__GPIO_1_15			20
MX6Q_PAD_SD2_DAT0__DCIC2_DCIC_OUT		21
MX6Q_PAD_SD2_DAT0__TESTO_2			22
MX6Q_PAD_RGMII_TXC__USBOH3_H2_DATA		23
MX6Q_PAD_RGMII_TXC__ENET_RGMII_TXC		24
MX6Q_PAD_RGMII_TXC__SPDIF_SPDIF_EXTCLK		25
MX6Q_PAD_RGMII_TXC__GPIO_6_19			26
MX6Q_PAD_RGMII_TXC__MIPI_CORE_DPHY_IN_0		27
MX6Q_PAD_RGMII_TXC__ANATOP_24M_OUT		28
MX6Q_PAD_RGMII_TD0__MIPI_HSI_CRL_TX_RDY		29
MX6Q_PAD_RGMII_TD0__ENET_RGMII_TD0		30
MX6Q_PAD_RGMII_TD0__GPIO_6_20			31
MX6Q_PAD_RGMII_TD0__MIPI_CORE_DPHY_IN_1		32
MX6Q_PAD_RGMII_TD1__MIPI_HSI_CRL_RX_FLG		33
MX6Q_PAD_RGMII_TD1__ENET_RGMII_TD1		34
MX6Q_PAD_RGMII_TD1__GPIO_6_21			35
MX6Q_PAD_RGMII_TD1__MIPI_CORE_DPHY_IN_2		36
MX6Q_PAD_RGMII_TD1__CCM_PLL3_BYP		37
MX6Q_PAD_RGMII_TD2__MIPI_HSI_CRL_RX_DTA		38
MX6Q_PAD_RGMII_TD2__ENET_RGMII_TD2		39
MX6Q_PAD_RGMII_TD2__GPIO_6_22			40
MX6Q_PAD_RGMII_TD2__MIPI_CORE_DPHY_IN_3		41
MX6Q_PAD_RGMII_TD2__CCM_PLL2_BYP		42
MX6Q_PAD_RGMII_TD3__MIPI_HSI_CRL_RX_WAK		43
MX6Q_PAD_RGMII_TD3__ENET_RGMII_TD3		44
MX6Q_PAD_RGMII_TD3__GPIO_6_23			45
MX6Q_PAD_RGMII_TD3__MIPI_CORE_DPHY_IN_4		46
MX6Q_PAD_RGMII_RX_CTL__USBOH3_H3_DATA		47
MX6Q_PAD_RGMII_RX_CTL__RGMII_RX_CTL		48
MX6Q_PAD_RGMII_RX_CTL__GPIO_6_24		49
MX6Q_PAD_RGMII_RX_CTL__MIPI_DPHY_IN_5		50
MX6Q_PAD_RGMII_RD0__MIPI_HSI_CRL_RX_RDY		51
MX6Q_PAD_RGMII_RD0__ENET_RGMII_RD0		52
MX6Q_PAD_RGMII_RD0__GPIO_6_25			53
MX6Q_PAD_RGMII_RD0__MIPI_CORE_DPHY_IN_6		54
MX6Q_PAD_RGMII_TX_CTL__USBOH3_H2_STROBE		55
MX6Q_PAD_RGMII_TX_CTL__RGMII_TX_CTL		56
MX6Q_PAD_RGMII_TX_CTL__GPIO_6_26		57
MX6Q_PAD_RGMII_TX_CTL__CORE_DPHY_IN_7		58
MX6Q_PAD_RGMII_TX_CTL__ANATOP_REF_OUT		59
MX6Q_PAD_RGMII_RD1__MIPI_HSI_CTRL_TX_FL		60
MX6Q_PAD_RGMII_RD1__ENET_RGMII_RD1		61
MX6Q_PAD_RGMII_RD1__GPIO_6_27			62
MX6Q_PAD_RGMII_RD1__CORE_DPHY_TEST_IN_8		63
MX6Q_PAD_RGMII_RD1__SJC_FAIL			64
MX6Q_PAD_RGMII_RD2__MIPI_HSI_CRL_TX_DTA		65
MX6Q_PAD_RGMII_RD2__ENET_RGMII_RD2		66
MX6Q_PAD_RGMII_RD2__GPIO_6_28			67
MX6Q_PAD_RGMII_RD2__MIPI_CORE_DPHY_IN_9		68
MX6Q_PAD_RGMII_RD3__MIPI_HSI_CRL_TX_WAK		69
MX6Q_PAD_RGMII_RD3__ENET_RGMII_RD3		70
MX6Q_PAD_RGMII_RD3__GPIO_6_29			71
MX6Q_PAD_RGMII_RD3__MIPI_CORE_DPHY_IN10		72
MX6Q_PAD_RGMII_RXC__USBOH3_H3_STROBE		73
MX6Q_PAD_RGMII_RXC__ENET_RGMII_RXC		74
MX6Q_PAD_RGMII_RXC__GPIO_6_30			75
MX6Q_PAD_RGMII_RXC__MIPI_CORE_DPHY_IN11		76
MX6Q_PAD_EIM_A25__WEIM_WEIM_A_25		77
MX6Q_PAD_EIM_A25__ECSPI4_SS1			78
MX6Q_PAD_EIM_A25__ECSPI2_RDY			79
MX6Q_PAD_EIM_A25__IPU1_DI1_PIN12		80
MX6Q_PAD_EIM_A25__IPU1_DI0_D1_CS		81
MX6Q_PAD_EIM_A25__GPIO_5_2			82
MX6Q_PAD_EIM_A25__HDMI_TX_CEC_LINE		83
MX6Q_PAD_EIM_A25__PL301_PER1_HBURST_0		84
MX6Q_PAD_EIM_EB2__WEIM_WEIM_EB_2		85
MX6Q_PAD_EIM_EB2__ECSPI1_SS0			86
MX6Q_PAD_EIM_EB2__CCM_DI1_EXT_CLK		87
MX6Q_PAD_EIM_EB2__IPU2_CSI1_D_19		88
MX6Q_PAD_EIM_EB2__HDMI_TX_DDC_SCL		89
MX6Q_PAD_EIM_EB2__GPIO_2_30			90
MX6Q_PAD_EIM_EB2__I2C2_SCL			91
MX6Q_PAD_EIM_EB2__SRC_BT_CFG_30			92
MX6Q_PAD_EIM_D16__WEIM_WEIM_D_16		93
MX6Q_PAD_EIM_D16__ECSPI1_SCLK			94
MX6Q_PAD_EIM_D16__IPU1_DI0_PIN5			95
MX6Q_PAD_EIM_D16__IPU2_CSI1_D_18		96
MX6Q_PAD_EIM_D16__HDMI_TX_DDC_SDA		97
MX6Q_PAD_EIM_D16__GPIO_3_16			98
MX6Q_PAD_EIM_D16__I2C2_SDA			99
MX6Q_PAD_EIM_D17__WEIM_WEIM_D_17		100
MX6Q_PAD_EIM_D17__ECSPI1_MISO			101
MX6Q_PAD_EIM_D17__IPU1_DI0_PIN6			102
MX6Q_PAD_EIM_D17__IPU2_CSI1_PIXCLK		103
MX6Q_PAD_EIM_D17__DCIC1_DCIC_OUT		104
MX6Q_PAD_EIM_D17__GPIO_3_17			105
MX6Q_PAD_EIM_D17__I2C3_SCL			106
MX6Q_PAD_EIM_D17__PL301_PER1_HBURST_1		107
MX6Q_PAD_EIM_D18__WEIM_WEIM_D_18		108
MX6Q_PAD_EIM_D18__ECSPI1_MOSI			109
MX6Q_PAD_EIM_D18__IPU1_DI0_PIN7			110
MX6Q_PAD_EIM_D18__IPU2_CSI1_D_17		111
MX6Q_PAD_EIM_D18__IPU1_DI1_D0_CS		112
MX6Q_PAD_EIM_D18__GPIO_3_18			113
MX6Q_PAD_EIM_D18__I2C3_SDA			114
MX6Q_PAD_EIM_D18__PL301_PER1_HBURST_2		115
MX6Q_PAD_EIM_D19__WEIM_WEIM_D_19		116
MX6Q_PAD_EIM_D19__ECSPI1_SS1			117
MX6Q_PAD_EIM_D19__IPU1_DI0_PIN8			118
MX6Q_PAD_EIM_D19__IPU2_CSI1_D_16		119
MX6Q_PAD_EIM_D19__UART1_CTS			120
MX6Q_PAD_EIM_D19__GPIO_3_19			121
MX6Q_PAD_EIM_D19__EPIT1_EPITO			122
MX6Q_PAD_EIM_D19__PL301_PER1_HRESP		123
MX6Q_PAD_EIM_D20__WEIM_WEIM_D_20		124
MX6Q_PAD_EIM_D20__ECSPI4_SS0			125
MX6Q_PAD_EIM_D20__IPU1_DI0_PIN16		126
MX6Q_PAD_EIM_D20__IPU2_CSI1_D_15		127
MX6Q_PAD_EIM_D20__UART1_RTS			128
MX6Q_PAD_EIM_D20__GPIO_3_20			129
MX6Q_PAD_EIM_D20__EPIT2_EPITO			130
MX6Q_PAD_EIM_D21__WEIM_WEIM_D_21		131
MX6Q_PAD_EIM_D21__ECSPI4_SCLK			132
MX6Q_PAD_EIM_D21__IPU1_DI0_PIN17		133
MX6Q_PAD_EIM_D21__IPU2_CSI1_D_11		134
MX6Q_PAD_EIM_D21__USBOH3_USBOTG_OC		135
MX6Q_PAD_EIM_D21__GPIO_3_21			136
MX6Q_PAD_EIM_D21__I2C1_SCL			137
MX6Q_PAD_EIM_D21__SPDIF_IN1			138
MX6Q_PAD_EIM_D22__WEIM_WEIM_D_22		139
MX6Q_PAD_EIM_D22__ECSPI4_MISO			140
MX6Q_PAD_EIM_D22__IPU1_DI0_PIN1			141
MX6Q_PAD_EIM_D22__IPU2_CSI1_D_10		142
MX6Q_PAD_EIM_D22__USBOH3_USBOTG_PWR		143
MX6Q_PAD_EIM_D22__GPIO_3_22			144
MX6Q_PAD_EIM_D22__SPDIF_OUT1			145
MX6Q_PAD_EIM_D22__PL301_PER1_HWRITE		146
MX6Q_PAD_EIM_D23__WEIM_WEIM_D_23		147
MX6Q_PAD_EIM_D23__IPU1_DI0_D0_CS		148
MX6Q_PAD_EIM_D23__UART3_CTS			149
MX6Q_PAD_EIM_D23__UART1_DCD			150
MX6Q_PAD_EIM_D23__IPU2_CSI1_DATA_EN		151
MX6Q_PAD_EIM_D23__GPIO_3_23			152
MX6Q_PAD_EIM_D23__IPU1_DI1_PIN2			153
MX6Q_PAD_EIM_D23__IPU1_DI1_PIN14		154
MX6Q_PAD_EIM_EB3__WEIM_WEIM_EB_3		155
MX6Q_PAD_EIM_EB3__ECSPI4_RDY			156
MX6Q_PAD_EIM_EB3__UART3_RTS			157
MX6Q_PAD_EIM_EB3__UART1_RI			158
MX6Q_PAD_EIM_EB3__IPU2_CSI1_HSYNC		159
MX6Q_PAD_EIM_EB3__GPIO_2_31			160
MX6Q_PAD_EIM_EB3__IPU1_DI1_PIN3			161
MX6Q_PAD_EIM_EB3__SRC_BT_CFG_31			162
MX6Q_PAD_EIM_D24__WEIM_WEIM_D_24		163
MX6Q_PAD_EIM_D24__ECSPI4_SS2			164
MX6Q_PAD_EIM_D24__UART3_TXD			165
MX6Q_PAD_EIM_D24__ECSPI1_SS2			166
MX6Q_PAD_EIM_D24__ECSPI2_SS2			167
MX6Q_PAD_EIM_D24__GPIO_3_24			168
MX6Q_PAD_EIM_D24__AUDMUX_AUD5_RXFS		169
MX6Q_PAD_EIM_D24__UART1_DTR			170
MX6Q_PAD_EIM_D25__WEIM_WEIM_D_25		171
MX6Q_PAD_EIM_D25__ECSPI4_SS3			172
MX6Q_PAD_EIM_D25__UART3_RXD			173
MX6Q_PAD_EIM_D25__ECSPI1_SS3			174
MX6Q_PAD_EIM_D25__ECSPI2_SS3			175
MX6Q_PAD_EIM_D25__GPIO_3_25			176
MX6Q_PAD_EIM_D25__AUDMUX_AUD5_RXC		177
MX6Q_PAD_EIM_D25__UART1_DSR			178
MX6Q_PAD_EIM_D26__WEIM_WEIM_D_26		179
MX6Q_PAD_EIM_D26__IPU1_DI1_PIN11		180
MX6Q_PAD_EIM_D26__IPU1_CSI0_D_1			181
MX6Q_PAD_EIM_D26__IPU2_CSI1_D_14		182
MX6Q_PAD_EIM_D26__UART2_TXD			183
MX6Q_PAD_EIM_D26__GPIO_3_26			184
MX6Q_PAD_EIM_D26__IPU1_SISG_2			185
MX6Q_PAD_EIM_D26__IPU1_DISP1_DAT_22		186
MX6Q_PAD_EIM_D27__WEIM_WEIM_D_27		187
MX6Q_PAD_EIM_D27__IPU1_DI1_PIN13		188
MX6Q_PAD_EIM_D27__IPU1_CSI0_D_0			189
MX6Q_PAD_EIM_D27__IPU2_CSI1_D_13		190
MX6Q_PAD_EIM_D27__UART2_RXD			191
MX6Q_PAD_EIM_D27__GPIO_3_27			192
MX6Q_PAD_EIM_D27__IPU1_SISG_3			193
MX6Q_PAD_EIM_D27__IPU1_DISP1_DAT_23		194
MX6Q_PAD_EIM_D28__WEIM_WEIM_D_28		195
MX6Q_PAD_EIM_D28__I2C1_SDA			196
MX6Q_PAD_EIM_D28__ECSPI4_MOSI			197
MX6Q_PAD_EIM_D28__IPU2_CSI1_D_12		198
MX6Q_PAD_EIM_D28__UART2_CTS			199
MX6Q_PAD_EIM_D28__GPIO_3_28			200
MX6Q_PAD_EIM_D28__IPU1_EXT_TRIG			201
MX6Q_PAD_EIM_D28__IPU1_DI0_PIN13		202
MX6Q_PAD_EIM_D29__WEIM_WEIM_D_29		203
MX6Q_PAD_EIM_D29__IPU1_DI1_PIN15		204
MX6Q_PAD_EIM_D29__ECSPI4_SS0			205
MX6Q_PAD_EIM_D29__UART2_RTS			206
MX6Q_PAD_EIM_D29__GPIO_3_29			207
MX6Q_PAD_EIM_D29__IPU2_CSI1_VSYNC		208
MX6Q_PAD_EIM_D29__IPU1_DI0_PIN14		209
MX6Q_PAD_EIM_D30__WEIM_WEIM_D_30		210
MX6Q_PAD_EIM_D30__IPU1_DISP1_DAT_21		211
MX6Q_PAD_EIM_D30__IPU1_DI0_PIN11		212
MX6Q_PAD_EIM_D30__IPU1_CSI0_D_3			213
MX6Q_PAD_EIM_D30__UART3_CTS			214
MX6Q_PAD_EIM_D30__GPIO_3_30			215
MX6Q_PAD_EIM_D30__USBOH3_USBH1_OC		216
MX6Q_PAD_EIM_D30__PL301_PER1_HPROT_0		217
MX6Q_PAD_EIM_D31__WEIM_WEIM_D_31		218
MX6Q_PAD_EIM_D31__IPU1_DISP1_DAT_20		219
MX6Q_PAD_EIM_D31__IPU1_DI0_PIN12		220
MX6Q_PAD_EIM_D31__IPU1_CSI0_D_2			221
MX6Q_PAD_EIM_D31__UART3_RTS			222
MX6Q_PAD_EIM_D31__GPIO_3_31			223
MX6Q_PAD_EIM_D31__USBOH3_USBH1_PWR		224
MX6Q_PAD_EIM_D31__PL301_PER1_HPROT_1		225
MX6Q_PAD_EIM_A24__WEIM_WEIM_A_24		226
MX6Q_PAD_EIM_A24__IPU1_DISP1_DAT_19		227
MX6Q_PAD_EIM_A24__IPU2_CSI1_D_19		228
MX6Q_PAD_EIM_A24__IPU2_SISG_2			229
MX6Q_PAD_EIM_A24__IPU1_SISG_2			230
MX6Q_PAD_EIM_A24__GPIO_5_4			231
MX6Q_PAD_EIM_A24__PL301_PER1_HPROT_2		232
MX6Q_PAD_EIM_A24__SRC_BT_CFG_24			233
MX6Q_PAD_EIM_A23__WEIM_WEIM_A_23		234
MX6Q_PAD_EIM_A23__IPU1_DISP1_DAT_18		235
MX6Q_PAD_EIM_A23__IPU2_CSI1_D_18		236
MX6Q_PAD_EIM_A23__IPU2_SISG_3			237
MX6Q_PAD_EIM_A23__IPU1_SISG_3			238
MX6Q_PAD_EIM_A23__GPIO_6_6			239
MX6Q_PAD_EIM_A23__PL301_PER1_HPROT_3		240
MX6Q_PAD_EIM_A23__SRC_BT_CFG_23			241
MX6Q_PAD_EIM_A22__WEIM_WEIM_A_22		242
MX6Q_PAD_EIM_A22__IPU1_DISP1_DAT_17		243
MX6Q_PAD_EIM_A22__IPU2_CSI1_D_17		244
MX6Q_PAD_EIM_A22__GPIO_2_16			245
MX6Q_PAD_EIM_A22__TPSMP_HDATA_0			246
MX6Q_PAD_EIM_A22__SRC_BT_CFG_22			247
MX6Q_PAD_EIM_A21__WEIM_WEIM_A_21		248
MX6Q_PAD_EIM_A21__IPU1_DISP1_DAT_16		249
MX6Q_PAD_EIM_A21__IPU2_CSI1_D_16		250
MX6Q_PAD_EIM_A21__RESERVED_RESERVED		251
MX6Q_PAD_EIM_A21__MIPI_CORE_DPHY_OUT_18		252
MX6Q_PAD_EIM_A21__GPIO_2_17			253
MX6Q_PAD_EIM_A21__TPSMP_HDATA_1			254
MX6Q_PAD_EIM_A21__SRC_BT_CFG_21			255
MX6Q_PAD_EIM_A20__WEIM_WEIM_A_20		256
MX6Q_PAD_EIM_A20__IPU1_DISP1_DAT_15		257
MX6Q_PAD_EIM_A20__IPU2_CSI1_D_15		258
MX6Q_PAD_EIM_A20__RESERVED_RESERVED		259
MX6Q_PAD_EIM_A20__MIPI_CORE_DPHY_OUT_19		260
MX6Q_PAD_EIM_A20__GPIO_2_18			261
MX6Q_PAD_EIM_A20__TPSMP_HDATA_2			262
MX6Q_PAD_EIM_A20__SRC_BT_CFG_20			263
MX6Q_PAD_EIM_A19__WEIM_WEIM_A_19		264
MX6Q_PAD_EIM_A19__IPU1_DISP1_DAT_14		265
MX6Q_PAD_EIM_A19__IPU2_CSI1_D_14		266
MX6Q_PAD_EIM_A19__RESERVED_RESERVED		267
MX6Q_PAD_EIM_A19__MIPI_CORE_DPHY_OUT_20		268
MX6Q_PAD_EIM_A19__GPIO_2_19			269
MX6Q_PAD_EIM_A19__TPSMP_HDATA_3			270
MX6Q_PAD_EIM_A19__SRC_BT_CFG_19			271
MX6Q_PAD_EIM_A18__WEIM_WEIM_A_18		272
MX6Q_PAD_EIM_A18__IPU1_DISP1_DAT_13		273
MX6Q_PAD_EIM_A18__IPU2_CSI1_D_13		274
MX6Q_PAD_EIM_A18__RESERVED_RESERVED		275
MX6Q_PAD_EIM_A18__MIPI_CORE_DPHY_OUT_21		276
MX6Q_PAD_EIM_A18__GPIO_2_20			277
MX6Q_PAD_EIM_A18__TPSMP_HDATA_4			278
MX6Q_PAD_EIM_A18__SRC_BT_CFG_18			279
MX6Q_PAD_EIM_A17__WEIM_WEIM_A_17		280
MX6Q_PAD_EIM_A17__IPU1_DISP1_DAT_12		281
MX6Q_PAD_EIM_A17__IPU2_CSI1_D_12		282
MX6Q_PAD_EIM_A17__RESERVED_RESERVED		283
MX6Q_PAD_EIM_A17__MIPI_CORE_DPHY_OUT_22		284
MX6Q_PAD_EIM_A17__GPIO_2_21			285
MX6Q_PAD_EIM_A17__TPSMP_HDATA_5			286
MX6Q_PAD_EIM_A17__SRC_BT_CFG_17			287
MX6Q_PAD_EIM_A16__WEIM_WEIM_A_16		288
MX6Q_PAD_EIM_A16__IPU1_DI1_DISP_CLK		289
MX6Q_PAD_EIM_A16__IPU2_CSI1_PIXCLK		290
MX6Q_PAD_EIM_A16__MIPI_CORE_DPHY_OUT_23		291
MX6Q_PAD_EIM_A16__GPIO_2_22			292
MX6Q_PAD_EIM_A16__TPSMP_HDATA_6			293
MX6Q_PAD_EIM_A16__SRC_BT_CFG_16			294
MX6Q_PAD_EIM_CS0__WEIM_WEIM_CS_0		295
MX6Q_PAD_EIM_CS0__IPU1_DI1_PIN5			296
MX6Q_PAD_EIM_CS0__ECSPI2_SCLK			297
MX6Q_PAD_EIM_CS0__MIPI_CORE_DPHY_OUT_24		298
MX6Q_PAD_EIM_CS0__GPIO_2_23			299
MX6Q_PAD_EIM_CS0__TPSMP_HDATA_7			300
MX6Q_PAD_EIM_CS1__WEIM_WEIM_CS_1		301
MX6Q_PAD_EIM_CS1__IPU1_DI1_PIN6			302
MX6Q_PAD_EIM_CS1__ECSPI2_MOSI			303
MX6Q_PAD_EIM_CS1__MIPI_CORE_DPHY_OUT_25		304
MX6Q_PAD_EIM_CS1__GPIO_2_24			305
MX6Q_PAD_EIM_CS1__TPSMP_HDATA_8			306
MX6Q_PAD_EIM_OE__WEIM_WEIM_OE			307
MX6Q_PAD_EIM_OE__IPU1_DI1_PIN7			308
MX6Q_PAD_EIM_OE__ECSPI2_MISO			309
MX6Q_PAD_EIM_OE__MIPI_CORE_DPHY_OUT_26		310
MX6Q_PAD_EIM_OE__GPIO_2_25			311
MX6Q_PAD_EIM_OE__TPSMP_HDATA_9			312
MX6Q_PAD_EIM_RW__WEIM_WEIM_RW			313
MX6Q_PAD_EIM_RW__IPU1_DI1_PIN8			314
MX6Q_PAD_EIM_RW__ECSPI2_SS0			315
MX6Q_PAD_EIM_RW__MIPI_CORE_DPHY_OUT_27		316
MX6Q_PAD_EIM_RW__GPIO_2_26			317
MX6Q_PAD_EIM_RW__TPSMP_HDATA_10			318
MX6Q_PAD_EIM_RW__SRC_BT_CFG_29			319
MX6Q_PAD_EIM_LBA__WEIM_WEIM_LBA			320
MX6Q_PAD_EIM_LBA__IPU1_DI1_PIN17		321
MX6Q_PAD_EIM_LBA__ECSPI2_SS1			322
MX6Q_PAD_EIM_LBA__GPIO_2_27			323
MX6Q_PAD_EIM_LBA__TPSMP_HDATA_11		324
MX6Q_PAD_EIM_LBA__SRC_BT_CFG_26			325
MX6Q_PAD_EIM_EB0__WEIM_WEIM_EB_0		326
MX6Q_PAD_EIM_EB0__IPU1_DISP1_DAT_11		327
MX6Q_PAD_EIM_EB0__IPU2_CSI1_D_11		328
MX6Q_PAD_EIM_EB0__MIPI_CORE_DPHY_OUT_0		329
MX6Q_PAD_EIM_EB0__CCM_PMIC_RDY			330
MX6Q_PAD_EIM_EB0__GPIO_2_28			331
MX6Q_PAD_EIM_EB0__TPSMP_HDATA_12		332
MX6Q_PAD_EIM_EB0__SRC_BT_CFG_27			333
MX6Q_PAD_EIM_EB1__WEIM_WEIM_EB_1		334
MX6Q_PAD_EIM_EB1__IPU1_DISP1_DAT_10		335
MX6Q_PAD_EIM_EB1__IPU2_CSI1_D_10		336
MX6Q_PAD_EIM_EB1__MIPI_CORE_DPHY__OUT_1		337
MX6Q_PAD_EIM_EB1__GPIO_2_29			338
MX6Q_PAD_EIM_EB1__TPSMP_HDATA_13		339
MX6Q_PAD_EIM_EB1__SRC_BT_CFG_28			340
MX6Q_PAD_EIM_DA0__WEIM_WEIM_DA_A_0		341
MX6Q_PAD_EIM_DA0__IPU1_DISP1_DAT_9		342
MX6Q_PAD_EIM_DA0__IPU2_CSI1_D_9			343
MX6Q_PAD_EIM_DA0__MIPI_CORE_DPHY__OUT_2		344
MX6Q_PAD_EIM_DA0__GPIO_3_0			345
MX6Q_PAD_EIM_DA0__TPSMP_HDATA_14		346
MX6Q_PAD_EIM_DA0__SRC_BT_CFG_0			347
MX6Q_PAD_EIM_DA1__WEIM_WEIM_DA_A_1		348
MX6Q_PAD_EIM_DA1__IPU1_DISP1_DAT_8		349
MX6Q_PAD_EIM_DA1__IPU2_CSI1_D_8			350
MX6Q_PAD_EIM_DA1__MIPI_CORE_DPHY_OUT_3		351
MX6Q_PAD_EIM_DA1__USBPHY1_TX_LS_MODE		352
MX6Q_PAD_EIM_DA1__GPIO_3_1			353
MX6Q_PAD_EIM_DA1__TPSMP_HDATA_15		354
MX6Q_PAD_EIM_DA1__SRC_BT_CFG_1			355
MX6Q_PAD_EIM_DA2__WEIM_WEIM_DA_A_2		356
MX6Q_PAD_EIM_DA2__IPU1_DISP1_DAT_7		357
MX6Q_PAD_EIM_DA2__IPU2_CSI1_D_7			358
MX6Q_PAD_EIM_DA2__MIPI_CORE_DPHY_OUT_4		359
MX6Q_PAD_EIM_DA2__USBPHY1_TX_HS_MODE		360
MX6Q_PAD_EIM_DA2__GPIO_3_2			361
MX6Q_PAD_EIM_DA2__TPSMP_HDATA_16		362
MX6Q_PAD_EIM_DA2__SRC_BT_CFG_2			363
MX6Q_PAD_EIM_DA3__WEIM_WEIM_DA_A_3		364
MX6Q_PAD_EIM_DA3__IPU1_DISP1_DAT_6		365
MX6Q_PAD_EIM_DA3__IPU2_CSI1_D_6			366
MX6Q_PAD_EIM_DA3__MIPI_CORE_DPHY_OUT_5		367
MX6Q_PAD_EIM_DA3__USBPHY1_TX_HIZ		368
MX6Q_PAD_EIM_DA3__GPIO_3_3			369
MX6Q_PAD_EIM_DA3__TPSMP_HDATA_17		370
MX6Q_PAD_EIM_DA3__SRC_BT_CFG_3			371
MX6Q_PAD_EIM_DA4__WEIM_WEIM_DA_A_4		372
MX6Q_PAD_EIM_DA4__IPU1_DISP1_DAT_5		373
MX6Q_PAD_EIM_DA4__IPU2_CSI1_D_5			374
MX6Q_PAD_EIM_DA4__MIPI_CORE_DPHY_OUT_6		375
MX6Q_PAD_EIM_DA4__ANATOP_USBPHY1_TX_EN		376
MX6Q_PAD_EIM_DA4__GPIO_3_4			377
MX6Q_PAD_EIM_DA4__TPSMP_HDATA_18		378
MX6Q_PAD_EIM_DA4__SRC_BT_CFG_4			379
MX6Q_PAD_EIM_DA5__WEIM_WEIM_DA_A_5		380
MX6Q_PAD_EIM_DA5__IPU1_DISP1_DAT_4		381
MX6Q_PAD_EIM_DA5__IPU2_CSI1_D_4			382
MX6Q_PAD_EIM_DA5__MIPI_CORE_DPHY_OUT_7		383
MX6Q_PAD_EIM_DA5__ANATOP_USBPHY1_TX_DP		384
MX6Q_PAD_EIM_DA5__GPIO_3_5			385
MX6Q_PAD_EIM_DA5__TPSMP_HDATA_19		386
MX6Q_PAD_EIM_DA5__SRC_BT_CFG_5			387
MX6Q_PAD_EIM_DA6__WEIM_WEIM_DA_A_6		388
MX6Q_PAD_EIM_DA6__IPU1_DISP1_DAT_3		389
MX6Q_PAD_EIM_DA6__IPU2_CSI1_D_3			390
MX6Q_PAD_EIM_DA6__MIPI_CORE_DPHY_OUT_8		391
MX6Q_PAD_EIM_DA6__ANATOP_USBPHY1_TX_DN		392
MX6Q_PAD_EIM_DA6__GPIO_3_6			393
MX6Q_PAD_EIM_DA6__TPSMP_HDATA_20		394
MX6Q_PAD_EIM_DA6__SRC_BT_CFG_6			395
MX6Q_PAD_EIM_DA7__WEIM_WEIM_DA_A_7		396
MX6Q_PAD_EIM_DA7__IPU1_DISP1_DAT_2		397
MX6Q_PAD_EIM_DA7__IPU2_CSI1_D_2			398
MX6Q_PAD_EIM_DA7__MIPI_CORE_DPHY_OUT_9		399
MX6Q_PAD_EIM_DA7__GPIO_3_7			400
MX6Q_PAD_EIM_DA7__TPSMP_HDATA_21		401
MX6Q_PAD_EIM_DA7__SRC_BT_CFG_7			402
MX6Q_PAD_EIM_DA8__WEIM_WEIM_DA_A_8		403
MX6Q_PAD_EIM_DA8__IPU1_DISP1_DAT_1		404
MX6Q_PAD_EIM_DA8__IPU2_CSI1_D_1			405
MX6Q_PAD_EIM_DA8__MIPI_CORE_DPHY_OUT_10		406
MX6Q_PAD_EIM_DA8__GPIO_3_8			407
MX6Q_PAD_EIM_DA8__TPSMP_HDATA_22		408
MX6Q_PAD_EIM_DA8__SRC_BT_CFG_8			409
MX6Q_PAD_EIM_DA9__WEIM_WEIM_DA_A_9		410
MX6Q_PAD_EIM_DA9__IPU1_DISP1_DAT_0		411
MX6Q_PAD_EIM_DA9__IPU2_CSI1_D_0			412
MX6Q_PAD_EIM_DA9__MIPI_CORE_DPHY_OUT_11		413
MX6Q_PAD_EIM_DA9__GPIO_3_9			414
MX6Q_PAD_EIM_DA9__TPSMP_HDATA_23		415
MX6Q_PAD_EIM_DA9__SRC_BT_CFG_9			416
MX6Q_PAD_EIM_DA10__WEIM_WEIM_DA_A_10		417
MX6Q_PAD_EIM_DA10__IPU1_DI1_PIN15		418
MX6Q_PAD_EIM_DA10__IPU2_CSI1_DATA_EN		419
MX6Q_PAD_EIM_DA10__MIPI_CORE_DPHY_OUT12		420
MX6Q_PAD_EIM_DA10__GPIO_3_10			421
MX6Q_PAD_EIM_DA10__TPSMP_HDATA_24		422
MX6Q_PAD_EIM_DA10__SRC_BT_CFG_10		423
MX6Q_PAD_EIM_DA11__WEIM_WEIM_DA_A_11		424
MX6Q_PAD_EIM_DA11__IPU1_DI1_PIN2		425
MX6Q_PAD_EIM_DA11__IPU2_CSI1_HSYNC		426
MX6Q_PAD_EIM_DA11__MIPI_CORE_DPHY_OUT13		427
MX6Q_PAD_EIM_DA11__SDMA_DBG_EVT_CHN_6		428
MX6Q_PAD_EIM_DA11__GPIO_3_11			429
MX6Q_PAD_EIM_DA11__TPSMP_HDATA_25		430
MX6Q_PAD_EIM_DA11__SRC_BT_CFG_11		431
MX6Q_PAD_EIM_DA12__WEIM_WEIM_DA_A_12		432
MX6Q_PAD_EIM_DA12__IPU1_DI1_PIN3		433
MX6Q_PAD_EIM_DA12__IPU2_CSI1_VSYNC		434
MX6Q_PAD_EIM_DA12__MIPI_CORE_DPHY_OUT14		435
MX6Q_PAD_EIM_DA12__SDMA_DEBUG_EVT_CHN_3		436
MX6Q_PAD_EIM_DA12__GPIO_3_12			437
MX6Q_PAD_EIM_DA12__TPSMP_HDATA_26		438
MX6Q_PAD_EIM_DA12__SRC_BT_CFG_12		439
MX6Q_PAD_EIM_DA13__WEIM_WEIM_DA_A_13		440
MX6Q_PAD_EIM_DA13__IPU1_DI1_D0_CS		441
MX6Q_PAD_EIM_DA13__CCM_DI1_EXT_CLK		442
MX6Q_PAD_EIM_DA13__MIPI_CORE_DPHY_OUT15		443
MX6Q_PAD_EIM_DA13__SDMA_DEBUG_EVT_CHN_4		444
MX6Q_PAD_EIM_DA13__GPIO_3_13			445
MX6Q_PAD_EIM_DA13__TPSMP_HDATA_27		446
MX6Q_PAD_EIM_DA13__SRC_BT_CFG_13		447
MX6Q_PAD_EIM_DA14__WEIM_WEIM_DA_A_14		448
MX6Q_PAD_EIM_DA14__IPU1_DI1_D1_CS		449
MX6Q_PAD_EIM_DA14__CCM_DI0_EXT_CLK		450
MX6Q_PAD_EIM_DA14__MIPI_CORE_DPHY_OUT16		451
MX6Q_PAD_EIM_DA14__SDMA_DEBUG_EVT_CHN_5		452
MX6Q_PAD_EIM_DA14__GPIO_3_14			453
MX6Q_PAD_EIM_DA14__TPSMP_HDATA_28		454
MX6Q_PAD_EIM_DA14__SRC_BT_CFG_14		455
MX6Q_PAD_EIM_DA15__WEIM_WEIM_DA_A_15		456
MX6Q_PAD_EIM_DA15__IPU1_DI1_PIN1		457
MX6Q_PAD_EIM_DA15__IPU1_DI1_PIN4		458
MX6Q_PAD_EIM_DA15__MIPI_CORE_DPHY_OUT17		459
MX6Q_PAD_EIM_DA15__GPIO_3_15			460
MX6Q_PAD_EIM_DA15__TPSMP_HDATA_29		461
MX6Q_PAD_EIM_DA15__SRC_BT_CFG_15		462
MX6Q_PAD_EIM_WAIT__WEIM_WEIM_WAIT		463
MX6Q_PAD_EIM_WAIT__WEIM_WEIM_DTACK_B		464
MX6Q_PAD_EIM_WAIT__GPIO_5_0			465
MX6Q_PAD_EIM_WAIT__TPSMP_HDATA_30		466
MX6Q_PAD_EIM_WAIT__SRC_BT_CFG_25		467
MX6Q_PAD_EIM_BCLK__WEIM_WEIM_BCLK		468
MX6Q_PAD_EIM_BCLK__IPU1_DI1_PIN16		469
MX6Q_PAD_EIM_BCLK__GPIO_6_31			470
MX6Q_PAD_EIM_BCLK__TPSMP_HDATA_31		471
MX6Q_PAD_DI0_DISP_CLK__IPU1_DI0_DSP_CLK		472
MX6Q_PAD_DI0_DISP_CLK__IPU2_DI0_DSP_CLK		473
MX6Q_PAD_DI0_DISP_CLK__MIPI_CR_DPY_OT28		474
MX6Q_PAD_DI0_DISP_CLK__SDMA_DBG_CR_STA0		475
MX6Q_PAD_DI0_DISP_CLK__GPIO_4_16		476
MX6Q_PAD_DI0_DISP_CLK__MMDC_DEBUG_0		477
MX6Q_PAD_DI0_PIN15__IPU1_DI0_PIN15		478
MX6Q_PAD_DI0_PIN15__IPU2_DI0_PIN15		479
MX6Q_PAD_DI0_PIN15__AUDMUX_AUD6_TXC		480
MX6Q_PAD_DI0_PIN15__MIPI_CR_DPHY_OUT_29		481
MX6Q_PAD_DI0_PIN15__SDMA_DBG_CORE_STA_1		482
MX6Q_PAD_DI0_PIN15__GPIO_4_17			483
MX6Q_PAD_DI0_PIN15__MMDC_MMDC_DEBUG_1		484
MX6Q_PAD_DI0_PIN2__IPU1_DI0_PIN2		485
MX6Q_PAD_DI0_PIN2__IPU2_DI0_PIN2		486
MX6Q_PAD_DI0_PIN2__AUDMUX_AUD6_TXD		487
MX6Q_PAD_DI0_PIN2__MIPI_CR_DPHY_OUT_30		488
MX6Q_PAD_DI0_PIN2__SDMA_DBG_CORE_STA_2		489
MX6Q_PAD_DI0_PIN2__GPIO_4_18			490
MX6Q_PAD_DI0_PIN2__MMDC_DEBUG_2			491
MX6Q_PAD_DI0_PIN2__PL301_PER1_HADDR_9		492
MX6Q_PAD_DI0_PIN3__IPU1_DI0_PIN3		493
MX6Q_PAD_DI0_PIN3__IPU2_DI0_PIN3		494
MX6Q_PAD_DI0_PIN3__AUDMUX_AUD6_TXFS		495
MX6Q_PAD_DI0_PIN3__MIPI_CORE_DPHY_OUT31		496
MX6Q_PAD_DI0_PIN3__SDMA_DBG_CORE_STA_3		497
MX6Q_PAD_DI0_PIN3__GPIO_4_19			498
MX6Q_PAD_DI0_PIN3__MMDC_MMDC_DEBUG_3		499
MX6Q_PAD_DI0_PIN3__PL301_PER1_HADDR_10		500
MX6Q_PAD_DI0_PIN4__IPU1_DI0_PIN4		501
MX6Q_PAD_DI0_PIN4__IPU2_DI0_PIN4		502
MX6Q_PAD_DI0_PIN4__AUDMUX_AUD6_RXD		503
MX6Q_PAD_DI0_PIN4__USDHC1_WP			504
MX6Q_PAD_DI0_PIN4__SDMA_DEBUG_YIELD		505
MX6Q_PAD_DI0_PIN4__GPIO_4_20			506
MX6Q_PAD_DI0_PIN4__MMDC_MMDC_DEBUG_4		507
MX6Q_PAD_DI0_PIN4__PL301_PER1_HADDR_11		508
MX6Q_PAD_DISP0_DAT0__IPU1_DISP0_DAT_0		509
MX6Q_PAD_DISP0_DAT0__IPU2_DISP0_DAT_0		510
MX6Q_PAD_DISP0_DAT0__ECSPI3_SCLK		511
MX6Q_PAD_DISP0_DAT0__USDHC1_USDHC_DBG_0		512
MX6Q_PAD_DISP0_DAT0__SDMA_DBG_CORE_RUN		513
MX6Q_PAD_DISP0_DAT0__GPIO_4_21			514
MX6Q_PAD_DISP0_DAT0__MMDC_MMDC_DEBUG_5		515
MX6Q_PAD_DISP0_DAT1__IPU1_DISP0_DAT_1		516
MX6Q_PAD_DISP0_DAT1__IPU2_DISP0_DAT_1		517
MX6Q_PAD_DISP0_DAT1__ECSPI3_MOSI		518
MX6Q_PAD_DISP0_DAT1__USDHC1_USDHC_DBG_1		519
MX6Q_PAD_DISP0_DAT1__SDMA_DBG_EVT_CHNSL		520
MX6Q_PAD_DISP0_DAT1__GPIO_4_22			521
MX6Q_PAD_DISP0_DAT1__MMDC_DEBUG_6		522
MX6Q_PAD_DISP0_DAT1__PL301_PER1_HADR_12		523
MX6Q_PAD_DISP0_DAT2__IPU1_DISP0_DAT_2		524
MX6Q_PAD_DISP0_DAT2__IPU2_DISP0_DAT_2		525
MX6Q_PAD_DISP0_DAT2__ECSPI3_MISO		526
MX6Q_PAD_DISP0_DAT2__USDHC1_USDHC_DBG_2		527
MX6Q_PAD_DISP0_DAT2__SDMA_DEBUG_MODE		528
MX6Q_PAD_DISP0_DAT2__GPIO_4_23			529
MX6Q_PAD_DISP0_DAT2__MMDC_DEBUG_7		530
MX6Q_PAD_DISP0_DAT2__PL301_PER1_HADR_13		531
MX6Q_PAD_DISP0_DAT3__IPU1_DISP0_DAT_3		532
MX6Q_PAD_DISP0_DAT3__IPU2_DISP0_DAT_3		533
MX6Q_PAD_DISP0_DAT3__ECSPI3_SS0			534
MX6Q_PAD_DISP0_DAT3__USDHC1_USDHC_DBG_3		535
MX6Q_PAD_DISP0_DAT3__SDMA_DBG_BUS_ERROR		536
MX6Q_PAD_DISP0_DAT3__GPIO_4_24			537
MX6Q_PAD_DISP0_DAT3__MMDC_MMDC_DBG_8		538
MX6Q_PAD_DISP0_DAT3__PL301_PER1_HADR_14		539
MX6Q_PAD_DISP0_DAT4__IPU1_DISP0_DAT_4		540
MX6Q_PAD_DISP0_DAT4__IPU2_DISP0_DAT_4		541
MX6Q_PAD_DISP0_DAT4__ECSPI3_SS1			542
MX6Q_PAD_DISP0_DAT4__USDHC1_USDHC_DBG_4		543
MX6Q_PAD_DISP0_DAT4__SDMA_DEBUG_BUS_RWB		544
MX6Q_PAD_DISP0_DAT4__GPIO_4_25			545
MX6Q_PAD_DISP0_DAT4__MMDC_MMDC_DEBUG_9		546
MX6Q_PAD_DISP0_DAT4__PL301_PER1_HADR_15		547
MX6Q_PAD_DISP0_DAT5__IPU1_DISP0_DAT_5		548
MX6Q_PAD_DISP0_DAT5__IPU2_DISP0_DAT_5		549
MX6Q_PAD_DISP0_DAT5__ECSPI3_SS2			550
MX6Q_PAD_DISP0_DAT5__AUDMUX_AUD6_RXFS		551
MX6Q_PAD_DISP0_DAT5__SDMA_DBG_MCH_DMBUS		552
MX6Q_PAD_DISP0_DAT5__GPIO_4_26			553
MX6Q_PAD_DISP0_DAT5__MMDC_DEBUG_10		554
MX6Q_PAD_DISP0_DAT5__PL301_PER1_HADR_16		555
MX6Q_PAD_DISP0_DAT6__IPU1_DISP0_DAT_6		556
MX6Q_PAD_DISP0_DAT6__IPU2_DISP0_DAT_6		557
MX6Q_PAD_DISP0_DAT6__ECSPI3_SS3			558
MX6Q_PAD_DISP0_DAT6__AUDMUX_AUD6_RXC		559
MX6Q_PAD_DISP0_DAT6__SDMA_DBG_RTBUF_WRT		560
MX6Q_PAD_DISP0_DAT6__GPIO_4_27			561
MX6Q_PAD_DISP0_DAT6__MMDC_DEBUG_11		562
MX6Q_PAD_DISP0_DAT6__PL301_PER1_HADR_17		563
MX6Q_PAD_DISP0_DAT7__IPU1_DISP0_DAT_7		564
MX6Q_PAD_DISP0_DAT7__IPU2_DISP0_DAT_7		565
MX6Q_PAD_DISP0_DAT7__ECSPI3_RDY			566
MX6Q_PAD_DISP0_DAT7__USDHC1_USDHC_DBG_5		567
MX6Q_PAD_DISP0_DAT7__SDMA_DBG_EVT_CHN_0		568
MX6Q_PAD_DISP0_DAT7__GPIO_4_28			569
MX6Q_PAD_DISP0_DAT7__MMDC_DEBUG_12		570
MX6Q_PAD_DISP0_DAT7__PL301_PER1_HADR_18		571
MX6Q_PAD_DISP0_DAT8__IPU1_DISP0_DAT_8		572
MX6Q_PAD_DISP0_DAT8__IPU2_DISP0_DAT_8		573
MX6Q_PAD_DISP0_DAT8__PWM1_PWMO			574
MX6Q_PAD_DISP0_DAT8__WDOG1_WDOG_B		575
MX6Q_PAD_DISP0_DAT8__SDMA_DBG_EVT_CHN_1		576
MX6Q_PAD_DISP0_DAT8__GPIO_4_29			577
MX6Q_PAD_DISP0_DAT8__MMDC_DEBUG_13		578
MX6Q_PAD_DISP0_DAT8__PL301_PER1_HADR_19		579
MX6Q_PAD_DISP0_DAT9__IPU1_DISP0_DAT_9		580
MX6Q_PAD_DISP0_DAT9__IPU2_DISP0_DAT_9		581
MX6Q_PAD_DISP0_DAT9__PWM2_PWMO			582
MX6Q_PAD_DISP0_DAT9__WDOG2_WDOG_B		583
MX6Q_PAD_DISP0_DAT9__SDMA_DBG_EVT_CHN_2		584
MX6Q_PAD_DISP0_DAT9__GPIO_4_30			585
MX6Q_PAD_DISP0_DAT9__MMDC_DEBUG_14		586
MX6Q_PAD_DISP0_DAT9__PL301_PER1_HADR_20		587
MX6Q_PAD_DISP0_DAT10__IPU1_DISP0_DAT_10		588
MX6Q_PAD_DISP0_DAT10__IPU2_DISP0_DAT_10		589
MX6Q_PAD_DISP0_DAT10__USDHC1_DBG_6		590
MX6Q_PAD_DISP0_DAT10__SDMA_DBG_EVT_CHN3		591
MX6Q_PAD_DISP0_DAT10__GPIO_4_31			592
MX6Q_PAD_DISP0_DAT10__MMDC_DEBUG_15		593
MX6Q_PAD_DISP0_DAT10__PL301_PER1_HADR21		594
MX6Q_PAD_DISP0_DAT11__IPU1_DISP0_DAT_11		595
MX6Q_PAD_DISP0_DAT11__IPU2_DISP0_DAT_11		596
MX6Q_PAD_DISP0_DAT11__USDHC1_USDHC_DBG7		597
MX6Q_PAD_DISP0_DAT11__SDMA_DBG_EVT_CHN4		598
MX6Q_PAD_DISP0_DAT11__GPIO_5_5			599
MX6Q_PAD_DISP0_DAT11__MMDC_DEBUG_16		600
MX6Q_PAD_DISP0_DAT11__PL301_PER1_HADR22		601
MX6Q_PAD_DISP0_DAT12__IPU1_DISP0_DAT_12		602
MX6Q_PAD_DISP0_DAT12__IPU2_DISP0_DAT_12		603
MX6Q_PAD_DISP0_DAT12__RESERVED_RESERVED		604
MX6Q_PAD_DISP0_DAT12__SDMA_DBG_EVT_CHN5		605
MX6Q_PAD_DISP0_DAT12__GPIO_5_6			606
MX6Q_PAD_DISP0_DAT12__MMDC_DEBUG_17		607
MX6Q_PAD_DISP0_DAT12__PL301_PER1_HADR23		608
MX6Q_PAD_DISP0_DAT13__IPU1_DISP0_DAT_13		609
MX6Q_PAD_DISP0_DAT13__IPU2_DISP0_DAT_13		610
MX6Q_PAD_DISP0_DAT13__AUDMUX_AUD5_RXFS		611
MX6Q_PAD_DISP0_DAT13__SDMA_DBG_EVT_CHN0		612
MX6Q_PAD_DISP0_DAT13__GPIO_5_7			613
MX6Q_PAD_DISP0_DAT13__MMDC_DEBUG_18		614
MX6Q_PAD_DISP0_DAT13__PL301_PER1_HADR24		615
MX6Q_PAD_DISP0_DAT14__IPU1_DISP0_DAT_14		616
MX6Q_PAD_DISP0_DAT14__IPU2_DISP0_DAT_14		617
MX6Q_PAD_DISP0_DAT14__AUDMUX_AUD5_RXC		618
MX6Q_PAD_DISP0_DAT14__SDMA_DBG_EVT_CHN1		619
MX6Q_PAD_DISP0_DAT14__GPIO_5_8			620
MX6Q_PAD_DISP0_DAT14__MMDC_DEBUG_19		621
MX6Q_PAD_DISP0_DAT15__IPU1_DISP0_DAT_15		622
MX6Q_PAD_DISP0_DAT15__IPU2_DISP0_DAT_15		623
MX6Q_PAD_DISP0_DAT15__ECSPI1_SS1		624
MX6Q_PAD_DISP0_DAT15__ECSPI2_SS1		625
MX6Q_PAD_DISP0_DAT15__SDMA_DBG_EVT_CHN2		626
MX6Q_PAD_DISP0_DAT15__GPIO_5_9			627
MX6Q_PAD_DISP0_DAT15__MMDC_DEBUG_20		628
MX6Q_PAD_DISP0_DAT15__PL301_PER1_HADR25		629
MX6Q_PAD_DISP0_DAT16__IPU1_DISP0_DAT_16		630
MX6Q_PAD_DISP0_DAT16__IPU2_DISP0_DAT_16		631
MX6Q_PAD_DISP0_DAT16__ECSPI2_MOSI		632
MX6Q_PAD_DISP0_DAT16__AUDMUX_AUD5_TXC		633
MX6Q_PAD_DISP0_DAT16__SDMA_EXT_EVENT_0		634
MX6Q_PAD_DISP0_DAT16__GPIO_5_10			635
MX6Q_PAD_DISP0_DAT16__MMDC_DEBUG_21		636
MX6Q_PAD_DISP0_DAT16__PL301_PER1_HADR26		637
MX6Q_PAD_DISP0_DAT17__IPU1_DISP0_DAT_17		638
MX6Q_PAD_DISP0_DAT17__IPU2_DISP0_DAT_17		639
MX6Q_PAD_DISP0_DAT17__ECSPI2_MISO		640
MX6Q_PAD_DISP0_DAT17__AUDMUX_AUD5_TXD		641
MX6Q_PAD_DISP0_DAT17__SDMA_EXT_EVENT_1		642
MX6Q_PAD_DISP0_DAT17__GPIO_5_11			643
MX6Q_PAD_DISP0_DAT17__MMDC_DEBUG_22		644
MX6Q_PAD_DISP0_DAT17__PL301_PER1_HADR27		645
MX6Q_PAD_DISP0_DAT18__IPU1_DISP0_DAT_18		646
MX6Q_PAD_DISP0_DAT18__IPU2_DISP0_DAT_18		647
MX6Q_PAD_DISP0_DAT18__ECSPI2_SS0		648
MX6Q_PAD_DISP0_DAT18__AUDMUX_AUD5_TXFS		649
MX6Q_PAD_DISP0_DAT18__AUDMUX_AUD4_RXFS		650
MX6Q_PAD_DISP0_DAT18__GPIO_5_12			651
MX6Q_PAD_DISP0_DAT18__MMDC_DEBUG_23		652
MX6Q_PAD_DISP0_DAT18__WEIM_WEIM_CS_2		653
MX6Q_PAD_DISP0_DAT19__IPU1_DISP0_DAT_19		654
MX6Q_PAD_DISP0_DAT19__IPU2_DISP0_DAT_19		655
MX6Q_PAD_DISP0_DAT19__ECSPI2_SCLK		656
MX6Q_PAD_DISP0_DAT19__AUDMUX_AUD5_RXD		657
MX6Q_PAD_DISP0_DAT19__AUDMUX_AUD4_RXC		658
MX6Q_PAD_DISP0_DAT19__GPIO_5_13			659
MX6Q_PAD_DISP0_DAT19__MMDC_DEBUG_24		660
MX6Q_PAD_DISP0_DAT19__WEIM_WEIM_CS_3		661
MX6Q_PAD_DISP0_DAT20__IPU1_DISP0_DAT_20		662
MX6Q_PAD_DISP0_DAT20__IPU2_DISP0_DAT_20		663
MX6Q_PAD_DISP0_DAT20__ECSPI1_SCLK		664
MX6Q_PAD_DISP0_DAT20__AUDMUX_AUD4_TXC		665
MX6Q_PAD_DISP0_DAT20__SDMA_DBG_EVT_CHN7		666
MX6Q_PAD_DISP0_DAT20__GPIO_5_14			667
MX6Q_PAD_DISP0_DAT20__MMDC_DEBUG_25		668
MX6Q_PAD_DISP0_DAT20__PL301_PER1_HADR28		669
MX6Q_PAD_DISP0_DAT21__IPU1_DISP0_DAT_21		670
MX6Q_PAD_DISP0_DAT21__IPU2_DISP0_DAT_21		671
MX6Q_PAD_DISP0_DAT21__ECSPI1_MOSI		672
MX6Q_PAD_DISP0_DAT21__AUDMUX_AUD4_TXD		673
MX6Q_PAD_DISP0_DAT21__SDMA_DBG_BUS_DEV0		674
MX6Q_PAD_DISP0_DAT21__GPIO_5_15			675
MX6Q_PAD_DISP0_DAT21__MMDC_DEBUG_26		676
MX6Q_PAD_DISP0_DAT21__PL301_PER1_HADR29		677
MX6Q_PAD_DISP0_DAT22__IPU1_DISP0_DAT_22		678
MX6Q_PAD_DISP0_DAT22__IPU2_DISP0_DAT_22		679
MX6Q_PAD_DISP0_DAT22__ECSPI1_MISO		680
MX6Q_PAD_DISP0_DAT22__AUDMUX_AUD4_TXFS		681
MX6Q_PAD_DISP0_DAT22__SDMA_DBG_BUS_DEV1		682
MX6Q_PAD_DISP0_DAT22__GPIO_5_16			683
MX6Q_PAD_DISP0_DAT22__MMDC_DEBUG_27		684
MX6Q_PAD_DISP0_DAT22__PL301_PER1_HADR30		685
MX6Q_PAD_DISP0_DAT23__IPU1_DISP0_DAT_23		686
MX6Q_PAD_DISP0_DAT23__IPU2_DISP0_DAT_23		687
MX6Q_PAD_DISP0_DAT23__ECSPI1_SS0		688
MX6Q_PAD_DISP0_DAT23__AUDMUX_AUD4_RXD		689
MX6Q_PAD_DISP0_DAT23__SDMA_DBG_BUS_DEV2		690
MX6Q_PAD_DISP0_DAT23__GPIO_5_17			691
MX6Q_PAD_DISP0_DAT23__MMDC_DEBUG_28		692
MX6Q_PAD_DISP0_DAT23__PL301_PER1_HADR31		693
MX6Q_PAD_ENET_MDIO__RESERVED_RESERVED		694
MX6Q_PAD_ENET_MDIO__ENET_MDIO			695
MX6Q_PAD_ENET_MDIO__ESAI1_SCKR			696
MX6Q_PAD_ENET_MDIO__SDMA_DEBUG_BUS_DEV3		697
MX6Q_PAD_ENET_MDIO__ENET_1588_EVT1_OUT		698
MX6Q_PAD_ENET_MDIO__GPIO_1_22			699
MX6Q_PAD_ENET_MDIO__SPDIF_PLOCK			700
MX6Q_PAD_ENET_REF_CLK__RESERVED_RSRVED		701
MX6Q_PAD_ENET_REF_CLK__ENET_TX_CLK		702
MX6Q_PAD_ENET_REF_CLK__ESAI1_FSR		703
MX6Q_PAD_ENET_REF_CLK__SDMA_DBGBUS_DEV4		704
MX6Q_PAD_ENET_REF_CLK__GPIO_1_23		705
MX6Q_PAD_ENET_REF_CLK__SPDIF_SRCLK		706
MX6Q_PAD_ENET_REF_CLK__USBPHY1_RX_SQH		707
MX6Q_PAD_ENET_RX_ER__ENET_RX_ER			708
MX6Q_PAD_ENET_RX_ER__ESAI1_HCKR			709
MX6Q_PAD_ENET_RX_ER__SPDIF_IN1			710
MX6Q_PAD_ENET_RX_ER__ENET_1588_EVT2_OUT		711
MX6Q_PAD_ENET_RX_ER__GPIO_1_24			712
MX6Q_PAD_ENET_RX_ER__PHY_TDI			713
MX6Q_PAD_ENET_RX_ER__USBPHY1_RX_HS_RXD		714
MX6Q_PAD_ENET_CRS_DV__RESERVED_RSRVED		715
MX6Q_PAD_ENET_CRS_DV__ENET_RX_EN		716
MX6Q_PAD_ENET_CRS_DV__ESAI1_SCKT		717
MX6Q_PAD_ENET_CRS_DV__SPDIF_EXTCLK		718
MX6Q_PAD_ENET_CRS_DV__GPIO_1_25			719
MX6Q_PAD_ENET_CRS_DV__PHY_TDO			720
MX6Q_PAD_ENET_CRS_DV__USBPHY1_RX_FS_RXD		721
MX6Q_PAD_ENET_RXD1__MLB_MLBSIG			722
MX6Q_PAD_ENET_RXD1__ENET_RDATA_1		723
MX6Q_PAD_ENET_RXD1__ESAI1_FST			724
MX6Q_PAD_ENET_RXD1__ENET_1588_EVT3_OUT		725
MX6Q_PAD_ENET_RXD1__GPIO_1_26			726
MX6Q_PAD_ENET_RXD1__PHY_TCK			727
MX6Q_PAD_ENET_RXD1__USBPHY1_RX_DISCON		728
MX6Q_PAD_ENET_RXD0__OSC32K_32K_OUT		729
MX6Q_PAD_ENET_RXD0__ENET_RDATA_0		730
MX6Q_PAD_ENET_RXD0__ESAI1_HCKT			731
MX6Q_PAD_ENET_RXD0__SPDIF_OUT1			732
MX6Q_PAD_ENET_RXD0__GPIO_1_27			733
MX6Q_PAD_ENET_RXD0__PHY_TMS			734
MX6Q_PAD_ENET_RXD0__USBPHY1_PLL_CK20DIV		735
MX6Q_PAD_ENET_TX_EN__RESERVED_RSRVED		736
MX6Q_PAD_ENET_TX_EN__ENET_TX_EN			737
MX6Q_PAD_ENET_TX_EN__ESAI1_TX3_RX2		738
MX6Q_PAD_ENET_TX_EN__GPIO_1_28			739
MX6Q_PAD_ENET_TX_EN__SATA_PHY_TDI		740
MX6Q_PAD_ENET_TX_EN__USBPHY2_RX_SQH		741
MX6Q_PAD_ENET_TXD1__MLB_MLBCLK			742
MX6Q_PAD_ENET_TXD1__ENET_TDATA_1		743
MX6Q_PAD_ENET_TXD1__ESAI1_TX2_RX3		744
MX6Q_PAD_ENET_TXD1__ENET_1588_EVENT0_IN		745
MX6Q_PAD_ENET_TXD1__GPIO_1_29			746
MX6Q_PAD_ENET_TXD1__SATA_PHY_TDO		747
MX6Q_PAD_ENET_TXD1__USBPHY2_RX_HS_RXD		748
MX6Q_PAD_ENET_TXD0__RESERVED_RSRVED		749
MX6Q_PAD_ENET_TXD0__ENET_TDATA_0		750
MX6Q_PAD_ENET_TXD0__ESAI1_TX4_RX1		751
MX6Q_PAD_ENET_TXD0__GPIO_1_30			752
MX6Q_PAD_ENET_TXD0__SATA_PHY_TCK		753
MX6Q_PAD_ENET_TXD0__USBPHY2_RX_FS_RXD		754
MX6Q_PAD_ENET_MDC__MLB_MLBDAT			755
MX6Q_PAD_ENET_MDC__ENET_MDC			756
MX6Q_PAD_ENET_MDC__ESAI1_TX5_RX0		757
MX6Q_PAD_ENET_MDC__ENET_1588_EVENT1_IN		758
MX6Q_PAD_ENET_MDC__GPIO_1_31			759
MX6Q_PAD_ENET_MDC__SATA_PHY_TMS			760
MX6Q_PAD_ENET_MDC__USBPHY2_RX_DISCON		761
MX6Q_PAD_DRAM_D40__MMDC_DRAM_D_40		762
MX6Q_PAD_DRAM_D41__MMDC_DRAM_D_41		763
MX6Q_PAD_DRAM_D42__MMDC_DRAM_D_42		764
MX6Q_PAD_DRAM_D43__MMDC_DRAM_D_43		765
MX6Q_PAD_DRAM_D44__MMDC_DRAM_D_44		766
MX6Q_PAD_DRAM_D45__MMDC_DRAM_D_45		767
MX6Q_PAD_DRAM_D46__MMDC_DRAM_D_46		768
MX6Q_PAD_DRAM_D47__MMDC_DRAM_D_47		769
MX6Q_PAD_DRAM_SDQS5__MMDC_DRAM_SDQS_5		770
MX6Q_PAD_DRAM_DQM5__MMDC_DRAM_DQM_5		771
MX6Q_PAD_DRAM_D32__MMDC_DRAM_D_32		772
MX6Q_PAD_DRAM_D33__MMDC_DRAM_D_33		773
MX6Q_PAD_DRAM_D34__MMDC_DRAM_D_34		774
MX6Q_PAD_DRAM_D35__MMDC_DRAM_D_35		775
MX6Q_PAD_DRAM_D36__MMDC_DRAM_D_36		776
MX6Q_PAD_DRAM_D37__MMDC_DRAM_D_37		777
MX6Q_PAD_DRAM_D38__MMDC_DRAM_D_38		778
MX6Q_PAD_DRAM_D39__MMDC_DRAM_D_39		779
MX6Q_PAD_DRAM_DQM4__MMDC_DRAM_DQM_4		780
MX6Q_PAD_DRAM_SDQS4__MMDC_DRAM_SDQS_4		781
MX6Q_PAD_DRAM_D24__MMDC_DRAM_D_24		782
MX6Q_PAD_DRAM_D25__MMDC_DRAM_D_25		783
MX6Q_PAD_DRAM_D26__MMDC_DRAM_D_26		784
MX6Q_PAD_DRAM_D27__MMDC_DRAM_D_27		785
MX6Q_PAD_DRAM_D28__MMDC_DRAM_D_28		786
MX6Q_PAD_DRAM_D29__MMDC_DRAM_D_29		787
MX6Q_PAD_DRAM_SDQS3__MMDC_DRAM_SDQS_3		788
MX6Q_PAD_DRAM_D30__MMDC_DRAM_D_30		789
MX6Q_PAD_DRAM_D31__MMDC_DRAM_D_31		790
MX6Q_PAD_DRAM_DQM3__MMDC_DRAM_DQM_3		791
MX6Q_PAD_DRAM_D16__MMDC_DRAM_D_16		792
MX6Q_PAD_DRAM_D17__MMDC_DRAM_D_17		793
MX6Q_PAD_DRAM_D18__MMDC_DRAM_D_18		794
MX6Q_PAD_DRAM_D19__MMDC_DRAM_D_19		795
MX6Q_PAD_DRAM_D20__MMDC_DRAM_D_20		796
MX6Q_PAD_DRAM_D21__MMDC_DRAM_D_21		797
MX6Q_PAD_DRAM_D22__MMDC_DRAM_D_22		798
MX6Q_PAD_DRAM_SDQS2__MMDC_DRAM_SDQS_2		799
MX6Q_PAD_DRAM_D23__MMDC_DRAM_D_23		800
MX6Q_PAD_DRAM_DQM2__MMDC_DRAM_DQM_2		801
MX6Q_PAD_DRAM_A0__MMDC_DRAM_A_0			802
MX6Q_PAD_DRAM_A1__MMDC_DRAM_A_1			803
MX6Q_PAD_DRAM_A2__MMDC_DRAM_A_2			804
MX6Q_PAD_DRAM_A3__MMDC_DRAM_A_3			805
MX6Q_PAD_DRAM_A4__MMDC_DRAM_A_4			806
MX6Q_PAD_DRAM_A5__MMDC_DRAM_A_5			807
MX6Q_PAD_DRAM_A6__MMDC_DRAM_A_6			808
MX6Q_PAD_DRAM_A7__MMDC_DRAM_A_7			809
MX6Q_PAD_DRAM_A8__MMDC_DRAM_A_8			810
MX6Q_PAD_DRAM_A9__MMDC_DRAM_A_9			811
MX6Q_PAD_DRAM_A10__MMDC_DRAM_A_10		812
MX6Q_PAD_DRAM_A11__MMDC_DRAM_A_11		813
MX6Q_PAD_DRAM_A12__MMDC_DRAM_A_12		814
MX6Q_PAD_DRAM_A13__MMDC_DRAM_A_13		815
MX6Q_PAD_DRAM_A14__MMDC_DRAM_A_14		816
MX6Q_PAD_DRAM_A15__MMDC_DRAM_A_15		817
MX6Q_PAD_DRAM_CAS__MMDC_DRAM_CAS		818
MX6Q_PAD_DRAM_CS0__MMDC_DRAM_CS_0		819
MX6Q_PAD_DRAM_CS1__MMDC_DRAM_CS_1		820
MX6Q_PAD_DRAM_RAS__MMDC_DRAM_RAS		821
MX6Q_PAD_DRAM_RESET__MMDC_DRAM_RESET		822
MX6Q_PAD_DRAM_SDBA0__MMDC_DRAM_SDBA_0		823
MX6Q_PAD_DRAM_SDBA1__MMDC_DRAM_SDBA_1		824
MX6Q_PAD_DRAM_SDCLK_0__MMDC_DRAM_SDCLK0		825
MX6Q_PAD_DRAM_SDBA2__MMDC_DRAM_SDBA_2		826
MX6Q_PAD_DRAM_SDCKE0__MMDC_DRAM_SDCKE_0		827
MX6Q_PAD_DRAM_SDCLK_1__MMDC_DRAM_SDCLK1		828
MX6Q_PAD_DRAM_SDCKE1__MMDC_DRAM_SDCKE_1		829
MX6Q_PAD_DRAM_SDODT0__MMDC_DRAM_ODT_0		830
MX6Q_PAD_DRAM_SDODT1__MMDC_DRAM_ODT_1		831
MX6Q_PAD_DRAM_SDWE__MMDC_DRAM_SDWE		832
MX6Q_PAD_DRAM_D0__MMDC_DRAM_D_0			833
MX6Q_PAD_DRAM_D1__MMDC_DRAM_D_1			834
MX6Q_PAD_DRAM_D2__MMDC_DRAM_D_2			835
MX6Q_PAD_DRAM_D3__MMDC_DRAM_D_3			836
MX6Q_PAD_DRAM_D4__MMDC_DRAM_D_4			837
MX6Q_PAD_DRAM_D5__MMDC_DRAM_D_5			838
MX6Q_PAD_DRAM_SDQS0__MMDC_DRAM_SDQS_0		839
MX6Q_PAD_DRAM_D6__MMDC_DRAM_D_6			840
MX6Q_PAD_DRAM_D7__MMDC_DRAM_D_7			841
MX6Q_PAD_DRAM_DQM0__MMDC_DRAM_DQM_0		842
MX6Q_PAD_DRAM_D8__MMDC_DRAM_D_8			843
MX6Q_PAD_DRAM_D9__MMDC_DRAM_D_9			844
MX6Q_PAD_DRAM_D10__MMDC_DRAM_D_10		845
MX6Q_PAD_DRAM_D11__MMDC_DRAM_D_11		846
MX6Q_PAD_DRAM_D12__MMDC_DRAM_D_12		847
MX6Q_PAD_DRAM_D13__MMDC_DRAM_D_13		848
MX6Q_PAD_DRAM_D14__MMDC_DRAM_D_14		849
MX6Q_PAD_DRAM_SDQS1__MMDC_DRAM_SDQS_1		850
MX6Q_PAD_DRAM_D15__MMDC_DRAM_D_15		851
MX6Q_PAD_DRAM_DQM1__MMDC_DRAM_DQM_1		852
MX6Q_PAD_DRAM_D48__MMDC_DRAM_D_48		853
MX6Q_PAD_DRAM_D49__MMDC_DRAM_D_49		854
MX6Q_PAD_DRAM_D50__MMDC_DRAM_D_50		855
MX6Q_PAD_DRAM_D51__MMDC_DRAM_D_51		856
MX6Q_PAD_DRAM_D52__MMDC_DRAM_D_52		857
MX6Q_PAD_DRAM_D53__MMDC_DRAM_D_53		858
MX6Q_PAD_DRAM_D54__MMDC_DRAM_D_54		859
MX6Q_PAD_DRAM_D55__MMDC_DRAM_D_55		860
MX6Q_PAD_DRAM_SDQS6__MMDC_DRAM_SDQS_6		861
MX6Q_PAD_DRAM_DQM6__MMDC_DRAM_DQM_6		862
MX6Q_PAD_DRAM_D56__MMDC_DRAM_D_56		863
MX6Q_PAD_DRAM_SDQS7__MMDC_DRAM_SDQS_7		864
MX6Q_PAD_DRAM_D57__MMDC_DRAM_D_57		865
MX6Q_PAD_DRAM_D58__MMDC_DRAM_D_58		866
MX6Q_PAD_DRAM_D59__MMDC_DRAM_D_59		867
MX6Q_PAD_DRAM_D60__MMDC_DRAM_D_60		868
MX6Q_PAD_DRAM_DQM7__MMDC_DRAM_DQM_7		869
MX6Q_PAD_DRAM_D61__MMDC_DRAM_D_61		870
MX6Q_PAD_DRAM_D62__MMDC_DRAM_D_62		871
MX6Q_PAD_DRAM_D63__MMDC_DRAM_D_63		872
MX6Q_PAD_KEY_COL0__ECSPI1_SCLK			873
MX6Q_PAD_KEY_COL0__ENET_RDATA_3			874
MX6Q_PAD_KEY_COL0__AUDMUX_AUD5_TXC		875
MX6Q_PAD_KEY_COL0__KPP_COL_0			876
MX6Q_PAD_KEY_COL0__UART4_TXD			877
MX6Q_PAD_KEY_COL0__GPIO_4_6			878
MX6Q_PAD_KEY_COL0__DCIC1_DCIC_OUT		879
MX6Q_PAD_KEY_COL0__SRC_ANY_PU_RST		880
MX6Q_PAD_KEY_ROW0__ECSPI1_MOSI			881
MX6Q_PAD_KEY_ROW0__ENET_TDATA_3			882
MX6Q_PAD_KEY_ROW0__AUDMUX_AUD5_TXD		883
MX6Q_PAD_KEY_ROW0__KPP_ROW_0			884
MX6Q_PAD_KEY_ROW0__UART4_RXD			885
MX6Q_PAD_KEY_ROW0__GPIO_4_7			886
MX6Q_PAD_KEY_ROW0__DCIC2_DCIC_OUT		887
MX6Q_PAD_KEY_ROW0__PL301_PER1_HADR_0		888
MX6Q_PAD_KEY_COL1__ECSPI1_MISO			889
MX6Q_PAD_KEY_COL1__ENET_MDIO			890
MX6Q_PAD_KEY_COL1__AUDMUX_AUD5_TXFS		891
MX6Q_PAD_KEY_COL1__KPP_COL_1			892
MX6Q_PAD_KEY_COL1__UART5_TXD			893
MX6Q_PAD_KEY_COL1__GPIO_4_8			894
MX6Q_PAD_KEY_COL1__USDHC1_VSELECT		895
MX6Q_PAD_KEY_COL1__PL301MX_PER1_HADR_1		896
MX6Q_PAD_KEY_ROW1__ECSPI1_SS0			897
MX6Q_PAD_KEY_ROW1__ENET_COL			898
MX6Q_PAD_KEY_ROW1__AUDMUX_AUD5_RXD		899
MX6Q_PAD_KEY_ROW1__KPP_ROW_1			900
MX6Q_PAD_KEY_ROW1__UART5_RXD			901
MX6Q_PAD_KEY_ROW1__GPIO_4_9			902
MX6Q_PAD_KEY_ROW1__USDHC2_VSELECT		903
MX6Q_PAD_KEY_ROW1__PL301_PER1_HADDR_2		904
MX6Q_PAD_KEY_COL2__ECSPI1_SS1			905
MX6Q_PAD_KEY_COL2__ENET_RDATA_2			906
MX6Q_PAD_KEY_COL2__CAN1_TXCAN			907
MX6Q_PAD_KEY_COL2__KPP_COL_2			908
MX6Q_PAD_KEY_COL2__ENET_MDC			909
MX6Q_PAD_KEY_COL2__GPIO_4_10			910
MX6Q_PAD_KEY_COL2__USBOH3_H1_PWRCTL_WKP		911
MX6Q_PAD_KEY_COL2__PL301_PER1_HADDR_3		912
MX6Q_PAD_KEY_ROW2__ECSPI1_SS2			913
MX6Q_PAD_KEY_ROW2__ENET_TDATA_2			914
MX6Q_PAD_KEY_ROW2__CAN1_RXCAN			915
MX6Q_PAD_KEY_ROW2__KPP_ROW_2			916
MX6Q_PAD_KEY_ROW2__USDHC2_VSELECT		917
MX6Q_PAD_KEY_ROW2__GPIO_4_11			918
MX6Q_PAD_KEY_ROW2__HDMI_TX_CEC_LINE		919
MX6Q_PAD_KEY_ROW2__PL301_PER1_HADR_4		920
MX6Q_PAD_KEY_COL3__ECSPI1_SS3			921
MX6Q_PAD_KEY_COL3__ENET_CRS			922
MX6Q_PAD_KEY_COL3__HDMI_TX_DDC_SCL		923
MX6Q_PAD_KEY_COL3__KPP_COL_3			924
MX6Q_PAD_KEY_COL3__I2C2_SCL			925
MX6Q_PAD_KEY_COL3__GPIO_4_12			926
MX6Q_PAD_KEY_COL3__SPDIF_IN1			927
MX6Q_PAD_KEY_COL3__PL301_PER1_HADR_5		928
MX6Q_PAD_KEY_ROW3__OSC32K_32K_OUT		929
MX6Q_PAD_KEY_ROW3__ASRC_ASRC_EXT_CLK		930
MX6Q_PAD_KEY_ROW3__HDMI_TX_DDC_SDA		931
MX6Q_PAD_KEY_ROW3__KPP_ROW_3			932
MX6Q_PAD_KEY_ROW3__I2C2_SDA			933
MX6Q_PAD_KEY_ROW3__GPIO_4_13			934
MX6Q_PAD_KEY_ROW3__USDHC1_VSELECT		935
MX6Q_PAD_KEY_ROW3__PL301_PER1_HADR_6		936
MX6Q_PAD_KEY_COL4__CAN2_TXCAN			937
MX6Q_PAD_KEY_COL4__IPU1_SISG_4			938
MX6Q_PAD_KEY_COL4__USBOH3_USBOTG_OC		939
MX6Q_PAD_KEY_COL4__KPP_COL_4			940
MX6Q_PAD_KEY_COL4__UART5_RTS			941
MX6Q_PAD_KEY_COL4__GPIO_4_14			942
MX6Q_PAD_KEY_COL4__MMDC_DEBUG_49		943
MX6Q_PAD_KEY_COL4__PL301_PER1_HADDR_7		944
MX6Q_PAD_KEY_ROW4__CAN2_RXCAN			945
MX6Q_PAD_KEY_ROW4__IPU1_SISG_5			946
MX6Q_PAD_KEY_ROW4__USBOH3_USBOTG_PWR		947
MX6Q_PAD_KEY_ROW4__KPP_ROW_4			948
MX6Q_PAD_KEY_ROW4__UART5_CTS			949
MX6Q_PAD_KEY_ROW4__GPIO_4_15			950
MX6Q_PAD_KEY_ROW4__MMDC_DEBUG_50		951
MX6Q_PAD_KEY_ROW4__PL301_PER1_HADR_8		952
MX6Q_PAD_GPIO_0__CCM_CLKO			953
MX6Q_PAD_GPIO_0__KPP_COL_5			954
MX6Q_PAD_GPIO_0__ASRC_ASRC_EXT_CLK		955
MX6Q_PAD_GPIO_0__EPIT1_EPITO			956
MX6Q_PAD_GPIO_0__GPIO_1_0			957
MX6Q_PAD_GPIO_0__USBOH3_USBH1_PWR		958
MX6Q_PAD_GPIO_0__SNVS_HP_WRAP_SNVS_VIO5		959
MX6Q_PAD_GPIO_1__ESAI1_SCKR			960
MX6Q_PAD_GPIO_1__WDOG2_WDOG_B			961
MX6Q_PAD_GPIO_1__KPP_ROW_5			962
MX6Q_PAD_GPIO_1__PWM2_PWMO			963
MX6Q_PAD_GPIO_1__GPIO_1_1			964
MX6Q_PAD_GPIO_1__USDHC1_CD			965
MX6Q_PAD_GPIO_1__SRC_TESTER_ACK			966
MX6Q_PAD_GPIO_9__ESAI1_FSR			967
MX6Q_PAD_GPIO_9__WDOG1_WDOG_B			968
MX6Q_PAD_GPIO_9__KPP_COL_6			969
MX6Q_PAD_GPIO_9__CCM_REF_EN_B			970
MX6Q_PAD_GPIO_9__PWM1_PWMO			971
MX6Q_PAD_GPIO_9__GPIO_1_9			972
MX6Q_PAD_GPIO_9__USDHC1_WP			973
MX6Q_PAD_GPIO_9__SRC_EARLY_RST			974
MX6Q_PAD_GPIO_3__ESAI1_HCKR			975
MX6Q_PAD_GPIO_3__OBSERVE_MUX_INT_OUT0		976
MX6Q_PAD_GPIO_3__I2C3_SCL			977
MX6Q_PAD_GPIO_3__ANATOP_24M_OUT			978
MX6Q_PAD_GPIO_3__CCM_CLKO2			979
MX6Q_PAD_GPIO_3__GPIO_1_3			980
MX6Q_PAD_GPIO_3__USBOH3_USBH1_OC		981
MX6Q_PAD_GPIO_3__MLB_MLBCLK			982
MX6Q_PAD_GPIO_6__ESAI1_SCKT			983
MX6Q_PAD_GPIO_6__OBSERVE_MUX_INT_OUT1		984
MX6Q_PAD_GPIO_6__I2C3_SDA			985
MX6Q_PAD_GPIO_6__CCM_CCM_OUT_0			986
MX6Q_PAD_GPIO_6__CSU_CSU_INT_DEB		987
MX6Q_PAD_GPIO_6__GPIO_1_6			988
MX6Q_PAD_GPIO_6__USDHC2_LCTL			989
MX6Q_PAD_GPIO_6__MLB_MLBSIG			990
MX6Q_PAD_GPIO_2__ESAI1_FST			991
MX6Q_PAD_GPIO_2__OBSERVE_MUX_INT_OUT2		992
MX6Q_PAD_GPIO_2__KPP_ROW_6			993
MX6Q_PAD_GPIO_2__CCM_CCM_OUT_1			994
MX6Q_PAD_GPIO_2__CSU_CSU_ALARM_AUT_0		995
MX6Q_PAD_GPIO_2__GPIO_1_2			996
MX6Q_PAD_GPIO_2__USDHC2_WP			997
MX6Q_PAD_GPIO_2__MLB_MLBDAT			998
MX6Q_PAD_GPIO_4__ESAI1_HCKT			999
MX6Q_PAD_GPIO_4__OBSERVE_MUX_INT_OUT3		1000
MX6Q_PAD_GPIO_4__KPP_COL_7			1001
MX6Q_PAD_GPIO_4__CCM_CCM_OUT_2			1002
MX6Q_PAD_GPIO_4__CSU_CSU_ALARM_AUT_1		1003
MX6Q_PAD_GPIO_4__GPIO_1_4			1004
MX6Q_PAD_GPIO_4__USDHC2_CD			1005
MX6Q_PAD_GPIO_4__OCOTP_CRL_WRAR_FUSE_LA		1006
MX6Q_PAD_GPIO_5__ESAI1_TX2_RX3			1007
MX6Q_PAD_GPIO_5__OBSERVE_MUX_INT_OUT4		1008
MX6Q_PAD_GPIO_5__KPP_ROW_7			1009
MX6Q_PAD_GPIO_5__CCM_CLKO			1010
MX6Q_PAD_GPIO_5__CSU_CSU_ALARM_AUT_2		1011
MX6Q_PAD_GPIO_5__GPIO_1_5			1012
MX6Q_PAD_GPIO_5__I2C3_SCL			1013
MX6Q_PAD_GPIO_5__CHEETAH_EVENTI			1014
MX6Q_PAD_GPIO_7__ESAI1_TX4_RX1			1015
MX6Q_PAD_GPIO_7__ECSPI5_RDY			1016
MX6Q_PAD_GPIO_7__EPIT1_EPITO			1017
MX6Q_PAD_GPIO_7__CAN1_TXCAN			1018
MX6Q_PAD_GPIO_7__UART2_TXD			1019
MX6Q_PAD_GPIO_7__GPIO_1_7			1020
MX6Q_PAD_GPIO_7__SPDIF_PLOCK			1021
MX6Q_PAD_GPIO_7__USBOH3_OTGUSB_HST_MODE		1022
MX6Q_PAD_GPIO_8__ESAI1_TX5_RX0			1023
MX6Q_PAD_GPIO_8__ANATOP_ANATOP_32K_OUT		1024
MX6Q_PAD_GPIO_8__EPIT2_EPITO			1025
MX6Q_PAD_GPIO_8__CAN1_RXCAN			1026
MX6Q_PAD_GPIO_8__UART2_RXD			1027
MX6Q_PAD_GPIO_8__GPIO_1_8			1028
MX6Q_PAD_GPIO_8__SPDIF_SRCLK			1029
MX6Q_PAD_GPIO_8__USBOH3_OTG_PWRCTL_WAK		1030
MX6Q_PAD_GPIO_16__ESAI1_TX3_RX2			1031
MX6Q_PAD_GPIO_16__ENET_1588_EVENT2_IN		1032
MX6Q_PAD_GPIO_16__ENET_ETHERNET_REF_OUT		1033
MX6Q_PAD_GPIO_16__USDHC1_LCTL			1034
MX6Q_PAD_GPIO_16__SPDIF_IN1			1035
MX6Q_PAD_GPIO_16__GPIO_7_11			1036
MX6Q_PAD_GPIO_16__I2C3_SDA			1037
MX6Q_PAD_GPIO_16__SJC_DE_B			1038
MX6Q_PAD_GPIO_17__ESAI1_TX0			1039
MX6Q_PAD_GPIO_17__ENET_1588_EVENT3_IN		1040
MX6Q_PAD_GPIO_17__CCM_PMIC_RDY			1041
MX6Q_PAD_GPIO_17__SDMA_SDMA_EXT_EVENT_0		1042
MX6Q_PAD_GPIO_17__SPDIF_OUT1			1043
MX6Q_PAD_GPIO_17__GPIO_7_12			1044
MX6Q_PAD_GPIO_17__SJC_JTAG_ACT			1045
MX6Q_PAD_GPIO_18__ESAI1_TX1			1046
MX6Q_PAD_GPIO_18__ENET_RX_CLK			1047
MX6Q_PAD_GPIO_18__USDHC3_VSELECT		1048
MX6Q_PAD_GPIO_18__SDMA_SDMA_EXT_EVENT_1		1049
MX6Q_PAD_GPIO_18__ASRC_ASRC_EXT_CLK		1050
MX6Q_PAD_GPIO_18__GPIO_7_13			1051
MX6Q_PAD_GPIO_18__SNVS_HP_WRA_SNVS_VIO5		1052
MX6Q_PAD_GPIO_18__SRC_SYSTEM_RST		1053
MX6Q_PAD_GPIO_19__KPP_COL_5			1054
MX6Q_PAD_GPIO_19__ENET_1588_EVENT0_OUT		1055
MX6Q_PAD_GPIO_19__SPDIF_OUT1			1056
MX6Q_PAD_GPIO_19__CCM_CLKO			1057
MX6Q_PAD_GPIO_19__ECSPI1_RDY			1058
MX6Q_PAD_GPIO_19__GPIO_4_5			1059
MX6Q_PAD_GPIO_19__ENET_TX_ER			1060
MX6Q_PAD_GPIO_19__SRC_INT_BOOT			1061
MX6Q_PAD_CSI0_PIXCLK__IPU1_CSI0_PIXCLK		1062
MX6Q_PAD_CSI0_PIXCLK__PCIE_CTRL_MUX_12		1063
MX6Q_PAD_CSI0_PIXCLK__SDMA_DEBUG_PC_0		1064
MX6Q_PAD_CSI0_PIXCLK__GPIO_5_18			1065
MX6Q_PAD_CSI0_PIXCLK___MMDC_DEBUG_29		1066
MX6Q_PAD_CSI0_PIXCLK__CHEETAH_EVENTO		1067
MX6Q_PAD_CSI0_MCLK__IPU1_CSI0_HSYNC		1068
MX6Q_PAD_CSI0_MCLK__PCIE_CTRL_MUX_13		1069
MX6Q_PAD_CSI0_MCLK__CCM_CLKO			1070
MX6Q_PAD_CSI0_MCLK__SDMA_DEBUG_PC_1		1071
MX6Q_PAD_CSI0_MCLK__GPIO_5_19			1072
MX6Q_PAD_CSI0_MCLK__MMDC_MMDC_DEBUG_30		1073
MX6Q_PAD_CSI0_MCLK__CHEETAH_TRCTL		1074
MX6Q_PAD_CSI0_DATA_EN__IPU1_CSI0_DA_EN		1075
MX6Q_PAD_CSI0_DATA_EN__WEIM_WEIM_D_0		1076
MX6Q_PAD_CSI0_DATA_EN__PCIE_CTRL_MUX_14		1077
MX6Q_PAD_CSI0_DATA_EN__SDMA_DEBUG_PC_2		1078
MX6Q_PAD_CSI0_DATA_EN__GPIO_5_20		1079
MX6Q_PAD_CSI0_DATA_EN__MMDC_DEBUG_31		1080
MX6Q_PAD_CSI0_DATA_EN__CHEETAH_TRCLK		1081
MX6Q_PAD_CSI0_VSYNC__IPU1_CSI0_VSYNC		1082
MX6Q_PAD_CSI0_VSYNC__WEIM_WEIM_D_1		1083
MX6Q_PAD_CSI0_VSYNC__PCIE_CTRL_MUX_15		1084
MX6Q_PAD_CSI0_VSYNC__SDMA_DEBUG_PC_3		1085
MX6Q_PAD_CSI0_VSYNC__GPIO_5_21			1086
MX6Q_PAD_CSI0_VSYNC__MMDC_DEBUG_32		1087
MX6Q_PAD_CSI0_VSYNC__CHEETAH_TRACE_0		1088
MX6Q_PAD_CSI0_DAT4__IPU1_CSI0_D_4		1089
MX6Q_PAD_CSI0_DAT4__WEIM_WEIM_D_2		1090
MX6Q_PAD_CSI0_DAT4__ECSPI1_SCLK			1091
MX6Q_PAD_CSI0_DAT4__KPP_COL_5			1092
MX6Q_PAD_CSI0_DAT4__AUDMUX_AUD3_TXC		1093
MX6Q_PAD_CSI0_DAT4__GPIO_5_22			1094
MX6Q_PAD_CSI0_DAT4__MMDC_DEBUG_43		1095
MX6Q_PAD_CSI0_DAT4__CHEETAH_TRACE_1		1096
MX6Q_PAD_CSI0_DAT5__IPU1_CSI0_D_5		1097
MX6Q_PAD_CSI0_DAT5__WEIM_WEIM_D_3		1098
MX6Q_PAD_CSI0_DAT5__ECSPI1_MOSI			1099
MX6Q_PAD_CSI0_DAT5__KPP_ROW_5			1100
MX6Q_PAD_CSI0_DAT5__AUDMUX_AUD3_TXD		1101
MX6Q_PAD_CSI0_DAT5__GPIO_5_23			1102
MX6Q_PAD_CSI0_DAT5__MMDC_MMDC_DEBUG_44		1103
MX6Q_PAD_CSI0_DAT5__CHEETAH_TRACE_2		1104
MX6Q_PAD_CSI0_DAT6__IPU1_CSI0_D_6		1105
MX6Q_PAD_CSI0_DAT6__WEIM_WEIM_D_4		1106
MX6Q_PAD_CSI0_DAT6__ECSPI1_MISO			1107
MX6Q_PAD_CSI0_DAT6__KPP_COL_6			1108
MX6Q_PAD_CSI0_DAT6__AUDMUX_AUD3_TXFS		1109
MX6Q_PAD_CSI0_DAT6__GPIO_5_24			1110
MX6Q_PAD_CSI0_DAT6__MMDC_MMDC_DEBUG_45		1111
MX6Q_PAD_CSI0_DAT6__CHEETAH_TRACE_3		1112
MX6Q_PAD_CSI0_DAT7__IPU1_CSI0_D_7		1113
MX6Q_PAD_CSI0_DAT7__WEIM_WEIM_D_5		1114
MX6Q_PAD_CSI0_DAT7__ECSPI1_SS0			1115
MX6Q_PAD_CSI0_DAT7__KPP_ROW_6			1116
MX6Q_PAD_CSI0_DAT7__AUDMUX_AUD3_RXD		1117
MX6Q_PAD_CSI0_DAT7__GPIO_5_25			1118
MX6Q_PAD_CSI0_DAT7__MMDC_MMDC_DEBUG_46		1119
MX6Q_PAD_CSI0_DAT7__CHEETAH_TRACE_4		1120
MX6Q_PAD_CSI0_DAT8__IPU1_CSI0_D_8		1121
MX6Q_PAD_CSI0_DAT8__WEIM_WEIM_D_6		1122
MX6Q_PAD_CSI0_DAT8__ECSPI2_SCLK			1123
MX6Q_PAD_CSI0_DAT8__KPP_COL_7			1124
MX6Q_PAD_CSI0_DAT8__I2C1_SDA			1125
MX6Q_PAD_CSI0_DAT8__GPIO_5_26			1126
MX6Q_PAD_CSI0_DAT8__MMDC_MMDC_DEBUG_47		1127
MX6Q_PAD_CSI0_DAT8__CHEETAH_TRACE_5		1128
MX6Q_PAD_CSI0_DAT9__IPU1_CSI0_D_9		1129
MX6Q_PAD_CSI0_DAT9__WEIM_WEIM_D_7		1130
MX6Q_PAD_CSI0_DAT9__ECSPI2_MOSI			1131
MX6Q_PAD_CSI0_DAT9__KPP_ROW_7			1132
MX6Q_PAD_CSI0_DAT9__I2C1_SCL			1133
MX6Q_PAD_CSI0_DAT9__GPIO_5_27			1134
MX6Q_PAD_CSI0_DAT9__MMDC_MMDC_DEBUG_48		1135
MX6Q_PAD_CSI0_DAT9__CHEETAH_TRACE_6		1136
MX6Q_PAD_CSI0_DAT10__IPU1_CSI0_D_10		1137
MX6Q_PAD_CSI0_DAT10__AUDMUX_AUD3_RXC		1138
MX6Q_PAD_CSI0_DAT10__ECSPI2_MISO		1139
MX6Q_PAD_CSI0_DAT10__UART1_TXD			1140
MX6Q_PAD_CSI0_DAT10__SDMA_DEBUG_PC_4		1141
MX6Q_PAD_CSI0_DAT10__GPIO_5_28			1142
MX6Q_PAD_CSI0_DAT10__MMDC_MMDC_DEBUG_33		1143
MX6Q_PAD_CSI0_DAT10__CHEETAH_TRACE_7		1144
MX6Q_PAD_CSI0_DAT11__IPU1_CSI0_D_11		1145
MX6Q_PAD_CSI0_DAT11__AUDMUX_AUD3_RXFS		1146
MX6Q_PAD_CSI0_DAT11__ECSPI2_SS0			1147
MX6Q_PAD_CSI0_DAT11__UART1_RXD			1148
MX6Q_PAD_CSI0_DAT11__SDMA_DEBUG_PC_5		1149
MX6Q_PAD_CSI0_DAT11__GPIO_5_29			1150
MX6Q_PAD_CSI0_DAT11__MMDC_MMDC_DEBUG_34		1151
MX6Q_PAD_CSI0_DAT11__CHEETAH_TRACE_8		1152
MX6Q_PAD_CSI0_DAT12__IPU1_CSI0_D_12		1153
MX6Q_PAD_CSI0_DAT12__WEIM_WEIM_D_8		1154
MX6Q_PAD_CSI0_DAT12__PCIE_CTRL_MUX_16		1155
MX6Q_PAD_CSI0_DAT12__UART4_TXD			1156
MX6Q_PAD_CSI0_DAT12__SDMA_DEBUG_PC_6		1157
MX6Q_PAD_CSI0_DAT12__GPIO_5_30			1158
MX6Q_PAD_CSI0_DAT12__MMDC_MMDC_DEBUG_35		1159
MX6Q_PAD_CSI0_DAT12__CHEETAH_TRACE_9		1160
MX6Q_PAD_CSI0_DAT13__IPU1_CSI0_D_13		1161
MX6Q_PAD_CSI0_DAT13__WEIM_WEIM_D_9		1162
MX6Q_PAD_CSI0_DAT13__PCIE_CTRL_MUX_17		1163
MX6Q_PAD_CSI0_DAT13__UART4_RXD			1164
MX6Q_PAD_CSI0_DAT13__SDMA_DEBUG_PC_7		1165
MX6Q_PAD_CSI0_DAT13__GPIO_5_31			1166
MX6Q_PAD_CSI0_DAT13__MMDC_MMDC_DEBUG_36		1167
MX6Q_PAD_CSI0_DAT13__CHEETAH_TRACE_10		1168
MX6Q_PAD_CSI0_DAT14__IPU1_CSI0_D_14		1169
MX6Q_PAD_CSI0_DAT14__WEIM_WEIM_D_10		1170
MX6Q_PAD_CSI0_DAT14__PCIE_CTRL_MUX_18		1171
MX6Q_PAD_CSI0_DAT14__UART5_TXD			1172
MX6Q_PAD_CSI0_DAT14__SDMA_DEBUG_PC_8		1173
MX6Q_PAD_CSI0_DAT14__GPIO_6_0			1174
MX6Q_PAD_CSI0_DAT14__MMDC_MMDC_DEBUG_37		1175
MX6Q_PAD_CSI0_DAT14__CHEETAH_TRACE_11		1176
MX6Q_PAD_CSI0_DAT15__IPU1_CSI0_D_15		1177
MX6Q_PAD_CSI0_DAT15__WEIM_WEIM_D_11		1178
MX6Q_PAD_CSI0_DAT15__PCIE_CTRL_MUX_19		1179
MX6Q_PAD_CSI0_DAT15__UART5_RXD			1180
MX6Q_PAD_CSI0_DAT15__SDMA_DEBUG_PC_9		1181
MX6Q_PAD_CSI0_DAT15__GPIO_6_1			1182
MX6Q_PAD_CSI0_DAT15__MMDC_MMDC_DEBUG_38		1183
MX6Q_PAD_CSI0_DAT15__CHEETAH_TRACE_12		1184
MX6Q_PAD_CSI0_DAT16__IPU1_CSI0_D_16		1185
MX6Q_PAD_CSI0_DAT16__WEIM_WEIM_D_12		1186
MX6Q_PAD_CSI0_DAT16__PCIE_CTRL_MUX_20		1187
MX6Q_PAD_CSI0_DAT16__UART4_RTS			1188
MX6Q_PAD_CSI0_DAT16__SDMA_DEBUG_PC_10		1189
MX6Q_PAD_CSI0_DAT16__GPIO_6_2			1190
MX6Q_PAD_CSI0_DAT16__MMDC_MMDC_DEBUG_39		1191
MX6Q_PAD_CSI0_DAT16__CHEETAH_TRACE_13		1192
MX6Q_PAD_CSI0_DAT17__IPU1_CSI0_D_17		1193
MX6Q_PAD_CSI0_DAT17__WEIM_WEIM_D_13		1194
MX6Q_PAD_CSI0_DAT17__PCIE_CTRL_MUX_21		1195
MX6Q_PAD_CSI0_DAT17__UART4_CTS			1196
MX6Q_PAD_CSI0_DAT17__SDMA_DEBUG_PC_11		1197
MX6Q_PAD_CSI0_DAT17__GPIO_6_3			1198
MX6Q_PAD_CSI0_DAT17__MMDC_MMDC_DEBUG_40		1199
MX6Q_PAD_CSI0_DAT17__CHEETAH_TRACE_14		1200
MX6Q_PAD_CSI0_DAT18__IPU1_CSI0_D_18		1201
MX6Q_PAD_CSI0_DAT18__WEIM_WEIM_D_14		1202
MX6Q_PAD_CSI0_DAT18__PCIE_CTRL_MUX_22		1203
MX6Q_PAD_CSI0_DAT18__UART5_RTS			1204
MX6Q_PAD_CSI0_DAT18__SDMA_DEBUG_PC_12		1205
MX6Q_PAD_CSI0_DAT18__GPIO_6_4			1206
MX6Q_PAD_CSI0_DAT18__MMDC_MMDC_DEBUG_41		1207
MX6Q_PAD_CSI0_DAT18__CHEETAH_TRACE_15		1208
MX6Q_PAD_CSI0_DAT19__IPU1_CSI0_D_19		1209
MX6Q_PAD_CSI0_DAT19__WEIM_WEIM_D_15		1210
MX6Q_PAD_CSI0_DAT19__PCIE_CTRL_MUX_23		1211
MX6Q_PAD_CSI0_DAT19__UART5_CTS			1212
MX6Q_PAD_CSI0_DAT19__SDMA_DEBUG_PC_13		1213
MX6Q_PAD_CSI0_DAT19__GPIO_6_5			1214
MX6Q_PAD_CSI0_DAT19__MMDC_MMDC_DEBUG_42		1215
MX6Q_PAD_CSI0_DAT19__ANATOP_TESTO_9		1216
MX6Q_PAD_JTAG_TMS__SJC_TMS			1217
MX6Q_PAD_JTAG_MOD__SJC_MOD			1218
MX6Q_PAD_JTAG_TRSTB__SJC_TRSTB			1219
MX6Q_PAD_JTAG_TDI__SJC_TDI			1220
MX6Q_PAD_JTAG_TCK__SJC_TCK			1221
MX6Q_PAD_JTAG_TDO__SJC_TDO			1222
MX6Q_PAD_LVDS1_TX3_P__LDB_LVDS1_TX3		1223
MX6Q_PAD_LVDS1_TX2_P__LDB_LVDS1_TX2		1224
MX6Q_PAD_LVDS1_CLK_P__LDB_LVDS1_CLK		1225
MX6Q_PAD_LVDS1_TX1_P__LDB_LVDS1_TX1		1226
MX6Q_PAD_LVDS1_TX0_P__LDB_LVDS1_TX0		1227
MX6Q_PAD_LVDS0_TX3_P__LDB_LVDS0_TX3		1228
MX6Q_PAD_LVDS0_CLK_P__LDB_LVDS0_CLK		1229
MX6Q_PAD_LVDS0_TX2_P__LDB_LVDS0_TX2		1230
MX6Q_PAD_LVDS0_TX1_P__LDB_LVDS0_TX1		1231
MX6Q_PAD_LVDS0_TX0_P__LDB_LVDS0_TX0		1232
MX6Q_PAD_TAMPER__SNVS_LP_WRAP_SNVS_TD1		1233
MX6Q_PAD_PMIC_ON_REQ__SNVS_LPWRAP_WKALM		1234
MX6Q_PAD_PMIC_STBY_REQ__CCM_PMIC_STBYRQ		1235
MX6Q_PAD_POR_B__SRC_POR_B			1236
MX6Q_PAD_BOOT_MODE1__SRC_BOOT_MODE_1		1237
MX6Q_PAD_RESET_IN_B__SRC_RESET_B		1238
MX6Q_PAD_BOOT_MODE0__SRC_BOOT_MODE_0		1239
MX6Q_PAD_TEST_MODE__TCU_TEST_MODE		1240
MX6Q_PAD_SD3_DAT7__USDHC3_DAT7			1241
MX6Q_PAD_SD3_DAT7__UART1_TXD			1242
MX6Q_PAD_SD3_DAT7__PCIE_CTRL_MUX_24		1243
MX6Q_PAD_SD3_DAT7__USBOH3_UH3_DFD_OUT_0		1244
MX6Q_PAD_SD3_DAT7__USBOH3_UH2_DFD_OUT_0		1245
MX6Q_PAD_SD3_DAT7__GPIO_6_17			1246
MX6Q_PAD_SD3_DAT7__MIPI_CORE_DPHY_IN_12		1247
MX6Q_PAD_SD3_DAT7__USBPHY2_CLK20DIV		1248
MX6Q_PAD_SD3_DAT6__USDHC3_DAT6			1249
MX6Q_PAD_SD3_DAT6__UART1_RXD			1250
MX6Q_PAD_SD3_DAT6__PCIE_CTRL_MUX_25		1251
MX6Q_PAD_SD3_DAT6__USBOH3_UH3_DFD_OUT_1		1252
MX6Q_PAD_SD3_DAT6__USBOH3_UH2_DFD_OUT_1		1253
MX6Q_PAD_SD3_DAT6__GPIO_6_18			1254
MX6Q_PAD_SD3_DAT6__MIPI_CORE_DPHY_IN_13		1255
MX6Q_PAD_SD3_DAT6__ANATOP_TESTO_10		1256
MX6Q_PAD_SD3_DAT5__USDHC3_DAT5			1257
MX6Q_PAD_SD3_DAT5__UART2_TXD			1258
MX6Q_PAD_SD3_DAT5__PCIE_CTRL_MUX_26		1259
MX6Q_PAD_SD3_DAT5__USBOH3_UH3_DFD_OUT_2		1260
MX6Q_PAD_SD3_DAT5__USBOH3_UH2_DFD_OUT_2		1261
MX6Q_PAD_SD3_DAT5__GPIO_7_0			1262
MX6Q_PAD_SD3_DAT5__MIPI_CORE_DPHY_IN_14		1263
MX6Q_PAD_SD3_DAT5__ANATOP_TESTO_11		1264
MX6Q_PAD_SD3_DAT4__USDHC3_DAT4			1265
MX6Q_PAD_SD3_DAT4__UART2_RXD			1266
MX6Q_PAD_SD3_DAT4__PCIE_CTRL_MUX_27		1267
MX6Q_PAD_SD3_DAT4__USBOH3_UH3_DFD_OUT_3		1268
MX6Q_PAD_SD3_DAT4__USBOH3_UH2_DFD_OUT_3		1269
MX6Q_PAD_SD3_DAT4__GPIO_7_1			1270
MX6Q_PAD_SD3_DAT4__MIPI_CORE_DPHY_IN_15		1271
MX6Q_PAD_SD3_DAT4__ANATOP_TESTO_12		1272
MX6Q_PAD_SD3_CMD__USDHC3_CMD			1273
MX6Q_PAD_SD3_CMD__UART2_CTS			1274
MX6Q_PAD_SD3_CMD__CAN1_TXCAN			1275
MX6Q_PAD_SD3_CMD__USBOH3_UH3_DFD_OUT_4		1276
MX6Q_PAD_SD3_CMD__USBOH3_UH2_DFD_OUT_4		1277
MX6Q_PAD_SD3_CMD__GPIO_7_2			1278
MX6Q_PAD_SD3_CMD__MIPI_CORE_DPHY_IN_16		1279
MX6Q_PAD_SD3_CMD__ANATOP_TESTO_13		1280
MX6Q_PAD_SD3_CLK__USDHC3_CLK			1281
MX6Q_PAD_SD3_CLK__UART2_RTS			1282
MX6Q_PAD_SD3_CLK__CAN1_RXCAN			1283
MX6Q_PAD_SD3_CLK__USBOH3_UH3_DFD_OUT_5		1284
MX6Q_PAD_SD3_CLK__USBOH3_UH2_DFD_OUT_5		1285
MX6Q_PAD_SD3_CLK__GPIO_7_3			1286
MX6Q_PAD_SD3_CLK__MIPI_CORE_DPHY_IN_17		1287
MX6Q_PAD_SD3_CLK__ANATOP_TESTO_14		1288
MX6Q_PAD_SD3_DAT0__USDHC3_DAT0			1289
MX6Q_PAD_SD3_DAT0__UART1_CTS			1290
MX6Q_PAD_SD3_DAT0__CAN2_TXCAN			1291
MX6Q_PAD_SD3_DAT0__USBOH3_UH3_DFD_OUT_6		1292
MX6Q_PAD_SD3_DAT0__USBOH3_UH2_DFD_OUT_6		1293
MX6Q_PAD_SD3_DAT0__GPIO_7_4			1294
MX6Q_PAD_SD3_DAT0__MIPI_CORE_DPHY_IN_18		1295
MX6Q_PAD_SD3_DAT0__ANATOP_TESTO_15		1296
MX6Q_PAD_SD3_DAT1__USDHC3_DAT1			1297
MX6Q_PAD_SD3_DAT1__UART1_RTS			1298
MX6Q_PAD_SD3_DAT1__CAN2_RXCAN			1299
MX6Q_PAD_SD3_DAT1__USBOH3_UH3_DFD_OUT_7		1300
MX6Q_PAD_SD3_DAT1__USBOH3_UH2_DFD_OUT_7		1301
MX6Q_PAD_SD3_DAT1__GPIO_7_5			1302
MX6Q_PAD_SD3_DAT1__MIPI_CORE_DPHY_IN_19		1303
MX6Q_PAD_SD3_DAT1__ANATOP_TESTI_0		1304
MX6Q_PAD_SD3_DAT2__USDHC3_DAT2			1305
MX6Q_PAD_SD3_DAT2__PCIE_CTRL_MUX_28		1306
MX6Q_PAD_SD3_DAT2__USBOH3_UH3_DFD_OUT_8		1307
MX6Q_PAD_SD3_DAT2__USBOH3_UH2_DFD_OUT_8		1308
MX6Q_PAD_SD3_DAT2__GPIO_7_6			1309
MX6Q_PAD_SD3_DAT2__MIPI_CORE_DPHY_IN_20		1310
MX6Q_PAD_SD3_DAT2__ANATOP_TESTI_1		1311
MX6Q_PAD_SD3_DAT3__USDHC3_DAT3			1312
MX6Q_PAD_SD3_DAT3__UART3_CTS			1313
MX6Q_PAD_SD3_DAT3__PCIE_CTRL_MUX_29		1314
MX6Q_PAD_SD3_DAT3__USBOH3_UH3_DFD_OUT_9		1315
MX6Q_PAD_SD3_DAT3__USBOH3_UH2_DFD_OUT_9		1316
MX6Q_PAD_SD3_DAT3__GPIO_7_7			1317
MX6Q_PAD_SD3_DAT3__MIPI_CORE_DPHY_IN_21		1318
MX6Q_PAD_SD3_DAT3__ANATOP_TESTI_2		1319
MX6Q_PAD_SD3_RST__USDHC3_RST			1320
MX6Q_PAD_SD3_RST__UART3_RTS			1321
MX6Q_PAD_SD3_RST__PCIE_CTRL_MUX_30		1322
MX6Q_PAD_SD3_RST__USBOH3_UH3_DFD_OUT_10		1323
MX6Q_PAD_SD3_RST__USBOH3_UH2_DFD_OUT_10		1324
MX6Q_PAD_SD3_RST__GPIO_7_8			1325
MX6Q_PAD_SD3_RST__MIPI_CORE_DPHY_IN_22		1326
MX6Q_PAD_SD3_RST__ANATOP_ANATOP_TESTI_3		1327
MX6Q_PAD_NANDF_CLE__RAWNAND_CLE			1328
MX6Q_PAD_NANDF_CLE__IPU2_SISG_4			1329
MX6Q_PAD_NANDF_CLE__PCIE_CTRL_MUX_31		1330
MX6Q_PAD_NANDF_CLE__USBOH3_UH3_DFD_OT11		1331
MX6Q_PAD_NANDF_CLE__USBOH3_UH2_DFD_OT11		1332
MX6Q_PAD_NANDF_CLE__GPIO_6_7			1333
MX6Q_PAD_NANDF_CLE__MIPI_CORE_DPHY_IN23		1334
MX6Q_PAD_NANDF_CLE__TPSMP_HTRANS_0		1335
MX6Q_PAD_NANDF_ALE__RAWNAND_ALE			1336
MX6Q_PAD_NANDF_ALE__USDHC4_RST			1337
MX6Q_PAD_NANDF_ALE__PCIE_CTRL_MUX_0		1338
MX6Q_PAD_NANDF_ALE__USBOH3_UH3_DFD_OT12		1339
MX6Q_PAD_NANDF_ALE__USBOH3_UH2_DFD_OT12		1340
MX6Q_PAD_NANDF_ALE__GPIO_6_8			1341
MX6Q_PAD_NANDF_ALE__MIPI_CR_DPHY_IN_24		1342
MX6Q_PAD_NANDF_ALE__TPSMP_HTRANS_1		1343
MX6Q_PAD_NANDF_WP_B__RAWNAND_RESETN		1344
MX6Q_PAD_NANDF_WP_B__IPU2_SISG_5		1345
MX6Q_PAD_NANDF_WP_B__PCIE_CTRL__MUX_1		1346
MX6Q_PAD_NANDF_WP_B__USBOH3_UH3_DFDOT13		1347
MX6Q_PAD_NANDF_WP_B__USBOH3_UH2_DFDOT13		1348
MX6Q_PAD_NANDF_WP_B__GPIO_6_9			1349
MX6Q_PAD_NANDF_WP_B__MIPI_CR_DPHY_OUT32		1350
MX6Q_PAD_NANDF_WP_B__PL301_PER1_HSIZE_0		1351
MX6Q_PAD_NANDF_RB0__RAWNAND_READY0		1352
MX6Q_PAD_NANDF_RB0__IPU2_DI0_PIN1		1353
MX6Q_PAD_NANDF_RB0__PCIE_CTRL_MUX_2		1354
MX6Q_PAD_NANDF_RB0__USBOH3_UH3_DFD_OT14		1355
MX6Q_PAD_NANDF_RB0__USBOH3_UH2_DFD_OT14		1356
MX6Q_PAD_NANDF_RB0__GPIO_6_10			1357
MX6Q_PAD_NANDF_RB0__MIPI_CR_DPHY_OUT_33		1358
MX6Q_PAD_NANDF_RB0__PL301_PER1_HSIZE_1		1359
MX6Q_PAD_NANDF_CS0__RAWNAND_CE0N		1360
MX6Q_PAD_NANDF_CS0__USBOH3_UH3_DFD_OT15		1361
MX6Q_PAD_NANDF_CS0__USBOH3_UH2_DFD_OT15		1362
MX6Q_PAD_NANDF_CS0__GPIO_6_11			1363
MX6Q_PAD_NANDF_CS0__PL301_PER1_HSIZE_2		1364
MX6Q_PAD_NANDF_CS1__RAWNAND_CE1N		1365
MX6Q_PAD_NANDF_CS1__USDHC4_VSELECT		1366
MX6Q_PAD_NANDF_CS1__USDHC3_VSELECT		1367
MX6Q_PAD_NANDF_CS1__PCIE_CTRL_MUX_3		1368
MX6Q_PAD_NANDF_CS1__GPIO_6_14			1369
MX6Q_PAD_NANDF_CS1__PL301_PER1_HRDYOUT		1370
MX6Q_PAD_NANDF_CS2__RAWNAND_CE2N		1371
MX6Q_PAD_NANDF_CS2__IPU1_SISG_0			1372
MX6Q_PAD_NANDF_CS2__ESAI1_TX0			1373
MX6Q_PAD_NANDF_CS2__WEIM_WEIM_CRE		1374
MX6Q_PAD_NANDF_CS2__CCM_CLKO2			1375
MX6Q_PAD_NANDF_CS2__GPIO_6_15			1376
MX6Q_PAD_NANDF_CS2__IPU2_SISG_0			1377
MX6Q_PAD_NANDF_CS3__RAWNAND_CE3N		1378
MX6Q_PAD_NANDF_CS3__IPU1_SISG_1			1379
MX6Q_PAD_NANDF_CS3__ESAI1_TX1			1380
MX6Q_PAD_NANDF_CS3__WEIM_WEIM_A_26		1381
MX6Q_PAD_NANDF_CS3__PCIE_CTRL_MUX_4		1382
MX6Q_PAD_NANDF_CS3__GPIO_6_16			1383
MX6Q_PAD_NANDF_CS3__IPU2_SISG_1			1384
MX6Q_PAD_NANDF_CS3__TPSMP_CLK			1385
MX6Q_PAD_SD4_CMD__USDHC4_CMD			1386
MX6Q_PAD_SD4_CMD__RAWNAND_RDN			1387
MX6Q_PAD_SD4_CMD__UART3_TXD			1388
MX6Q_PAD_SD4_CMD__PCIE_CTRL_MUX_5		1389
MX6Q_PAD_SD4_CMD__GPIO_7_9			1390
MX6Q_PAD_SD4_CMD__TPSMP_HDATA_DIR		1391
MX6Q_PAD_SD4_CLK__USDHC4_CLK			1392
MX6Q_PAD_SD4_CLK__RAWNAND_WRN			1393
MX6Q_PAD_SD4_CLK__UART3_RXD			1394
MX6Q_PAD_SD4_CLK__PCIE_CTRL_MUX_6		1395
MX6Q_PAD_SD4_CLK__GPIO_7_10			1396
MX6Q_PAD_NANDF_D0__RAWNAND_D0			1397
MX6Q_PAD_NANDF_D0__USDHC1_DAT4			1398
MX6Q_PAD_NANDF_D0__GPU3D_GPU_DBG_OUT_0		1399
MX6Q_PAD_NANDF_D0__USBOH3_UH2_DFD_OUT16		1400
MX6Q_PAD_NANDF_D0__USBOH3_UH3_DFD_OUT16		1401
MX6Q_PAD_NANDF_D0__GPIO_2_0			1402
MX6Q_PAD_NANDF_D0__IPU1_IPU_DIAG_BUS_0		1403
MX6Q_PAD_NANDF_D0__IPU2_IPU_DIAG_BUS_0		1404
MX6Q_PAD_NANDF_D1__RAWNAND_D1			1405
MX6Q_PAD_NANDF_D1__USDHC1_DAT5			1406
MX6Q_PAD_NANDF_D1__GPU3D_GPU_DEBUG_OUT1		1407
MX6Q_PAD_NANDF_D1__USBOH3_UH2_DFD_OUT17		1408
MX6Q_PAD_NANDF_D1__USBOH3_UH3_DFD_OUT17		1409
MX6Q_PAD_NANDF_D1__GPIO_2_1			1410
MX6Q_PAD_NANDF_D1__IPU1_IPU_DIAG_BUS_1		1411
MX6Q_PAD_NANDF_D1__IPU2_IPU_DIAG_BUS_1		1412
MX6Q_PAD_NANDF_D2__RAWNAND_D2			1413
MX6Q_PAD_NANDF_D2__USDHC1_DAT6			1414
MX6Q_PAD_NANDF_D2__GPU3D_GPU_DBG_OUT_2		1415
MX6Q_PAD_NANDF_D2__USBOH3_UH2_DFD_OUT18		1416
MX6Q_PAD_NANDF_D2__USBOH3_UH3_DFD_OUT18		1417
MX6Q_PAD_NANDF_D2__GPIO_2_2			1418
MX6Q_PAD_NANDF_D2__IPU1_IPU_DIAG_BUS_2		1419
MX6Q_PAD_NANDF_D2__IPU2_IPU_DIAG_BUS_2		1420
MX6Q_PAD_NANDF_D3__RAWNAND_D3			1421
MX6Q_PAD_NANDF_D3__USDHC1_DAT7			1422
MX6Q_PAD_NANDF_D3__GPU3D_GPU_DBG_OUT_3		1423
MX6Q_PAD_NANDF_D3__USBOH3_UH2_DFD_OUT19		1424
MX6Q_PAD_NANDF_D3__USBOH3_UH3_DFD_OUT19		1425
MX6Q_PAD_NANDF_D3__GPIO_2_3			1426
MX6Q_PAD_NANDF_D3__IPU1_IPU_DIAG_BUS_3		1427
MX6Q_PAD_NANDF_D3__IPU2_IPU_DIAG_BUS_3		1428
MX6Q_PAD_NANDF_D4__RAWNAND_D4			1429
MX6Q_PAD_NANDF_D4__USDHC2_DAT4			1430
MX6Q_PAD_NANDF_D4__GPU3D_GPU_DBG_OUT_4		1431
MX6Q_PAD_NANDF_D4__USBOH3_UH2_DFD_OUT20		1432
MX6Q_PAD_NANDF_D4__USBOH3_UH3_DFD_OUT20		1433
MX6Q_PAD_NANDF_D4__GPIO_2_4			1434
MX6Q_PAD_NANDF_D4__IPU1_IPU_DIAG_BUS_4		1435
MX6Q_PAD_NANDF_D4__IPU2_IPU_DIAG_BUS_4		1436
MX6Q_PAD_NANDF_D5__RAWNAND_D5			1437
MX6Q_PAD_NANDF_D5__USDHC2_DAT5			1438
MX6Q_PAD_NANDF_D5__GPU3D_GPU_DBG_OUT_5		1439
MX6Q_PAD_NANDF_D5__USBOH3_UH2_DFD_OUT21		1440
MX6Q_PAD_NANDF_D5__USBOH3_UH3_DFD_OUT21		1441
MX6Q_PAD_NANDF_D5__GPIO_2_5			1442
MX6Q_PAD_NANDF_D5__IPU1_IPU_DIAG_BUS_5		1443
MX6Q_PAD_NANDF_D5__IPU2_IPU_DIAG_BUS_5		1444
MX6Q_PAD_NANDF_D6__RAWNAND_D6			1445
MX6Q_PAD_NANDF_D6__USDHC2_DAT6			1446
MX6Q_PAD_NANDF_D6__GPU3D_GPU_DBG_OUT_6		1447
MX6Q_PAD_NANDF_D6__USBOH3_UH2_DFD_OUT22		1448
MX6Q_PAD_NANDF_D6__USBOH3_UH3_DFD_OUT22		1449
MX6Q_PAD_NANDF_D6__GPIO_2_6			1450
MX6Q_PAD_NANDF_D6__IPU1_IPU_DIAG_BUS_6		1451
MX6Q_PAD_NANDF_D6__IPU2_IPU_DIAG_BUS_6		1452
MX6Q_PAD_NANDF_D7__RAWNAND_D7			1453
MX6Q_PAD_NANDF_D7__USDHC2_DAT7			1454
MX6Q_PAD_NANDF_D7__GPU3D_GPU_DBG_OUT_7		1455
MX6Q_PAD_NANDF_D7__USBOH3_UH2_DFD_OUT23		1456
MX6Q_PAD_NANDF_D7__USBOH3_UH3_DFD_OUT23		1457
MX6Q_PAD_NANDF_D7__GPIO_2_7			1458
MX6Q_PAD_NANDF_D7__IPU1_IPU_DIAG_BUS_7		1459
MX6Q_PAD_NANDF_D7__IPU2_IPU_DIAG_BUS_7		1460
MX6Q_PAD_SD4_DAT0__RAWNAND_D8			1461
MX6Q_PAD_SD4_DAT0__USDHC4_DAT0			1462
MX6Q_PAD_SD4_DAT0__RAWNAND_DQS			1463
MX6Q_PAD_SD4_DAT0__USBOH3_UH2_DFD_OUT24		1464
MX6Q_PAD_SD4_DAT0__USBOH3_UH3_DFD_OUT24		1465
MX6Q_PAD_SD4_DAT0__GPIO_2_8			1466
MX6Q_PAD_SD4_DAT0__IPU1_IPU_DIAG_BUS_8		1467
MX6Q_PAD_SD4_DAT0__IPU2_IPU_DIAG_BUS_8		1468
MX6Q_PAD_SD4_DAT1__RAWNAND_D9			1469
MX6Q_PAD_SD4_DAT1__USDHC4_DAT1			1470
MX6Q_PAD_SD4_DAT1__PWM3_PWMO			1471
MX6Q_PAD_SD4_DAT1__USBOH3_UH2_DFD_OUT25		1472
MX6Q_PAD_SD4_DAT1__USBOH3_UH3_DFD_OUT25		1473
MX6Q_PAD_SD4_DAT1__GPIO_2_9			1474
MX6Q_PAD_SD4_DAT1__IPU1_IPU_DIAG_BUS_9		1475
MX6Q_PAD_SD4_DAT1__IPU2_IPU_DIAG_BUS_9		1476
MX6Q_PAD_SD4_DAT2__RAWNAND_D10			1477
MX6Q_PAD_SD4_DAT2__USDHC4_DAT2			1478
MX6Q_PAD_SD4_DAT2__PWM4_PWMO			1479
MX6Q_PAD_SD4_DAT2__USBOH3_UH2_DFD_OUT26		1480
MX6Q_PAD_SD4_DAT2__USBOH3_UH3_DFD_OUT26		1481
MX6Q_PAD_SD4_DAT2__GPIO_2_10			1482
MX6Q_PAD_SD4_DAT2__IPU1_IPU_DIAG_BUS_10		1483
MX6Q_PAD_SD4_DAT2__IPU2_IPU_DIAG_BUS_10		1484
MX6Q_PAD_SD4_DAT3__RAWNAND_D11			1485
MX6Q_PAD_SD4_DAT3__USDHC4_DAT3			1486
MX6Q_PAD_SD4_DAT3__USBOH3_UH2_DFD_OUT27		1487
MX6Q_PAD_SD4_DAT3__USBOH3_UH3_DFD_OUT27		1488
MX6Q_PAD_SD4_DAT3__GPIO_2_11			1489
MX6Q_PAD_SD4_DAT3__IPU1_IPU_DIAG_BUS_11		1490
MX6Q_PAD_SD4_DAT3__IPU2_IPU_DIAG_BUS_11		1491
MX6Q_PAD_SD4_DAT4__RAWNAND_D12			1492
MX6Q_PAD_SD4_DAT4__USDHC4_DAT4			1493
MX6Q_PAD_SD4_DAT4__UART2_RXD			1494
MX6Q_PAD_SD4_DAT4__USBOH3_UH2_DFD_OUT28		1495
MX6Q_PAD_SD4_DAT4__USBOH3_UH3_DFD_OUT28		1496
MX6Q_PAD_SD4_DAT4__GPIO_2_12			1497
MX6Q_PAD_SD4_DAT4__IPU1_IPU_DIAG_BUS_12		1498
MX6Q_PAD_SD4_DAT4__IPU2_IPU_DIAG_BUS_12		1499
MX6Q_PAD_SD4_DAT5__RAWNAND_D13			1500
MX6Q_PAD_SD4_DAT5__USDHC4_DAT5			1501
MX6Q_PAD_SD4_DAT5__UART2_RTS			1502
MX6Q_PAD_SD4_DAT5__USBOH3_UH2_DFD_OUT29		1503
MX6Q_PAD_SD4_DAT5__USBOH3_UH3_DFD_OUT29		1504
MX6Q_PAD_SD4_DAT5__GPIO_2_13			1505
MX6Q_PAD_SD4_DAT5__IPU1_IPU_DIAG_BUS_13		1506
MX6Q_PAD_SD4_DAT5__IPU2_IPU_DIAG_BUS_13		1507
MX6Q_PAD_SD4_DAT6__RAWNAND_D14			1508
MX6Q_PAD_SD4_DAT6__USDHC4_DAT6			1509
MX6Q_PAD_SD4_DAT6__UART2_CTS			1510
MX6Q_PAD_SD4_DAT6__USBOH3_UH2_DFD_OUT30		1511
MX6Q_PAD_SD4_DAT6__USBOH3_UH3_DFD_OUT30		1512
MX6Q_PAD_SD4_DAT6__GPIO_2_14			1513
MX6Q_PAD_SD4_DAT6__IPU1_IPU_DIAG_BUS_14		1514
MX6Q_PAD_SD4_DAT6__IPU2_IPU_DIAG_BUS_14		1515
MX6Q_PAD_SD4_DAT7__RAWNAND_D15			1516
MX6Q_PAD_SD4_DAT7__USDHC4_DAT7			1517
MX6Q_PAD_SD4_DAT7__UART2_TXD			1518
MX6Q_PAD_SD4_DAT7__USBOH3_UH2_DFD_OUT31		1519
MX6Q_PAD_SD4_DAT7__USBOH3_UH3_DFD_OUT31		1520
MX6Q_PAD_SD4_DAT7__GPIO_2_15			1521
MX6Q_PAD_SD4_DAT7__IPU1_IPU_DIAG_BUS_15		1522
MX6Q_PAD_SD4_DAT7__IPU2_IPU_DIAG_BUS_15		1523
MX6Q_PAD_SD1_DAT1__USDHC1_DAT1			1524
MX6Q_PAD_SD1_DAT1__ECSPI5_SS0			1525
MX6Q_PAD_SD1_DAT1__PWM3_PWMO			1526
MX6Q_PAD_SD1_DAT1__GPT_CAPIN2			1527
MX6Q_PAD_SD1_DAT1__PCIE_CTRL_MUX_7		1528
MX6Q_PAD_SD1_DAT1__GPIO_1_17			1529
MX6Q_PAD_SD1_DAT1__HDMI_TX_OPHYDTB_0		1530
MX6Q_PAD_SD1_DAT1__ANATOP_TESTO_8		1531
MX6Q_PAD_SD1_DAT0__USDHC1_DAT0			1532
MX6Q_PAD_SD1_DAT0__ECSPI5_MISO			1533
MX6Q_PAD_SD1_DAT0__CAAM_WRAP_RNG_OSCOBS		1534
MX6Q_PAD_SD1_DAT0__GPT_CAPIN1			1535
MX6Q_PAD_SD1_DAT0__PCIE_CTRL_MUX_8		1536
MX6Q_PAD_SD1_DAT0__GPIO_1_16			1537
MX6Q_PAD_SD1_DAT0__HDMI_TX_OPHYDTB_1		1538
MX6Q_PAD_SD1_DAT0__ANATOP_TESTO_7		1539
MX6Q_PAD_SD1_DAT3__USDHC1_DAT3			1540
MX6Q_PAD_SD1_DAT3__ECSPI5_SS2			1541
MX6Q_PAD_SD1_DAT3__GPT_CMPOUT3			1542
MX6Q_PAD_SD1_DAT3__PWM1_PWMO			1543
MX6Q_PAD_SD1_DAT3__WDOG2_WDOG_B			1544
MX6Q_PAD_SD1_DAT3__GPIO_1_21			1545
MX6Q_PAD_SD1_DAT3__WDOG2_WDOG_RST_B_DEB		1546
MX6Q_PAD_SD1_DAT3__ANATOP_TESTO_6		1547
MX6Q_PAD_SD1_CMD__USDHC1_CMD			1548
MX6Q_PAD_SD1_CMD__ECSPI5_MOSI			1549
MX6Q_PAD_SD1_CMD__PWM4_PWMO			1550
MX6Q_PAD_SD1_CMD__GPT_CMPOUT1			1551
MX6Q_PAD_SD1_CMD__GPIO_1_18			1552
MX6Q_PAD_SD1_CMD__ANATOP_TESTO_5		1553
MX6Q_PAD_SD1_DAT2__USDHC1_DAT2			1554
MX6Q_PAD_SD1_DAT2__ECSPI5_SS1			1555
MX6Q_PAD_SD1_DAT2__GPT_CMPOUT2			1556
MX6Q_PAD_SD1_DAT2__PWM2_PWMO			1557
MX6Q_PAD_SD1_DAT2__WDOG1_WDOG_B			1558
MX6Q_PAD_SD1_DAT2__GPIO_1_19			1559
MX6Q_PAD_SD1_DAT2__WDOG1_WDOG_RST_B_DEB		1560
MX6Q_PAD_SD1_DAT2__ANATOP_TESTO_4		1561
MX6Q_PAD_SD1_CLK__USDHC1_CLK			1562
MX6Q_PAD_SD1_CLK__ECSPI5_SCLK			1563
MX6Q_PAD_SD1_CLK__OSC32K_32K_OUT		1564
MX6Q_PAD_SD1_CLK__GPT_CLKIN			1565
MX6Q_PAD_SD1_CLK__GPIO_1_20			1566
MX6Q_PAD_SD1_CLK__PHY_DTB_0			1567
MX6Q_PAD_SD1_CLK__SATA_PHY_DTB_0		1568
MX6Q_PAD_SD2_CLK__USDHC2_CLK			1569
MX6Q_PAD_SD2_CLK__ECSPI5_SCLK			1570
MX6Q_PAD_SD2_CLK__KPP_COL_5			1571
MX6Q_PAD_SD2_CLK__AUDMUX_AUD4_RXFS		1572
MX6Q_PAD_SD2_CLK__PCIE_CTRL_MUX_9		1573
MX6Q_PAD_SD2_CLK__GPIO_1_10			1574
MX6Q_PAD_SD2_CLK__PHY_DTB_1			1575
MX6Q_PAD_SD2_CLK__SATA_PHY_DTB_1		1576
MX6Q_PAD_SD2_CMD__USDHC2_CMD			1577
MX6Q_PAD_SD2_CMD__ECSPI5_MOSI			1578
MX6Q_PAD_SD2_CMD__KPP_ROW_5			1579
MX6Q_PAD_SD2_CMD__AUDMUX_AUD4_RXC		1580
MX6Q_PAD_SD2_CMD__PCIE_CTRL_MUX_10		1581
MX6Q_PAD_SD2_CMD__GPIO_1_11			1582
MX6Q_PAD_SD2_DAT3__USDHC2_DAT3			1583
MX6Q_PAD_SD2_DAT3__ECSPI5_SS3			1584
MX6Q_PAD_SD2_DAT3__KPP_COL_6			1585
MX6Q_PAD_SD2_DAT3__AUDMUX_AUD4_TXC		1586
MX6Q_PAD_SD2_DAT3__PCIE_CTRL_MUX_11		1587
MX6Q_PAD_SD2_DAT3__GPIO_1_12			1588
MX6Q_PAD_SD2_DAT3__SJC_DONE			1589
MX6Q_PAD_SD2_DAT3__ANATOP_TESTO_3		1590
MX6Q_PAD_ENET_RX_ER__ANATOP_USBOTG_ID		1591
MX6Q_PAD_GPIO_1__ANATOP_USBOTG_ID		1592
