#
#
#   These data are based on the CRTC parameters in
#
#       VIA Integration Graphics Chip
#       (C) 2004 VIA Technologies Inc.
#

#
#   640x480, 60 Hz, Non-Interlaced (25.175 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      640     480
#   Scan Frequency      31.469 kHz  59.94 Hz
#   Sync Width      3.813 us    0.064 ms
#               12 chars    2 lines
#   Front Porch     0.636 us    0.318  ms
#               2 chars     10 lines
#   Back Porch      1.907 us    1.048  ms
#               6 chars     33 lines
#   Active Time     25.422 us   15.253 ms
#               80 chars    480 lines
#   Blank Time      6.356 us    1.430 ms
#               20 chars    45 lines
#   Polarity        negative    negative
#

mode "640x480-60"
# D: 25.175 MHz, H: 31.469 kHz, V: 59.94 Hz
    geometry 640 480 640 480 32
    timings 39722 48 16 33 10 96 2 endmode mode "480x640-60"
# D: 24.823 MHz, H: 39.780 kHz, V: 60.00 Hz
    geometry 480 640 480 640 32 timings 39722 72 24 19 1 48 3 endmode
#
#   640x480, 75 Hz, Non-Interlaced (31.50 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      640     480
#   Scan Frequency      37.500 kHz  75.00 Hz
#   Sync Width      2.032 us    0.080 ms
#               8 chars     3 lines
#   Front Porch     0.508 us    0.027 ms
#               2 chars     1 lines
#   Back Porch      3.810 us    0.427 ms
#               15 chars    16 lines
#   Active Time     20.317 us   12.800 ms
#               80 chars    480 lines
#   Blank Time      6.349 us    0.533 ms
#               25 chars    20 lines
#   Polarity        negative    negative
#
    mode "640x480-75"
# D: 31.50 MHz, H: 37.500 kHz, V: 75.00 Hz
    geometry 640 480 640 480 32 timings 31747 120 16 16 1 64 3 endmode
#
#   640x480, 85 Hz, Non-Interlaced (36.000 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      640     480
#   Scan Frequency  43.269 kHz  85.00 Hz
#   Sync Width      1.556 us    0.069 ms
#               7 chars     3 lines
#   Front Porch     1.556 us    0.023 ms
#               7 chars     1 lines
#   Back Porch      2.222 us    0.578 ms
#               10 chars    25 lines
#   Active Time     17.778 us   11.093 ms
#               80 chars    480 lines
#   Blank Time      5.333 us    0.670 ms
#               24 chars    29 lines
#   Polarity        negative    negative
#
    mode "640x480-85"
# D: 36.000 MHz, H: 43.269 kHz, V: 85.00 Hz
    geometry 640 480 640 480 32 timings 27777 80 56 25 1 56 3 endmode
#
#   640x480, 100 Hz, Non-Interlaced (43.163 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      640     480
#   Scan Frequency      50.900 kHz  100.00 Hz
#   Sync Width      1.483 us    0.058 ms
#               8 chars     3 lines
#   Front Porch     0.927 us    0.019 ms
#               5 chars     1 lines
#   Back Porch      2.409 us    0.475 ms
#               13 chars    25 lines
#   Active Time     14.827 us   9.430 ms
#               80 chars    480 lines
#   Blank Time      4.819 us    0.570 ms
#               26 chars    29 lines
#   Polarity        positive    positive
#
    mode "640x480-100"
# D: 43.163 MHz, H: 50.900 kHz, V: 100.00 Hz
    geometry 640 480 640 480 32 timings 23168 104 40 25 1 64 3 endmode
#
#   640x480, 120 Hz, Non-Interlaced (52.406 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      640     480
#   Scan Frequency      61.800 kHz  120.00 Hz
#   Sync Width      1.221 us    0.048 ms
#               8 chars         3 lines
#   Front Porch     0.763 us    0.016 ms
#               5 chars     1 lines
#   Back Porch      1.984 us    0.496 ms
#               13 chars    31 lines
#   Active Time     12.212 us   7.767 ms
#               80 chars    480 lines
#   Blank Time      3.969 us    0.566 ms
#               26 chars    35 lines
#   Polarity        positive    positive
#
    mode "640x480-120"
# D: 52.406 MHz, H: 61.800 kHz, V: 120.00 Hz
    geometry 640 480 640 480 32 timings 19081 104 40 31 1 64 3 endmode
#
#   720x480, 60 Hz, Non-Interlaced (26.880 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      720     480
#   Scan Frequency      30.000 kHz  60.241 Hz
#   Sync Width      2.679 us    0.099 ms
#               9 chars     3 lines
#   Front Porch     0.595 us    0.033 ms
#               2 chars     1 lines
#   Back Porch      3.274 us    0.462 ms
#               11 chars    14 lines
#   Active Time     26.786 us   16.000 ms
#               90 chars    480 lines
#   Blank Time      6.548 us    0.600 ms
#               22 chars    18 lines
#   Polarity        positive    positive
#
    mode "720x480-60"
# D: 26.880 MHz, H: 30.000 kHz, V: 60.24 Hz
    geometry 720 480 720 480 32 timings 37202 88 16 14 1 72 3 endmode
#
#   800x480, 60 Hz, Non-Interlaced (29.581 MHz dotclock)
#
#               Horizontal    Vertical
#   Resolution      800         480
#   Scan Frequency  29.892 kHz  60.00 Hz
#   Sync Width      2.704 us    100.604 us
#                   10 chars    3 lines
#   Front Porch     0.541 us    33.535 us
#                   2 chars     1 lines
#   Back Porch      3.245 us    435.949 us
#                   12 chars    13 lines
#   Active Time     27.044 us   16.097 ms
#                   100 chars   480 lines
#   Blank Time      6.491 us    0.570 ms
#                   24 chars    17 lines
#   Polarity        positive    positive
#
    mode "800x480-60"
# D: 29.500 MHz, H: 29.738 kHz, V: 60.00 Hz
    geometry 800 480 800 480 32 timings 33805 96 24 10 3 72 7 endmode
#
#   720x576, 60 Hz, Non-Interlaced (32.668 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      720     576
#   Scan Frequency      35.820 kHz  60.00 Hz
#   Sync Width      2.204 us    0.083 ms
#               9 chars     3 lines
#   Front Porch     0.735 us    0.027 ms
#               3 chars     1 lines
#   Back Porch      2.939 us    0.459 ms
#               12 chars    17 lines
#   Active Time     22.040 us   16.080 ms
#               90 chars    476 lines
#   Blank Time      5.877 us    0.586 ms
#               24 chars    21 lines
#   Polarity        positive    positive
#
    mode "720x576-60"
# D: 32.668 MHz, H: 35.820 kHz, V: 60.00 Hz
    geometry 720 576 720 576 32 timings 30611 96 24 17 1 72 3 endmode
#
#   800x600, 60 Hz, Non-Interlaced (40.00 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      800     600
#   Scan Frequency      37.879 kHz  60.32 Hz
#   Sync Width      3.200 us    0.106 ms
#               16 chars    4 lines
#   Front Porch     1.000 us    0.026 ms
#               5 chars     1 lines
#   Back Porch      2.200 us    0.607 ms
#               11 chars    23 lines
#   Active Time     20.000 us   15.840 ms
#               100 chars   600 lines
#   Blank Time      6.400 us    0.739 ms
#               32 chars    28 lines
#   Polarity        positive    positive
#
    mode "800x600-60"
# D: 40.00 MHz, H: 37.879 kHz, V: 60.32 Hz
    geometry 800 600 800 600 32
    timings 25000 88 40 23 1 128 4 hsync high vsync high endmode
#
#   800x600, 75 Hz, Non-Interlaced (49.50 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      800     600
#   Scan Frequency      46.875 kHz  75.00 Hz
#   Sync Width      1.616 us    0.064 ms
#               10 chars    3 lines
#   Front Porch     0.323 us    0.021 ms
#               2 chars     1 lines
#   Back Porch      3.232 us    0.448 ms
#               20 chars    21 lines
#   Active Time     16.162 us   12.800 ms
#               100 chars   600 lines
#   Blank Time      5.172 us    0.533 ms
#               32 chars    25 lines
#   Polarity        positive    positive
#
    mode "800x600-75"
# D: 49.50 MHz, H: 46.875 kHz, V: 75.00 Hz
    geometry 800 600 800 600 32
    timings 20203 160 16 21 1 80 3 hsync high vsync high endmode
#
#   800x600, 85 Hz, Non-Interlaced (56.25 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      800     600
#   Scan Frequency      53.674 kHz  85.061 Hz
#   Sync Width      1.138 us    0.056 ms
#               8 chars     3 lines
#   Front Porch     0.569 us    0.019 ms
#               4 chars     1 lines
#   Back Porch      2.702 us    0.503 ms
#               19 chars    27 lines
#   Active Time     14.222 us   11.179 ms
#               100 chars   600 lines
#   Blank Time      4.409 us    0.578 ms
#               31 chars    31 lines
#   Polarity        positive    positive
#
    mode "800x600-85"
# D: 56.25 MHz, H: 53.674 kHz, V: 85.061 Hz
    geometry 800 600 800 600 32
    timings 17777 152 32 27 1 64 3 hsync high vsync high endmode
#
#   800x600, 100 Hz, Non-Interlaced (67.50 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      800     600
#   Scan Frequency      62.500 kHz  100.00 Hz
#   Sync Width      0.948 us    0.064 ms
#               8 chars     4 lines
#   Front Porch     0.000 us    0.112 ms
#               0 chars     7 lines
#   Back Porch      3.200 us    0.224 ms
#               27 chars    14 lines
#   Active Time     11.852 us   9.600 ms
#               100 chars   600 lines
#   Blank Time      4.148 us    0.400 ms
#               35 chars    25 lines
#   Polarity        positive    positive
#
    mode "800x600-100"
# D: 67.50 MHz, H: 62.500 kHz, V: 100.00 Hz
    geometry 800 600 800 600 32
    timings 14667 216 0 14 7 64 4 hsync high vsync high endmode
#
#   800x600, 120 Hz, Non-Interlaced (83.950 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      800     600
#   Scan Frequency  77.160 kHz  120.00 Hz
#   Sync Width      1.048 us    0.039 ms
#               11 chars    3 lines
#   Front Porch     0.667 us    0.013 ms
#               7 chars     1 lines
#   Back Porch      1.715 us    0.507 ms
#               18 chars    39 lines
#   Active Time     9.529 us    7.776 ms
#               100 chars   600 lines
#   Blank Time      3.431 us    0.557 ms
#               36 chars    43 lines
#   Polarity        positive    positive
#
    mode "800x600-120"
# D: 83.950 MHz, H: 77.160 kHz, V: 120.00 Hz
    geometry 800 600 800 600 32
    timings 11912 144 56 39 1 88 3 hsync high vsync high endmode
#
#   848x480, 60 Hz, Non-Interlaced (31.490 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      848     480
#   Scan Frequency  29.820 kHz  60.00 Hz
#   Sync Width      2.795 us    0.099 ms
#               11 chars    3 lines
#   Front Porch     0.508 us    0.033 ms
#               2 chars     1 lines
#   Back Porch      3.303 us    0.429 ms
#               13 chars    13 lines
#   Active Time     26.929 us   16.097 ms
#               106 chars   480 lines
#   Blank Time      6.605 us    0.570 ms
#               26 chars    17 lines
#   Polarity        positive    positive
#
    mode "848x480-60"
# D: 31.500 MHz, H: 29.830 kHz, V: 60.00 Hz
    geometry 848 480 848 480 32
    timings 31746 104 24 12 3 80 5 hsync high vsync high endmode
#
#   856x480, 60 Hz, Non-Interlaced (31.728 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      856     480
#   Scan Frequency  29.820 kHz  60.00 Hz
#   Sync Width      2.774 us    0.099 ms
#               11 chars    3 lines
#   Front Porch     0.504 us    0.033 ms
#               2 chars     1 lines
#   Back Porch      3.728 us    0.429 ms
#               13 chars    13 lines
#   Active Time     26.979 us   16.097 ms
#               107 chars   480 lines
#   Blank Time      6.556 us    0.570 ms
#               26 chars    17 lines
#   Polarity        positive    positive
#
    mode "856x480-60"
# D: 31.728 MHz, H: 29.820 kHz, V: 60.00 Hz
    geometry 856 480 856 480 32
    timings 31518 104 16 13 1 88 3
    hsync high vsync high endmode mode "960x600-60"
# D: 45.250 MHz, H: 37.212 kHz, V: 60.00 Hz
    geometry 960 600 960 600 32 timings 22099 128 32 15 3 96 6 endmode
#
#   1000x600, 60 Hz, Non-Interlaced (48.068 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1000     600
#   Scan Frequency  37.320 kHz  60.00 Hz
#   Sync Width      2.164 us    0.080 ms
#               13 chars    3 lines
#   Front Porch     0.832 us    0.027 ms
#               5 chars     1 lines
#   Back Porch      2.996 us    0.483 ms
#               18 chars    18 lines
#   Active Time     20.804 us   16.077 ms
#               125 chars   600 lines
#   Blank Time      5.991 us    0.589 ms
#               36 chars    22 lines
#   Polarity        negative    positive
#
    mode "1000x600-60"
# D: 48.068 MHz, H: 37.320 kHz, V: 60.00 Hz
    geometry 1000 600 1000 600 32
    timings 20834 144 40 18 1 104 3 endmode mode "1024x576-60"
# D: 46.996 MHz, H: 35.820 kHz, V: 60.00 Hz
    geometry 1024 576 1024 576 32
    timings 21278 144 40 17 1 104 3 endmode mode "1024x600-60"
# D: 48.964 MHz, H: 37.320 kHz, V: 60.00 Hz
    geometry 1024 600 1024 600 32
    timings 20461 144 40 18 1 104 3 endmode mode "1088x612-60"
# D: 52.952 MHz, H: 38.040 kHz, V: 60.00 Hz
    geometry 1088 612 1088 612 32 timings 18877 152 48 16 3 104 5 endmode
#
#   1024x512, 60 Hz, Non-Interlaced (41.291 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1024    512
#   Scan Frequency  31.860 kHz  60.00 Hz
#   Sync Width      2.519 us    0.094 ms
#               13 chars    3 lines
#   Front Porch     0.775 us    0.031 ms
#               4 chars     1 lines
#   Back Porch      3.294 us    0.465 ms
#               17 chars    15 lines
#   Active Time     24.800 us   16.070 ms
#               128 chars   512 lines
#   Blank Time      6.587 us    0.596 ms
#               34 chars    19 lines
#   Polarity        positive    positive
#
    mode "1024x512-60"
# D: 41.291 MHz, H: 31.860 kHz, V: 60.00 Hz
    geometry 1024 512 1024 512 32
    timings 24218 126 32 15 1 104 3 hsync high vsync high endmode
#
#   1024x600, 60 Hz, Non-Interlaced (48.875 MHz dotclock)
#
#                     Horizontal  Vertical
#   Resolution          1024        768
#   Scan Frequency      37.252 kHz  60.00 Hz
#   Sync Width          2.128 us    80.532us
#                       13 chars    3 lines
#   Front Porch        0.818 us     26.844 us
#                       5 chars     1 lines
#   Back Porch          2.946 us    483.192 us
#                       18 chars    18 lines
#   Active Time         20.951 us   16.697 ms
#                       128 chars   622 lines
#   Blank Time          5.893 us    0.591 ms
#                       36 chars    22 lines
#   Polarity            negative    positive
#
#mode "1024x600-60"
#     # D: 48.875 MHz, H: 37.252 kHz, V: 60.00 Hz
#     geometry 1024 600 1024 600 32
#    timings 20460  144 40 18 1 104  3
# endmode
#
#   1024x768, 60 Hz, Non-Interlaced (65.00 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1024        768
#   Scan Frequency      48.363 kHz  60.00 Hz
#   Sync Width      2.092 us    0.124 ms
#               17 chars    6 lines
#   Front Porch     0.369 us    0.062 ms
#               3 chars     3 lines
#   Back Porch      2.462 us    0.601 ms
#               20 chars    29 lines
#   Active Time     15.754 us   15.880 ms
#               128 chars   768 lines
#   Blank Time      4.923 us    0.786 ms
#               40 chars    38 lines
#   Polarity        negative    negative
#
    mode "1024x768-60"
# D: 65.00 MHz, H: 48.363 kHz, V: 60.00 Hz
    geometry 1024 768 1024 768 32 timings 15385 160 24 29 3 136 6 endmode
#
#   1024x768, 75 Hz, Non-Interlaced (78.75 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1024        768
#   Scan Frequency      60.023 kHz  75.03 Hz
#   Sync Width      1.219 us    0.050 ms
#               12 chars    3 lines
#   Front Porch     0.203 us    0.017 ms
#               2 chars     1 lines
#   Back Porch      2.235 us    0.466 ms
#               22 chars    28 lines
#   Active Time     13.003 us   12.795 ms
#               128 chars   768 lines
#   Blank Time      3.657 us    0.533 ms
#               36 chars    32 lines
#   Polarity        positive    positive
#
    mode "1024x768-75"
# D: 78.75 MHz, H: 60.023 kHz, V: 75.03 Hz
    geometry 1024 768 1024 768 32
    timings 12699 176 16 28 1 96 3 hsync high vsync high endmode
#
#   1024x768, 85 Hz, Non-Interlaced (94.50 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1024        768
#   Scan Frequency  68.677 kHz  85.00 Hz
#   Sync Width      1.016 us    0.044 ms
#               12 chars    3 lines
#   Front Porch     0.508 us    0.015 ms
#               6 chars     1 lines
#   Back Porch      2.201 us    0.524 ms
#               26 chars    36 lines
#   Active Time     10.836 us   11.183 ms
#               128 chars   768 lines
#   Blank Time      3.725 us    0.582 ms
#               44 chars    40 lines
#   Polarity        positive    positive
#
    mode "1024x768-85"
# D: 94.50 MHz, H: 68.677 kHz, V: 85.00 Hz
    geometry 1024 768 1024 768 32
    timings 10582 208 48 36 1 96 3 hsync high vsync high endmode
#
#   1024x768, 100 Hz, Non-Interlaced (110.0 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1024        768
#   Scan Frequency      79.023 kHz  99.78 Hz
#   Sync Width      0.800 us    0.101 ms
#               11 chars    8 lines
#   Front Porch     0.000 us    0.000 ms
#               0 chars     0 lines
#   Back Porch      2.545 us    0.202 ms
#               35 chars    16 lines
#   Active Time     9.309 us    9.719 ms
#               128 chars   768 lines
#   Blank Time      3.345 us    0.304 ms
#               46 chars    24 lines
#   Polarity        negative    negative
#
    mode "1024x768-100"
# D: 113.3 MHz, H: 79.023 kHz, V: 99.78 Hz
    geometry 1024 768 1024 768 32
    timings 8825 280 0 16 0 88 8 endmode mode "1152x720-60"
# D: 66.750 MHz, H: 44.859 kHz, V: 60.00 Hz
    geometry 1152 720 1152 720 32 timings 14981 168 56 19 3 112 6 endmode
#
#   1152x864, 75 Hz, Non-Interlaced (110.0 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1152        864
#   Scan Frequency      75.137 kHz  74.99 Hz
#   Sync Width      1.309 us    0.106 ms
#               18 chars    8 lines
#   Front Porch     0.245 us    0.599 ms
#               3 chars     45 lines
#   Back Porch      1.282 us    1.132 ms
#               18 chars    85 lines
#   Active Time     10.473 us   11.499 ms
#               144 chars   864 lines
#   Blank Time      2.836 us    1.837 ms
#               39 chars    138 lines
#   Polarity        positive    positive
#
    mode "1152x864-75"
# D: 110.0 MHz, H: 75.137 kHz, V: 74.99 Hz
    geometry 1152 864 1152 864 32
    timings 9259 144 24 85 45 144 8
    hsync high vsync high endmode mode "1200x720-60"
# D: 70.184 MHz, H: 44.760 kHz, V: 60.00 Hz
    geometry 1200 720 1200 720 32
    timings 14253 184 28 22 1 128 3 endmode mode "1280x600-60"
# D: 61.503 MHz, H: 37.320 kHz, V: 60.00 Hz
    geometry 1280 600 1280 600 32
    timings 16260 184 28 18 1 128 3 endmode mode "1280x720-50"
# D: 60.466 MHz, H: 37.050 kHz, V: 50.00 Hz
    geometry 1280 720 1280 720 32
    timings 16538 176 48 17 1 128 3 endmode mode "1280x768-50"
# D: 65.178 MHz, H: 39.550 kHz, V: 50.00 Hz
    geometry 1280 768 1280 768 32 timings 15342 184 28 19 1 128 3 endmode
#
#   1280x768, 60 Hz, Non-Interlaced (80.136 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280    768
#   Scan Frequency  47.700 kHz  60.00 Hz
#   Sync Width      1.697 us    0.063 ms
#               17 chars    3 lines
#   Front Porch     0.799 us    0.021 ms
#               8 chars     1 lines
#   Back Porch      2.496 us    0.483 ms
#               25 chars    23 lines
#   Active Time     15.973 us   16.101 ms
#               160 chars   768 lines
#   Blank Time      4.992 us    0.566 ms
#               50 chars    27 lines
#   Polarity        positive    positive
#
    mode "1280x768-60"
# D: 80.13 MHz, H: 47.700 kHz, V: 60.00 Hz
    geometry 1280 768 1280 768 32
    timings 12480 200 48 23 1 126 3 hsync high vsync high endmode
#
#   1280x800, 60 Hz, Non-Interlaced (83.375 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280    800
#   Scan Frequency  49.628 kHz  60.00 Hz
#   Sync Width      1.631 us    60.450 us
#                   17 chars    3 lines
#   Front Porch     0.768 us    20.15 us
#                   8 chars     1 lines
#   Back Porch      2.399 us    0.483 ms
#                   25 chars    24 lines
#   Active Time     15.352 us   16.120 ms
#                   160 chars   800 lines
#   Blank Time      4.798 us    0.564 ms
#                   50 chars    28 lines
#   Polarity        negtive    positive
#
    mode "1280x800-60"
# D: 83.500 MHz, H: 49.702 kHz, V: 60.00 Hz
    geometry 1280 800 1280 800 32 timings 11994 200 72 22 3 128 6 endmode
#
#   1280x960, 60 Hz, Non-Interlaced (108.00 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280    960
#   Scan Frequency  60.000 kHz  60.00 Hz
#   Sync Width      1.037 us    0.050 ms
#               14 chars    3 lines
#   Front Porch     0.889 us    0.017 ms
#               12 chars    1 lines
#   Back Porch      2.889 us    0.600 ms
#               39 chars    36 lines
#   Active Time     11.852 us   16.000 ms
#               160 chars   960 lines
#   Blank Time      4.815 us    0.667 ms
#               65 chars    40 lines
#   Polarity        positive    positive
#
    mode "1280x960-60"
# D: 108.00 MHz, H: 60.000 kHz, V: 60.00 Hz
    geometry 1280 960 1280 960 32
    timings 9259 312 96 36 1 112 3 hsync high vsync high endmode
#
#   1280x1024, 60 Hz, Non-Interlaced (108.00 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280        1024
#   Scan Frequency      63.981 kHz  60.02 Hz
#   Sync Width      1.037 us    0.047 ms
#               14 chars    3 lines
#   Front Porch     0.444 us    0.015 ms
#               6 chars     1 lines
#   Back Porch      2.297 us    0.594 ms
#               31 chars    38 lines
#   Active Time     11.852 us   16.005 ms
#               160 chars   1024 lines
#   Blank Time      3.778 us    0.656 ms
#               51 chars    42 lines
#   Polarity        positive    positive
#
    mode "1280x1024-60"
# D: 108.00 MHz, H: 63.981 kHz, V: 60.02 Hz
    geometry 1280 1024 1280 1024 32
    timings 9260 248 48 38 1 112 3 hsync high vsync high endmode
#
#   1280x1024, 75 Hz, Non-Interlaced (135.00 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280        1024
#   Scan Frequency      79.976 kHz  75.02 Hz
#   Sync Width      1.067 us    0.038 ms
#               18 chars    3 lines
#   Front Porch     0.119 us    0.012 ms
#               2 chars     1 lines
#   Back Porch      1.837 us    0.475 ms
#               31 chars    38 lines
#   Active Time     9.481 us    12.804 ms
#               160 chars   1024 lines
#   Blank Time      3.022 us    0.525 ms
#               51 chars    42 lines
#   Polarity        positive    positive
#
    mode "1280x1024-75"
# D: 135.00 MHz, H: 79.976 kHz, V: 75.02 Hz
    geometry 1280 1024 1280 1024 32
    timings 7408 248 16 38 1 144 3 hsync high vsync high endmode
#
#   1280x1024, 85 Hz, Non-Interlaced (157.50 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280        1024
#   Scan Frequency  91.146 kHz  85.02 Hz
#   Sync Width      1.016 us    0.033 ms
#               20 chars    3 lines
#   Front Porch     0.406 us    0.011 ms
#               8 chars     1 lines
#   Back Porch      1.422 us    0.483 ms
#               28 chars    44 lines
#   Active Time     8.127 us    11.235 ms
#               160 chars   1024 lines
#   Blank Time      2.844 us    0.527 ms
#               56 chars    48 lines
#   Polarity        positive    positive
#
    mode "1280x1024-85"
# D: 157.50 MHz, H: 91.146 kHz, V: 85.02 Hz
    geometry 1280 1024 1280 1024 32
    timings 6349 224 64 44 1 160 3
    hsync high vsync high endmode mode "1440x900-60"
# D: 106.500 MHz, H: 55.935 kHz, V: 60.00 Hz
    geometry 1440 900 1440 900 32
    timings 9390 232 80 25 3 152 6
    hsync high vsync high endmode mode "1440x900-75"
# D: 136.750 MHz, H: 70.635 kHz, V: 75.00 Hz
    geometry 1440 900 1440 900 32
    timings 7315 248 96 33 3 152 6 hsync high vsync high endmode
#
#   1440x1050, 60 Hz, Non-Interlaced (125.10 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1440        1050
#   Scan Frequency      65.220 kHz  60.00 Hz
#   Sync Width      1.204 us    0.046 ms
#               19 chars    3 lines
#   Front Porch     0.760 us    0.015 ms
#               12 chars    1 lines
#   Back Porch      1.964 us    0.495 ms
#               31 chars    33 lines
#   Active Time     11.405 us   16.099 ms
#               180 chars   1050 lines
#   Blank Time      3.928 us    0.567 ms
#               62 chars    37 lines
#   Polarity        positive    positive
#
    mode "1440x1050-60"
# D: 125.10 MHz, H: 65.220 kHz, V: 60.00 Hz
    geometry 1440 1050 1440 1050 32
    timings 7993 248 96 33 1 152 3
    hsync high vsync high endmode mode "1600x900-60"
# D: 118.250 MHz, H: 55.990 kHz, V: 60.00 Hz
    geometry 1600 900 1600 900 32
    timings 8415 256 88 26 3 168 5 endmode mode "1600x1024-60"
# D: 136.358 MHz, H: 63.600 kHz, V: 60.00 Hz
    geometry 1600 1024 1600 1024 32 timings 7315 272 104 32 1 168 3 endmode
#
#   1600x1200, 60 Hz, Non-Interlaced (156.00 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1600        1200
#   Scan Frequency      76.200 kHz  60.00 Hz
#   Sync Width      1.026 us    0.105 ms
#               20 chars    8 lines
#   Front Porch     0.205 us    0.131 ms
#               4 chars     10 lines
#   Back Porch      1.636 us    0.682 ms
#               32 chars    52 lines
#   Active Time     10.256 us   15.748 ms
#               200 chars   1200 lines
#   Blank Time      2.872 us    0.866 ms
#               56 chars    66 lines
#   Polarity        negative    negative
#
    mode "1600x1200-60"
# D: 156.00 MHz, H: 76.200 kHz, V: 60.00 Hz
    geometry 1600 1200 1600 1200 32 timings 6172 256 32 52 10 160 8 endmode
#
#   1600x1200, 75 Hz, Non-Interlaced (202.50 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1600        1200
#   Scan Frequency  93.750 kHz  75.00 Hz
#   Sync Width      0.948 us    0.032 ms
#               24 chars    3 lines
#   Front Porch     0.316 us    0.011 ms
#               8 chars     1 lines
#   Back Porch      1.501 us    0.491 ms
#               38 chars    46 lines
#   Active Time     7.901 us    12.800 ms
#               200 chars   1200 lines
#   Blank Time      2.765 us    0.533 ms
#               70 chars    50 lines
#   Polarity    positive    positive
#
    mode "1600x1200-75"
# D: 202.50 MHz, H: 93.750 kHz, V: 75.00 Hz
    geometry 1600 1200 1600 1200 32
    timings 4938 304 64 46 1 192 3
    hsync high vsync high endmode mode "1680x1050-60"
# D: 146.250 MHz, H: 65.290 kHz, V: 59.954 Hz
    geometry 1680 1050 1680 1050 32
    timings 6814 280 104 30 3 176 6
    hsync high vsync high endmode mode "1680x1050-75"
# D: 187.000 MHz, H: 82.306 kHz, V: 74.892 Hz
    geometry 1680 1050 1680 1050 32
    timings 5348 296 120 40 3 176 6
    hsync high vsync high endmode mode "1792x1344-60"
# D: 202.975 MHz, H: 83.460 kHz, V: 60.00 Hz
    geometry 1792 1344 1792 1344 32
    timings 4902 320 128 43 1 192 3
    hsync high vsync high endmode mode "1856x1392-60"
# D: 218.571 MHz, H: 86.460 kHz, V: 60.00 Hz
    geometry 1856 1392 1856 1392 32
    timings 4577 336 136 45 1 200 3
    hsync high vsync high endmode mode "1920x1200-60"
# D: 193.250 MHz, H: 74.556 kHz, V: 60.00 Hz
    geometry 1920 1200 1920 1200 32
    timings 5173 336 136 36 3 200 6
    hsync high vsync high endmode mode "1920x1440-60"
# D: 234.000 MHz, H:90.000 kHz, V: 60.00 Hz
    geometry 1920 1440 1920 1440 32
    timings 4274 344 128 56 1 208 3
    hsync high vsync high endmode mode "1920x1440-75"
# D: 297.000 MHz, H:112.500 kHz, V: 75.00 Hz
    geometry 1920 1440 1920 1440 32
    timings 3367 352 144 56 1 224 3
    hsync high vsync high endmode mode "2048x1536-60"
# D: 267.250 MHz, H: 95.446 kHz, V: 60.00 Hz
    geometry 2048 1536 2048 1536 32
    timings 3742 376 152 49 3 224 4 hsync high vsync high endmode
#
#   1280x720, 60 Hz, Non-Interlaced (74.481 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1280        720
#   Scan Frequency      44.760 kHz  60.00 Hz
#   Sync Width      1.826 us    67.024 ms
#               17 chars    3 lines
#   Front Porch     0.752 us    22.341 ms
#               7 chars     1 lines
#   Back Porch      2.578 us    491.510 ms
#               24 chars    22 lines
#   Active Time     17.186 us   16.086 ms
#               160 chars   720 lines
#   Blank Time      5.156 us    0.581 ms
#               48 chars    26 lines
#   Polarity        negative    negative
#
    mode "1280x720-60"
# D: 74.481 MHz, H: 44.760 kHz, V: 60.00 Hz
    geometry 1280 720 1280 720 32 timings 13426 192 64 22 1 136 3 endmode
#
#   1920x1080, 60 Hz, Non-Interlaced (172.798 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1920        1080
#   Scan Frequency      67.080 kHz  60.00 Hz
#   Sync Width      1.204 us    44.723 ms
#               26 chars    3 lines
#   Front Porch     0.694 us    14.908 ms
#               15 chars     1 lines
#   Back Porch      1.898 us    506.857 ms
#               41 chars    34 lines
#   Active Time     11.111 us   16.100 ms
#               240 chars   1080 lines
#   Blank Time      3.796 us    0.566 ms
#               82 chars    38 lines
#   Polarity        negative    negative
#
    mode "1920x1080-60"
# D: 74.481 MHz, H: 67.080 kHz, V: 60.00 Hz
    geometry 1920 1080 1920 1080 32 timings 5787 328 120 34 1 208 3 endmode
#
#   1400x1050, 60 Hz, Non-Interlaced (122.61 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1400        1050
#   Scan Frequency      65.218 kHz  59.99 Hz
#   Sync Width      1.037 us    0.047 ms
#               19 chars    3 lines
#   Front Porch     0.444 us    0.015 ms
#               11 chars     1 lines
#   Back Porch      1.185 us    0.188 ms
#               30 chars    33 lines
#   Active Time     12.963 us   16.411 ms
#               175 chars   1050 lines
#   Blank Time      2.667 us    0.250 ms
#               60 chars    37 lines
#   Polarity        negative    positive
#
    mode "1400x1050-60"
# D: 122.750 MHz, H: 65.317 kHz, V: 59.99 Hz
    geometry 1400 1050 1408 1050 32
    timings 8214 232 88 32 3 144 4 endmode mode "1400x1050-75"
# D: 156.000 MHz, H: 82.278 kHz, V: 74.867 Hz
    geometry 1400 1050 1408 1050 32 timings 6410 248 104 42 3 144 4 endmode
#
#   1366x768, 60 Hz, Non-Interlaced (85.86 MHz dotclock)
#
#               Horizontal  Vertical
#   Resolution      1366        768
#   Scan Frequency      47.700 kHz  60.00 Hz
#   Sync Width      1.677 us    0.063 ms
#               18 chars    3 lines
#   Front Porch     0.839 us    0.021 ms
#               9 chars     1 lines
#   Back Porch      2.516 us    0.482 ms
#               27 chars    23 lines
#   Active Time     15.933 us   16.101 ms
#               171 chars   768 lines
#   Blank Time      5.031 us    0.566 ms
#               54 chars    27 lines
#   Polarity        negative    positive
#
    mode "1360x768-60"
# D: 84.750 MHz, H: 47.720 kHz, V: 60.00 Hz
    geometry 1360 768 1360 768 32
    timings 11799 208 72 22 3 136 5 endmode mode "1366x768-60"
# D: 85.86 MHz, H: 47.700 kHz, V: 60.00 Hz
    geometry 1366 768 1366 768 32
    timings 11647 216 72 23 1 144 3 endmode mode "1366x768-50"
# D: 69,924 MHz, H: 39.550 kHz, V: 50.00 Hz
    geometry 1366 768 1366 768 32 timings 14301 200 56 19 1 144 3 endmode
