* Freescale IMX53 IOMUX Controller

Please refer to fsl,imx-pinctrl.txt in this directory for common binding part
and usage.

Required properties:
- compatible: "fsl,imx53-iomuxc"
- fsl,pins: two integers array, represents a group of pins mux and config
  setting. The format is fsl,pins = <PIN_FUNC_ID CONFIG>, PIN_FUNC_ID is a
  pin working on a specific function, CONFIG is the pad setting value like
  pull-up for this pin. Please refer to imx53 datasheet for the valid pad
  config settings.

CONFIG bits definition:
PAD_CTL_HVE			(1 << 13)
PAD_CTL_HYS			(1 << 8)
PAD_CTL_PKE			(1 << 7)
PAD_CTL_PUE			(1 << 6)
PAD_CTL_PUS_100K_DOWN		(0 << 4)
PAD_CTL_PUS_47K_UP		(1 << 4)
PAD_CTL_PUS_100K_UP		(2 << 4)
PAD_CTL_PUS_22K_UP		(3 << 4)
PAD_CTL_ODE			(1 << 3)
PAD_CTL_DSE_LOW			(0 << 1)
PAD_CTL_DSE_MED			(1 << 1)
PAD_CTL_DSE_HIGH		(2 << 1)
PAD_CTL_DSE_MAX			(3 << 1)
PAD_CTL_SRE_FAST		(1 << 0)
PAD_CTL_SRE_SLOW		(0 << 0)

See below for available PIN_FUNC_ID for imx53:
MX53_PAD_GPIO_19__KPP_COL_5				0
MX53_PAD_GPIO_19__GPIO4_5				1
MX53_PAD_GPIO_19__CCM_CLKO				2
MX53_PAD_GPIO_19__SPDIF_OUT1				3
MX53_PAD_GPIO_19__RTC_CE_RTC_EXT_TRIG2			4
MX53_PAD_GPIO_19__ECSPI1_RDY				5
MX53_PAD_GPIO_19__FEC_TDATA_3				6
MX53_PAD_GPIO_19__SRC_INT_BOOT				7
MX53_PAD_KEY_COL0__KPP_COL_0				8
MX53_PAD_KEY_COL0__GPIO4_6				9
MX53_PAD_KEY_COL0__AUDMUX_AUD5_TXC			10
MX53_PAD_KEY_COL0__UART4_TXD_MUX			11
MX53_PAD_KEY_COL0__ECSPI1_SCLK				12
MX53_PAD_KEY_COL0__FEC_RDATA_3				13
MX53_PAD_KEY_COL0__SRC_ANY_PU_RST			14
MX53_PAD_KEY_ROW0__KPP_ROW_0				15
MX53_PAD_KEY_ROW0__GPIO4_7				16
MX53_PAD_KEY_ROW0__AUDMUX_AUD5_TXD			17
MX53_PAD_KEY_ROW0__UART4_RXD_MUX			18
MX53_PAD_KEY_ROW0__ECSPI1_MOSI				19
MX53_PAD_KEY_ROW0__FEC_TX_ER				20
MX53_PAD_KEY_COL1__KPP_COL_1				21
MX53_PAD_KEY_COL1__GPIO4_8				22
MX53_PAD_KEY_COL1__AUDMUX_AUD5_TXFS			23
MX53_PAD_KEY_COL1__UART5_TXD_MUX			24
MX53_PAD_KEY_COL1__ECSPI1_MISO				25
MX53_PAD_KEY_COL1__FEC_RX_CLK				26
MX53_PAD_KEY_COL1__USBPHY1_TXREADY			27
MX53_PAD_KEY_ROW1__KPP_ROW_1				28
MX53_PAD_KEY_ROW1__GPIO4_9				29
MX53_PAD_KEY_ROW1__AUDMUX_AUD5_RXD			30
MX53_PAD_KEY_ROW1__UART5_RXD_MUX			31
MX53_PAD_KEY_ROW1__ECSPI1_SS0				32
MX53_PAD_KEY_ROW1__FEC_COL				33
MX53_PAD_KEY_ROW1__USBPHY1_RXVALID			34
MX53_PAD_KEY_COL2__KPP_COL_2				35
MX53_PAD_KEY_COL2__GPIO4_10				36
MX53_PAD_KEY_COL2__CAN1_TXCAN				37
MX53_PAD_KEY_COL2__FEC_MDIO				38
MX53_PAD_KEY_COL2__ECSPI1_SS1				39
MX53_PAD_KEY_COL2__FEC_RDATA_2				40
MX53_PAD_KEY_COL2__USBPHY1_RXACTIVE			41
MX53_PAD_KEY_ROW2__KPP_ROW_2				42
MX53_PAD_KEY_ROW2__GPIO4_11				43
MX53_PAD_KEY_ROW2__CAN1_RXCAN				44
MX53_PAD_KEY_ROW2__FEC_MDC				45
MX53_PAD_KEY_ROW2__ECSPI1_SS2				46
MX53_PAD_KEY_ROW2__FEC_TDATA_2				47
MX53_PAD_KEY_ROW2__USBPHY1_RXERROR			48
MX53_PAD_KEY_COL3__KPP_COL_3				49
MX53_PAD_KEY_COL3__GPIO4_12				50
MX53_PAD_KEY_COL3__USBOH3_H2_DP				51
MX53_PAD_KEY_COL3__SPDIF_IN1				52
MX53_PAD_KEY_COL3__I2C2_SCL				53
MX53_PAD_KEY_COL3__ECSPI1_SS3				54
MX53_PAD_KEY_COL3__FEC_CRS				55
MX53_PAD_KEY_COL3__USBPHY1_SIECLOCK			56
MX53_PAD_KEY_ROW3__KPP_ROW_3				57
MX53_PAD_KEY_ROW3__GPIO4_13				58
MX53_PAD_KEY_ROW3__USBOH3_H2_DM				59
MX53_PAD_KEY_ROW3__CCM_ASRC_EXT_CLK			60
MX53_PAD_KEY_ROW3__I2C2_SDA				61
MX53_PAD_KEY_ROW3__OSC32K_32K_OUT			62
MX53_PAD_KEY_ROW3__CCM_PLL4_BYP				63
MX53_PAD_KEY_ROW3__USBPHY1_LINESTATE_0			64
MX53_PAD_KEY_COL4__KPP_COL_4				65
MX53_PAD_KEY_COL4__GPIO4_14				66
MX53_PAD_KEY_COL4__CAN2_TXCAN				67
MX53_PAD_KEY_COL4__IPU_SISG_4				68
MX53_PAD_KEY_COL4__UART5_RTS				69
MX53_PAD_KEY_COL4__USBOH3_USBOTG_OC			70
MX53_PAD_KEY_COL4__USBPHY1_LINESTATE_1			71
MX53_PAD_KEY_ROW4__KPP_ROW_4				72
MX53_PAD_KEY_ROW4__GPIO4_15				73
MX53_PAD_KEY_ROW4__CAN2_RXCAN				74
MX53_PAD_KEY_ROW4__IPU_SISG_5				75
MX53_PAD_KEY_ROW4__UART5_CTS				76
MX53_PAD_KEY_ROW4__USBOH3_USBOTG_PWR			77
MX53_PAD_KEY_ROW4__USBPHY1_VBUSVALID			78
MX53_PAD_DI0_DISP_CLK__IPU_DI0_DISP_CLK			79
MX53_PAD_DI0_DISP_CLK__GPIO4_16				80
MX53_PAD_DI0_DISP_CLK__USBOH3_USBH2_DIR			81
MX53_PAD_DI0_DISP_CLK__SDMA_DEBUG_CORE_STATE_0		82
MX53_PAD_DI0_DISP_CLK__EMI_EMI_DEBUG_0			83
MX53_PAD_DI0_DISP_CLK__USBPHY1_AVALID			84
MX53_PAD_DI0_PIN15__IPU_DI0_PIN15			85
MX53_PAD_DI0_PIN15__GPIO4_17				86
MX53_PAD_DI0_PIN15__AUDMUX_AUD6_TXC			87
MX53_PAD_DI0_PIN15__SDMA_DEBUG_CORE_STATE_1		88
MX53_PAD_DI0_PIN15__EMI_EMI_DEBUG_1			89
MX53_PAD_DI0_PIN15__USBPHY1_BVALID			90
MX53_PAD_DI0_PIN2__IPU_DI0_PIN2				91
MX53_PAD_DI0_PIN2__GPIO4_18				92
MX53_PAD_DI0_PIN2__AUDMUX_AUD6_TXD			93
MX53_PAD_DI0_PIN2__SDMA_DEBUG_CORE_STATE_2		94
MX53_PAD_DI0_PIN2__EMI_EMI_DEBUG_2			95
MX53_PAD_DI0_PIN2__USBPHY1_ENDSESSION			96
MX53_PAD_DI0_PIN3__IPU_DI0_PIN3				97
MX53_PAD_DI0_PIN3__GPIO4_19				98
MX53_PAD_DI0_PIN3__AUDMUX_AUD6_TXFS			99
MX53_PAD_DI0_PIN3__SDMA_DEBUG_CORE_STATE_3		100
MX53_PAD_DI0_PIN3__EMI_EMI_DEBUG_3			101
MX53_PAD_DI0_PIN3__USBPHY1_IDDIG			102
MX53_PAD_DI0_PIN4__IPU_DI0_PIN4				103
MX53_PAD_DI0_PIN4__GPIO4_20				104
MX53_PAD_DI0_PIN4__AUDMUX_AUD6_RXD			105
MX53_PAD_DI0_PIN4__ESDHC1_WP				106
MX53_PAD_DI0_PIN4__SDMA_DEBUG_YIELD			107
MX53_PAD_DI0_PIN4__EMI_EMI_DEBUG_4			108
MX53_PAD_DI0_PIN4__USBPHY1_HOSTDISCONNECT		109
MX53_PAD_DISP0_DAT0__IPU_DISP0_DAT_0			110
MX53_PAD_DISP0_DAT0__GPIO4_21				111
MX53_PAD_DISP0_DAT0__CSPI_SCLK				112
MX53_PAD_DISP0_DAT0__USBOH3_USBH2_DATA_0		113
MX53_PAD_DISP0_DAT0__SDMA_DEBUG_CORE_RUN		114
MX53_PAD_DISP0_DAT0__EMI_EMI_DEBUG_5			115
MX53_PAD_DISP0_DAT0__USBPHY2_TXREADY			116
MX53_PAD_DISP0_DAT1__IPU_DISP0_DAT_1			117
MX53_PAD_DISP0_DAT1__GPIO4_22				118
MX53_PAD_DISP0_DAT1__CSPI_MOSI				119
MX53_PAD_DISP0_DAT1__USBOH3_USBH2_DATA_1		120
MX53_PAD_DISP0_DAT1__SDMA_DEBUG_EVENT_CHANNEL_SEL	121
MX53_PAD_DISP0_DAT1__EMI_EMI_DEBUG_6			122
MX53_PAD_DISP0_DAT1__USBPHY2_RXVALID			123
MX53_PAD_DISP0_DAT2__IPU_DISP0_DAT_2			124
MX53_PAD_DISP0_DAT2__GPIO4_23				125
MX53_PAD_DISP0_DAT2__CSPI_MISO				126
MX53_PAD_DISP0_DAT2__USBOH3_USBH2_DATA_2		127
MX53_PAD_DISP0_DAT2__SDMA_DEBUG_MODE			128
MX53_PAD_DISP0_DAT2__EMI_EMI_DEBUG_7			129
MX53_PAD_DISP0_DAT2__USBPHY2_RXACTIVE			130
MX53_PAD_DISP0_DAT3__IPU_DISP0_DAT_3			131
MX53_PAD_DISP0_DAT3__GPIO4_24				132
MX53_PAD_DISP0_DAT3__CSPI_SS0				133
MX53_PAD_DISP0_DAT3__USBOH3_USBH2_DATA_3		134
MX53_PAD_DISP0_DAT3__SDMA_DEBUG_BUS_ERROR		135
MX53_PAD_DISP0_DAT3__EMI_EMI_DEBUG_8			136
MX53_PAD_DISP0_DAT3__USBPHY2_RXERROR			137
MX53_PAD_DISP0_DAT4__IPU_DISP0_DAT_4			138
MX53_PAD_DISP0_DAT4__GPIO4_25				139
MX53_PAD_DISP0_DAT4__CSPI_SS1				140
MX53_PAD_DISP0_DAT4__USBOH3_USBH2_DATA_4		141
MX53_PAD_DISP0_DAT4__SDMA_DEBUG_BUS_RWB			142
MX53_PAD_DISP0_DAT4__EMI_EMI_DEBUG_9			143
MX53_PAD_DISP0_DAT4__USBPHY2_SIECLOCK			144
MX53_PAD_DISP0_DAT5__IPU_DISP0_DAT_5			145
MX53_PAD_DISP0_DAT5__GPIO4_26				146
MX53_PAD_DISP0_DAT5__CSPI_SS2				147
MX53_PAD_DISP0_DAT5__USBOH3_USBH2_DATA_5		148
MX53_PAD_DISP0_DAT5__SDMA_DEBUG_MATCHED_DMBUS		149
MX53_PAD_DISP0_DAT5__EMI_EMI_DEBUG_10			150
MX53_PAD_DISP0_DAT5__USBPHY2_LINESTATE_0		151
MX53_PAD_DISP0_DAT6__IPU_DISP0_DAT_6			152
MX53_PAD_DISP0_DAT6__GPIO4_27				153
MX53_PAD_DISP0_DAT6__CSPI_SS3				154
MX53_PAD_DISP0_DAT6__USBOH3_USBH2_DATA_6		155
MX53_PAD_DISP0_DAT6__SDMA_DEBUG_RTBUFFER_WRITE		156
MX53_PAD_DISP0_DAT6__EMI_EMI_DEBUG_11			157
MX53_PAD_DISP0_DAT6__USBPHY2_LINESTATE_1		158
MX53_PAD_DISP0_DAT7__IPU_DISP0_DAT_7			159
MX53_PAD_DISP0_DAT7__GPIO4_28				160
MX53_PAD_DISP0_DAT7__CSPI_RDY				161
MX53_PAD_DISP0_DAT7__USBOH3_USBH2_DATA_7		162
MX53_PAD_DISP0_DAT7__SDMA_DEBUG_EVENT_CHANNEL_0		163
MX53_PAD_DISP0_DAT7__EMI_EMI_DEBUG_12			164
MX53_PAD_DISP0_DAT7__USBPHY2_VBUSVALID			165
MX53_PAD_DISP0_DAT8__IPU_DISP0_DAT_8			166
MX53_PAD_DISP0_DAT8__GPIO4_29				167
MX53_PAD_DISP0_DAT8__PWM1_PWMO				168
MX53_PAD_DISP0_DAT8__WDOG1_WDOG_B			169
MX53_PAD_DISP0_DAT8__SDMA_DEBUG_EVENT_CHANNEL_1		170
MX53_PAD_DISP0_DAT8__EMI_EMI_DEBUG_13			171
MX53_PAD_DISP0_DAT8__USBPHY2_AVALID			172
MX53_PAD_DISP0_DAT9__IPU_DISP0_DAT_9			173
MX53_PAD_DISP0_DAT9__GPIO4_30				174
MX53_PAD_DISP0_DAT9__PWM2_PWMO				175
MX53_PAD_DISP0_DAT9__WDOG2_WDOG_B			176
MX53_PAD_DISP0_DAT9__SDMA_DEBUG_EVENT_CHANNEL_2		177
MX53_PAD_DISP0_DAT9__EMI_EMI_DEBUG_14			178
MX53_PAD_DISP0_DAT9__USBPHY2_VSTATUS_0			179
MX53_PAD_DISP0_DAT10__IPU_DISP0_DAT_10			180
MX53_PAD_DISP0_DAT10__GPIO4_31				181
MX53_PAD_DISP0_DAT10__USBOH3_USBH2_STP			182
MX53_PAD_DISP0_DAT10__SDMA_DEBUG_EVENT_CHANNEL_3	183
MX53_PAD_DISP0_DAT10__EMI_EMI_DEBUG_15			184
MX53_PAD_DISP0_DAT10__USBPHY2_VSTATUS_1			185
MX53_PAD_DISP0_DAT11__IPU_DISP0_DAT_11			186
MX53_PAD_DISP0_DAT11__GPIO5_5				187
MX53_PAD_DISP0_DAT11__USBOH3_USBH2_NXT			188
MX53_PAD_DISP0_DAT11__SDMA_DEBUG_EVENT_CHANNEL_4	189
MX53_PAD_DISP0_DAT11__EMI_EMI_DEBUG_16			190
MX53_PAD_DISP0_DAT11__USBPHY2_VSTATUS_2			191
MX53_PAD_DISP0_DAT12__IPU_DISP0_DAT_12			192
MX53_PAD_DISP0_DAT12__GPIO5_6				193
MX53_PAD_DISP0_DAT12__USBOH3_USBH2_CLK			194
MX53_PAD_DISP0_DAT12__SDMA_DEBUG_EVENT_CHANNEL_5	195
MX53_PAD_DISP0_DAT12__EMI_EMI_DEBUG_17			196
MX53_PAD_DISP0_DAT12__USBPHY2_VSTATUS_3			197
MX53_PAD_DISP0_DAT13__IPU_DISP0_DAT_13			198
MX53_PAD_DISP0_DAT13__GPIO5_7				199
MX53_PAD_DISP0_DAT13__AUDMUX_AUD5_RXFS			200
MX53_PAD_DISP0_DAT13__SDMA_DEBUG_EVT_CHN_LINES_0	201
MX53_PAD_DISP0_DAT13__EMI_EMI_DEBUG_18			202
MX53_PAD_DISP0_DAT13__USBPHY2_VSTATUS_4			203
MX53_PAD_DISP0_DAT14__IPU_DISP0_DAT_14			204
MX53_PAD_DISP0_DAT14__GPIO5_8				205
MX53_PAD_DISP0_DAT14__AUDMUX_AUD5_RXC			206
MX53_PAD_DISP0_DAT14__SDMA_DEBUG_EVT_CHN_LINES_1	207
MX53_PAD_DISP0_DAT14__EMI_EMI_DEBUG_19			208
MX53_PAD_DISP0_DAT14__USBPHY2_VSTATUS_5			209
MX53_PAD_DISP0_DAT15__IPU_DISP0_DAT_15			210
MX53_PAD_DISP0_DAT15__GPIO5_9				211
MX53_PAD_DISP0_DAT15__ECSPI1_SS1			212
MX53_PAD_DISP0_DAT15__ECSPI2_SS1			213
MX53_PAD_DISP0_DAT15__SDMA_DEBUG_EVT_CHN_LINES_2	214
MX53_PAD_DISP0_DAT15__EMI_EMI_DEBUG_20			215
MX53_PAD_DISP0_DAT15__USBPHY2_VSTATUS_6			216
MX53_PAD_DISP0_DAT16__IPU_DISP0_DAT_16			217
MX53_PAD_DISP0_DAT16__GPIO5_10				218
MX53_PAD_DISP0_DAT16__ECSPI2_MOSI			219
MX53_PAD_DISP0_DAT16__AUDMUX_AUD5_TXC			220
MX53_PAD_DISP0_DAT16__SDMA_EXT_EVENT_0			221
MX53_PAD_DISP0_DAT16__SDMA_DEBUG_EVT_CHN_LINES_3	222
MX53_PAD_DISP0_DAT16__EMI_EMI_DEBUG_21			223
MX53_PAD_DISP0_DAT16__USBPHY2_VSTATUS_7			224
MX53_PAD_DISP0_DAT17__IPU_DISP0_DAT_17			225
MX53_PAD_DISP0_DAT17__GPIO5_11				226
MX53_PAD_DISP0_DAT17__ECSPI2_MISO			227
MX53_PAD_DISP0_DAT17__AUDMUX_AUD5_TXD			228
MX53_PAD_DISP0_DAT17__SDMA_EXT_EVENT_1			229
MX53_PAD_DISP0_DAT17__SDMA_DEBUG_EVT_CHN_LINES_4	230
MX53_PAD_DISP0_DAT17__EMI_EMI_DEBUG_22			231
MX53_PAD_DISP0_DAT18__IPU_DISP0_DAT_18			232
MX53_PAD_DISP0_DAT18__GPIO5_12				233
MX53_PAD_DISP0_DAT18__ECSPI2_SS0			234
MX53_PAD_DISP0_DAT18__AUDMUX_AUD5_TXFS			235
MX53_PAD_DISP0_DAT18__AUDMUX_AUD4_RXFS			236
MX53_PAD_DISP0_DAT18__SDMA_DEBUG_EVT_CHN_LINES_5	237
MX53_PAD_DISP0_DAT18__EMI_EMI_DEBUG_23			238
MX53_PAD_DISP0_DAT18__EMI_WEIM_CS_2			239
MX53_PAD_DISP0_DAT19__IPU_DISP0_DAT_19			240
MX53_PAD_DISP0_DAT19__GPIO5_13				241
MX53_PAD_DISP0_DAT19__ECSPI2_SCLK			242
MX53_PAD_DISP0_DAT19__AUDMUX_AUD5_RXD			243
MX53_PAD_DISP0_DAT19__AUDMUX_AUD4_RXC			244
MX53_PAD_DISP0_DAT19__SDMA_DEBUG_EVT_CHN_LINES_6	245
MX53_PAD_DISP0_DAT19__EMI_EMI_DEBUG_24			246
MX53_PAD_DISP0_DAT19__EMI_WEIM_CS_3			247
MX53_PAD_DISP0_DAT20__IPU_DISP0_DAT_20			248
MX53_PAD_DISP0_DAT20__GPIO5_14				249
MX53_PAD_DISP0_DAT20__ECSPI1_SCLK			250
MX53_PAD_DISP0_DAT20__AUDMUX_AUD4_TXC			251
MX53_PAD_DISP0_DAT20__SDMA_DEBUG_EVT_CHN_LINES_7	252
MX53_PAD_DISP0_DAT20__EMI_EMI_DEBUG_25			253
MX53_PAD_DISP0_DAT20__SATA_PHY_TDI			254
MX53_PAD_DISP0_DAT21__IPU_DISP0_DAT_21			255
MX53_PAD_DISP0_DAT21__GPIO5_15				256
MX53_PAD_DISP0_DAT21__ECSPI1_MOSI			257
MX53_PAD_DISP0_DAT21__AUDMUX_AUD4_TXD			258
MX53_PAD_DISP0_DAT21__SDMA_DEBUG_BUS_DEVICE_0		259
MX53_PAD_DISP0_DAT21__EMI_EMI_DEBUG_26			260
MX53_PAD_DISP0_DAT21__SATA_PHY_TDO			261
MX53_PAD_DISP0_DAT22__IPU_DISP0_DAT_22			262
MX53_PAD_DISP0_DAT22__GPIO5_16				263
MX53_PAD_DISP0_DAT22__ECSPI1_MISO			264
MX53_PAD_DISP0_DAT22__AUDMUX_AUD4_TXFS			265
MX53_PAD_DISP0_DAT22__SDMA_DEBUG_BUS_DEVICE_1		266
MX53_PAD_DISP0_DAT22__EMI_EMI_DEBUG_27			267
MX53_PAD_DISP0_DAT22__SATA_PHY_TCK			268
MX53_PAD_DISP0_DAT23__IPU_DISP0_DAT_23			269
MX53_PAD_DISP0_DAT23__GPIO5_17				270
MX53_PAD_DISP0_DAT23__ECSPI1_SS0			271
MX53_PAD_DISP0_DAT23__AUDMUX_AUD4_RXD			272
MX53_PAD_DISP0_DAT23__SDMA_DEBUG_BUS_DEVICE_2		273
MX53_PAD_DISP0_DAT23__EMI_EMI_DEBUG_28			274
MX53_PAD_DISP0_DAT23__SATA_PHY_TMS			275
MX53_PAD_CSI0_PIXCLK__IPU_CSI0_PIXCLK			276
MX53_PAD_CSI0_PIXCLK__GPIO5_18				277
MX53_PAD_CSI0_PIXCLK__SDMA_DEBUG_PC_0			278
MX53_PAD_CSI0_PIXCLK__EMI_EMI_DEBUG_29			279
MX53_PAD_CSI0_MCLK__IPU_CSI0_HSYNC			280
MX53_PAD_CSI0_MCLK__GPIO5_19				281
MX53_PAD_CSI0_MCLK__CCM_CSI0_MCLK			282
MX53_PAD_CSI0_MCLK__SDMA_DEBUG_PC_1			283
MX53_PAD_CSI0_MCLK__EMI_EMI_DEBUG_30			284
MX53_PAD_CSI0_MCLK__TPIU_TRCTL				285
MX53_PAD_CSI0_DATA_EN__IPU_CSI0_DATA_EN			286
MX53_PAD_CSI0_DATA_EN__GPIO5_20				287
MX53_PAD_CSI0_DATA_EN__SDMA_DEBUG_PC_2			288
MX53_PAD_CSI0_DATA_EN__EMI_EMI_DEBUG_31			289
MX53_PAD_CSI0_DATA_EN__TPIU_TRCLK			290
MX53_PAD_CSI0_VSYNC__IPU_CSI0_VSYNC			291
MX53_PAD_CSI0_VSYNC__GPIO5_21				292
MX53_PAD_CSI0_VSYNC__SDMA_DEBUG_PC_3			293
MX53_PAD_CSI0_VSYNC__EMI_EMI_DEBUG_32			294
MX53_PAD_CSI0_VSYNC__TPIU_TRACE_0			295
MX53_PAD_CSI0_DAT4__IPU_CSI0_D_4			296
MX53_PAD_CSI0_DAT4__GPIO5_22				297
MX53_PAD_CSI0_DAT4__KPP_COL_5				298
MX53_PAD_CSI0_DAT4__ECSPI1_SCLK				299
MX53_PAD_CSI0_DAT4__USBOH3_USBH3_STP			300
MX53_PAD_CSI0_DAT4__AUDMUX_AUD3_TXC			301
MX53_PAD_CSI0_DAT4__EMI_EMI_DEBUG_33			302
MX53_PAD_CSI0_DAT4__TPIU_TRACE_1			303
MX53_PAD_CSI0_DAT5__IPU_CSI0_D_5			304
MX53_PAD_CSI0_DAT5__GPIO5_23				305
MX53_PAD_CSI0_DAT5__KPP_ROW_5				306
MX53_PAD_CSI0_DAT5__ECSPI1_MOSI				307
MX53_PAD_CSI0_DAT5__USBOH3_USBH3_NXT			308
MX53_PAD_CSI0_DAT5__AUDMUX_AUD3_TXD			309
MX53_PAD_CSI0_DAT5__EMI_EMI_DEBUG_34			310
MX53_PAD_CSI0_DAT5__TPIU_TRACE_2			311
MX53_PAD_CSI0_DAT6__IPU_CSI0_D_6			312
MX53_PAD_CSI0_DAT6__GPIO5_24				313
MX53_PAD_CSI0_DAT6__KPP_COL_6				314
MX53_PAD_CSI0_DAT6__ECSPI1_MISO				315
MX53_PAD_CSI0_DAT6__USBOH3_USBH3_CLK			316
MX53_PAD_CSI0_DAT6__AUDMUX_AUD3_TXFS			317
MX53_PAD_CSI0_DAT6__EMI_EMI_DEBUG_35			318
MX53_PAD_CSI0_DAT6__TPIU_TRACE_3			319
MX53_PAD_CSI0_DAT7__IPU_CSI0_D_7			320
MX53_PAD_CSI0_DAT7__GPIO5_25				321
MX53_PAD_CSI0_DAT7__KPP_ROW_6				322
MX53_PAD_CSI0_DAT7__ECSPI1_SS0				323
MX53_PAD_CSI0_DAT7__USBOH3_USBH3_DIR			324
MX53_PAD_CSI0_DAT7__AUDMUX_AUD3_RXD			325
MX53_PAD_CSI0_DAT7__EMI_EMI_DEBUG_36			326
MX53_PAD_CSI0_DAT7__TPIU_TRACE_4			327
MX53_PAD_CSI0_DAT8__IPU_CSI0_D_8			328
MX53_PAD_CSI0_DAT8__GPIO5_26				329
MX53_PAD_CSI0_DAT8__KPP_COL_7				330
MX53_PAD_CSI0_DAT8__ECSPI2_SCLK				331
MX53_PAD_CSI0_DAT8__USBOH3_USBH3_OC			332
MX53_PAD_CSI0_DAT8__I2C1_SDA				333
MX53_PAD_CSI0_DAT8__EMI_EMI_DEBUG_37			334
MX53_PAD_CSI0_DAT8__TPIU_TRACE_5			335
MX53_PAD_CSI0_DAT9__IPU_CSI0_D_9			336
MX53_PAD_CSI0_DAT9__GPIO5_27				337
MX53_PAD_CSI0_DAT9__KPP_ROW_7				338
MX53_PAD_CSI0_DAT9__ECSPI2_MOSI				339
MX53_PAD_CSI0_DAT9__USBOH3_USBH3_PWR			340
MX53_PAD_CSI0_DAT9__I2C1_SCL				341
MX53_PAD_CSI0_DAT9__EMI_EMI_DEBUG_38			342
MX53_PAD_CSI0_DAT9__TPIU_TRACE_6			343
MX53_PAD_CSI0_DAT10__IPU_CSI0_D_10			344
MX53_PAD_CSI0_DAT10__GPIO5_28				345
MX53_PAD_CSI0_DAT10__UART1_TXD_MUX			346
MX53_PAD_CSI0_DAT10__ECSPI2_MISO			347
MX53_PAD_CSI0_DAT10__AUDMUX_AUD3_RXC			348
MX53_PAD_CSI0_DAT10__SDMA_DEBUG_PC_4			349
MX53_PAD_CSI0_DAT10__EMI_EMI_DEBUG_39			350
MX53_PAD_CSI0_DAT10__TPIU_TRACE_7			351
MX53_PAD_CSI0_DAT11__IPU_CSI0_D_11			352
MX53_PAD_CSI0_DAT11__GPIO5_29				353
MX53_PAD_CSI0_DAT11__UART1_RXD_MUX			354
MX53_PAD_CSI0_DAT11__ECSPI2_SS0				355
MX53_PAD_CSI0_DAT11__AUDMUX_AUD3_RXFS			356
MX53_PAD_CSI0_DAT11__SDMA_DEBUG_PC_5			357
MX53_PAD_CSI0_DAT11__EMI_EMI_DEBUG_40			358
MX53_PAD_CSI0_DAT11__TPIU_TRACE_8			359
MX53_PAD_CSI0_DAT12__IPU_CSI0_D_12			360
MX53_PAD_CSI0_DAT12__GPIO5_30				361
MX53_PAD_CSI0_DAT12__UART4_TXD_MUX			362
MX53_PAD_CSI0_DAT12__USBOH3_USBH3_DATA_0		363
MX53_PAD_CSI0_DAT12__SDMA_DEBUG_PC_6			364
MX53_PAD_CSI0_DAT12__EMI_EMI_DEBUG_41			365
MX53_PAD_CSI0_DAT12__TPIU_TRACE_9			366
MX53_PAD_CSI0_DAT13__IPU_CSI0_D_13			367
MX53_PAD_CSI0_DAT13__GPIO5_31				368
MX53_PAD_CSI0_DAT13__UART4_RXD_MUX			369
MX53_PAD_CSI0_DAT13__USBOH3_USBH3_DATA_1		370
MX53_PAD_CSI0_DAT13__SDMA_DEBUG_PC_7			371
MX53_PAD_CSI0_DAT13__EMI_EMI_DEBUG_42			372
MX53_PAD_CSI0_DAT13__TPIU_TRACE_10			373
MX53_PAD_CSI0_DAT14__IPU_CSI0_D_14			374
MX53_PAD_CSI0_DAT14__GPIO6_0				375
MX53_PAD_CSI0_DAT14__UART5_TXD_MUX			376
MX53_PAD_CSI0_DAT14__USBOH3_USBH3_DATA_2		377
MX53_PAD_CSI0_DAT14__SDMA_DEBUG_PC_8			378
MX53_PAD_CSI0_DAT14__EMI_EMI_DEBUG_43			379
MX53_PAD_CSI0_DAT14__TPIU_TRACE_11			380
MX53_PAD_CSI0_DAT15__IPU_CSI0_D_15			381
MX53_PAD_CSI0_DAT15__GPIO6_1				382
MX53_PAD_CSI0_DAT15__UART5_RXD_MUX			383
MX53_PAD_CSI0_DAT15__USBOH3_USBH3_DATA_3		384
MX53_PAD_CSI0_DAT15__SDMA_DEBUG_PC_9			385
MX53_PAD_CSI0_DAT15__EMI_EMI_DEBUG_44			386
MX53_PAD_CSI0_DAT15__TPIU_TRACE_12			387
MX53_PAD_CSI0_DAT16__IPU_CSI0_D_16			388
MX53_PAD_CSI0_DAT16__GPIO6_2				389
MX53_PAD_CSI0_DAT16__UART4_RTS				390
MX53_PAD_CSI0_DAT16__USBOH3_USBH3_DATA_4		391
MX53_PAD_CSI0_DAT16__SDMA_DEBUG_PC_10			392
MX53_PAD_CSI0_DAT16__EMI_EMI_DEBUG_45			393
MX53_PAD_CSI0_DAT16__TPIU_TRACE_13			394
MX53_PAD_CSI0_DAT17__IPU_CSI0_D_17			395
MX53_PAD_CSI0_DAT17__GPIO6_3				396
MX53_PAD_CSI0_DAT17__UART4_CTS				397
MX53_PAD_CSI0_DAT17__USBOH3_USBH3_DATA_5		398
MX53_PAD_CSI0_DAT17__SDMA_DEBUG_PC_11			399
MX53_PAD_CSI0_DAT17__EMI_EMI_DEBUG_46			400
MX53_PAD_CSI0_DAT17__TPIU_TRACE_14			401
MX53_PAD_CSI0_DAT18__IPU_CSI0_D_18			402
MX53_PAD_CSI0_DAT18__GPIO6_4				403
MX53_PAD_CSI0_DAT18__UART5_RTS				404
MX53_PAD_CSI0_DAT18__USBOH3_USBH3_DATA_6		405
MX53_PAD_CSI0_DAT18__SDMA_DEBUG_PC_12			406
MX53_PAD_CSI0_DAT18__EMI_EMI_DEBUG_47			407
MX53_PAD_CSI0_DAT18__TPIU_TRACE_15			408
MX53_PAD_CSI0_DAT19__IPU_CSI0_D_19			409
MX53_PAD_CSI0_DAT19__GPIO6_5				410
MX53_PAD_CSI0_DAT19__UART5_CTS				411
MX53_PAD_CSI0_DAT19__USBOH3_USBH3_DATA_7		412
MX53_PAD_CSI0_DAT19__SDMA_DEBUG_PC_13			413
MX53_PAD_CSI0_DAT19__EMI_EMI_DEBUG_48			414
MX53_PAD_CSI0_DAT19__USBPHY2_BISTOK			415
MX53_PAD_EIM_A25__EMI_WEIM_A_25				416
MX53_PAD_EIM_A25__GPIO5_2				417
MX53_PAD_EIM_A25__ECSPI2_RDY				418
MX53_PAD_EIM_A25__IPU_DI1_PIN12				419
MX53_PAD_EIM_A25__CSPI_SS1				420
MX53_PAD_EIM_A25__IPU_DI0_D1_CS				421
MX53_PAD_EIM_A25__USBPHY1_BISTOK			422
MX53_PAD_EIM_EB2__EMI_WEIM_EB_2				423
MX53_PAD_EIM_EB2__GPIO2_30				424
MX53_PAD_EIM_EB2__CCM_DI1_EXT_CLK			425
MX53_PAD_EIM_EB2__IPU_SER_DISP1_CS			426
MX53_PAD_EIM_EB2__ECSPI1_SS0				427
MX53_PAD_EIM_EB2__I2C2_SCL				428
MX53_PAD_EIM_D16__EMI_WEIM_D_16				429
MX53_PAD_EIM_D16__GPIO3_16				430
MX53_PAD_EIM_D16__IPU_DI0_PIN5				431
MX53_PAD_EIM_D16__IPU_DISPB1_SER_CLK			432
MX53_PAD_EIM_D16__ECSPI1_SCLK				433
MX53_PAD_EIM_D16__I2C2_SDA				434
MX53_PAD_EIM_D17__EMI_WEIM_D_17				435
MX53_PAD_EIM_D17__GPIO3_17				436
MX53_PAD_EIM_D17__IPU_DI0_PIN6				437
MX53_PAD_EIM_D17__IPU_DISPB1_SER_DIN			438
MX53_PAD_EIM_D17__ECSPI1_MISO				439
MX53_PAD_EIM_D17__I2C3_SCL				440
MX53_PAD_EIM_D18__EMI_WEIM_D_18				441
MX53_PAD_EIM_D18__GPIO3_18				442
MX53_PAD_EIM_D18__IPU_DI0_PIN7				443
MX53_PAD_EIM_D18__IPU_DISPB1_SER_DIO			444
MX53_PAD_EIM_D18__ECSPI1_MOSI				445
MX53_PAD_EIM_D18__I2C3_SDA				446
MX53_PAD_EIM_D18__IPU_DI1_D0_CS				447
MX53_PAD_EIM_D19__EMI_WEIM_D_19				448
MX53_PAD_EIM_D19__GPIO3_19				449
MX53_PAD_EIM_D19__IPU_DI0_PIN8				450
MX53_PAD_EIM_D19__IPU_DISPB1_SER_RS			451
MX53_PAD_EIM_D19__ECSPI1_SS1				452
MX53_PAD_EIM_D19__EPIT1_EPITO				453
MX53_PAD_EIM_D19__UART1_CTS				454
MX53_PAD_EIM_D19__USBOH3_USBH2_OC			455
MX53_PAD_EIM_D20__EMI_WEIM_D_20				456
MX53_PAD_EIM_D20__GPIO3_20				457
MX53_PAD_EIM_D20__IPU_DI0_PIN16				458
MX53_PAD_EIM_D20__IPU_SER_DISP0_CS			459
MX53_PAD_EIM_D20__CSPI_SS0				460
MX53_PAD_EIM_D20__EPIT2_EPITO				461
MX53_PAD_EIM_D20__UART1_RTS				462
MX53_PAD_EIM_D20__USBOH3_USBH2_PWR			463
MX53_PAD_EIM_D21__EMI_WEIM_D_21				464
MX53_PAD_EIM_D21__GPIO3_21				465
MX53_PAD_EIM_D21__IPU_DI0_PIN17				466
MX53_PAD_EIM_D21__IPU_DISPB0_SER_CLK			467
MX53_PAD_EIM_D21__CSPI_SCLK				468
MX53_PAD_EIM_D21__I2C1_SCL				469
MX53_PAD_EIM_D21__USBOH3_USBOTG_OC			470
MX53_PAD_EIM_D22__EMI_WEIM_D_22				471
MX53_PAD_EIM_D22__GPIO3_22				472
MX53_PAD_EIM_D22__IPU_DI0_PIN1				473
MX53_PAD_EIM_D22__IPU_DISPB0_SER_DIN			474
MX53_PAD_EIM_D22__CSPI_MISO				475
MX53_PAD_EIM_D22__USBOH3_USBOTG_PWR			476
MX53_PAD_EIM_D23__EMI_WEIM_D_23				477
MX53_PAD_EIM_D23__GPIO3_23				478
MX53_PAD_EIM_D23__UART3_CTS				479
MX53_PAD_EIM_D23__UART1_DCD				480
MX53_PAD_EIM_D23__IPU_DI0_D0_CS				481
MX53_PAD_EIM_D23__IPU_DI1_PIN2				482
MX53_PAD_EIM_D23__IPU_CSI1_DATA_EN			483
MX53_PAD_EIM_D23__IPU_DI1_PIN14				484
MX53_PAD_EIM_EB3__EMI_WEIM_EB_3				485
MX53_PAD_EIM_EB3__GPIO2_31				486
MX53_PAD_EIM_EB3__UART3_RTS				487
MX53_PAD_EIM_EB3__UART1_RI				488
MX53_PAD_EIM_EB3__IPU_DI1_PIN3				489
MX53_PAD_EIM_EB3__IPU_CSI1_HSYNC			490
MX53_PAD_EIM_EB3__IPU_DI1_PIN16				491
MX53_PAD_EIM_D24__EMI_WEIM_D_24				492
MX53_PAD_EIM_D24__GPIO3_24				493
MX53_PAD_EIM_D24__UART3_TXD_MUX				494
MX53_PAD_EIM_D24__ECSPI1_SS2				495
MX53_PAD_EIM_D24__CSPI_SS2				496
MX53_PAD_EIM_D24__AUDMUX_AUD5_RXFS			497
MX53_PAD_EIM_D24__ECSPI2_SS2				498
MX53_PAD_EIM_D24__UART1_DTR				499
MX53_PAD_EIM_D25__EMI_WEIM_D_25				500
MX53_PAD_EIM_D25__GPIO3_25				501
MX53_PAD_EIM_D25__UART3_RXD_MUX				502
MX53_PAD_EIM_D25__ECSPI1_SS3				503
MX53_PAD_EIM_D25__CSPI_SS3				504
MX53_PAD_EIM_D25__AUDMUX_AUD5_RXC			505
MX53_PAD_EIM_D25__ECSPI2_SS3				506
MX53_PAD_EIM_D25__UART1_DSR				507
MX53_PAD_EIM_D26__EMI_WEIM_D_26				508
MX53_PAD_EIM_D26__GPIO3_26				509
MX53_PAD_EIM_D26__UART2_TXD_MUX				510
MX53_PAD_EIM_D26__FIRI_RXD				511
MX53_PAD_EIM_D26__IPU_CSI0_D_1				512
MX53_PAD_EIM_D26__IPU_DI1_PIN11				513
MX53_PAD_EIM_D26__IPU_SISG_2				514
MX53_PAD_EIM_D26__IPU_DISP1_DAT_22			515
MX53_PAD_EIM_D27__EMI_WEIM_D_27				516
MX53_PAD_EIM_D27__GPIO3_27				517
MX53_PAD_EIM_D27__UART2_RXD_MUX				518
MX53_PAD_EIM_D27__FIRI_TXD				519
MX53_PAD_EIM_D27__IPU_CSI0_D_0				520
MX53_PAD_EIM_D27__IPU_DI1_PIN13				521
MX53_PAD_EIM_D27__IPU_SISG_3				522
MX53_PAD_EIM_D27__IPU_DISP1_DAT_23			523
MX53_PAD_EIM_D28__EMI_WEIM_D_28				524
MX53_PAD_EIM_D28__GPIO3_28				525
MX53_PAD_EIM_D28__UART2_CTS				526
MX53_PAD_EIM_D28__IPU_DISPB0_SER_DIO			527
MX53_PAD_EIM_D28__CSPI_MOSI				528
MX53_PAD_EIM_D28__I2C1_SDA				529
MX53_PAD_EIM_D28__IPU_EXT_TRIG				530
MX53_PAD_EIM_D28__IPU_DI0_PIN13				531
MX53_PAD_EIM_D29__EMI_WEIM_D_29				532
MX53_PAD_EIM_D29__GPIO3_29				533
MX53_PAD_EIM_D29__UART2_RTS				534
MX53_PAD_EIM_D29__IPU_DISPB0_SER_RS			535
MX53_PAD_EIM_D29__CSPI_SS0				536
MX53_PAD_EIM_D29__IPU_DI1_PIN15				537
MX53_PAD_EIM_D29__IPU_CSI1_VSYNC			538
MX53_PAD_EIM_D29__IPU_DI0_PIN14				539
MX53_PAD_EIM_D30__EMI_WEIM_D_30				540
MX53_PAD_EIM_D30__GPIO3_30				541
MX53_PAD_EIM_D30__UART3_CTS				542
MX53_PAD_EIM_D30__IPU_CSI0_D_3				543
MX53_PAD_EIM_D30__IPU_DI0_PIN11				544
MX53_PAD_EIM_D30__IPU_DISP1_DAT_21			545
MX53_PAD_EIM_D30__USBOH3_USBH1_OC			546
MX53_PAD_EIM_D30__USBOH3_USBH2_OC			547
MX53_PAD_EIM_D31__EMI_WEIM_D_31				548
MX53_PAD_EIM_D31__GPIO3_31				549
MX53_PAD_EIM_D31__UART3_RTS				550
MX53_PAD_EIM_D31__IPU_CSI0_D_2				551
MX53_PAD_EIM_D31__IPU_DI0_PIN12				552
MX53_PAD_EIM_D31__IPU_DISP1_DAT_20			553
MX53_PAD_EIM_D31__USBOH3_USBH1_PWR			554
MX53_PAD_EIM_D31__USBOH3_USBH2_PWR			555
MX53_PAD_EIM_A24__EMI_WEIM_A_24				556
MX53_PAD_EIM_A24__GPIO5_4				557
MX53_PAD_EIM_A24__IPU_DISP1_DAT_19			558
MX53_PAD_EIM_A24__IPU_CSI1_D_19				559
MX53_PAD_EIM_A24__IPU_SISG_2				560
MX53_PAD_EIM_A24__USBPHY2_BVALID			561
MX53_PAD_EIM_A23__EMI_WEIM_A_23				562
MX53_PAD_EIM_A23__GPIO6_6				563
MX53_PAD_EIM_A23__IPU_DISP1_DAT_18			564
MX53_PAD_EIM_A23__IPU_CSI1_D_18				565
MX53_PAD_EIM_A23__IPU_SISG_3				566
MX53_PAD_EIM_A23__USBPHY2_ENDSESSION			567
MX53_PAD_EIM_A22__EMI_WEIM_A_22				568
MX53_PAD_EIM_A22__GPIO2_16				569
MX53_PAD_EIM_A22__IPU_DISP1_DAT_17			570
MX53_PAD_EIM_A22__IPU_CSI1_D_17				571
MX53_PAD_EIM_A22__SRC_BT_CFG1_7				572
MX53_PAD_EIM_A21__EMI_WEIM_A_21				573
MX53_PAD_EIM_A21__GPIO2_17				574
MX53_PAD_EIM_A21__IPU_DISP1_DAT_16			575
MX53_PAD_EIM_A21__IPU_CSI1_D_16				576
MX53_PAD_EIM_A21__SRC_BT_CFG1_6				577
MX53_PAD_EIM_A20__EMI_WEIM_A_20				578
MX53_PAD_EIM_A20__GPIO2_18				579
MX53_PAD_EIM_A20__IPU_DISP1_DAT_15			580
MX53_PAD_EIM_A20__IPU_CSI1_D_15				581
MX53_PAD_EIM_A20__SRC_BT_CFG1_5				582
MX53_PAD_EIM_A19__EMI_WEIM_A_19				583
MX53_PAD_EIM_A19__GPIO2_19				584
MX53_PAD_EIM_A19__IPU_DISP1_DAT_14			585
MX53_PAD_EIM_A19__IPU_CSI1_D_14				586
MX53_PAD_EIM_A19__SRC_BT_CFG1_4				587
MX53_PAD_EIM_A18__EMI_WEIM_A_18				588
MX53_PAD_EIM_A18__GPIO2_20				589
MX53_PAD_EIM_A18__IPU_DISP1_DAT_13			590
MX53_PAD_EIM_A18__IPU_CSI1_D_13				591
MX53_PAD_EIM_A18__SRC_BT_CFG1_3				592
MX53_PAD_EIM_A17__EMI_WEIM_A_17				593
MX53_PAD_EIM_A17__GPIO2_21				594
MX53_PAD_EIM_A17__IPU_DISP1_DAT_12			595
MX53_PAD_EIM_A17__IPU_CSI1_D_12				596
MX53_PAD_EIM_A17__SRC_BT_CFG1_2				597
MX53_PAD_EIM_A16__EMI_WEIM_A_16				598
MX53_PAD_EIM_A16__GPIO2_22				599
MX53_PAD_EIM_A16__IPU_DI1_DISP_CLK			600
MX53_PAD_EIM_A16__IPU_CSI1_PIXCLK			601
MX53_PAD_EIM_A16__SRC_BT_CFG1_1				602
MX53_PAD_EIM_CS0__EMI_WEIM_CS_0				603
MX53_PAD_EIM_CS0__GPIO2_23				604
MX53_PAD_EIM_CS0__ECSPI2_SCLK				605
MX53_PAD_EIM_CS0__IPU_DI1_PIN5				606
MX53_PAD_EIM_CS1__EMI_WEIM_CS_1				607
MX53_PAD_EIM_CS1__GPIO2_24				608
MX53_PAD_EIM_CS1__ECSPI2_MOSI				609
MX53_PAD_EIM_CS1__IPU_DI1_PIN6				610
MX53_PAD_EIM_OE__EMI_WEIM_OE				611
MX53_PAD_EIM_OE__GPIO2_25				612
MX53_PAD_EIM_OE__ECSPI2_MISO				613
MX53_PAD_EIM_OE__IPU_DI1_PIN7				614
MX53_PAD_EIM_OE__USBPHY2_IDDIG				615
MX53_PAD_EIM_RW__EMI_WEIM_RW				616
MX53_PAD_EIM_RW__GPIO2_26				617
MX53_PAD_EIM_RW__ECSPI2_SS0				618
MX53_PAD_EIM_RW__IPU_DI1_PIN8				619
MX53_PAD_EIM_RW__USBPHY2_HOSTDISCONNECT			620
MX53_PAD_EIM_LBA__EMI_WEIM_LBA				621
MX53_PAD_EIM_LBA__GPIO2_27				622
MX53_PAD_EIM_LBA__ECSPI2_SS1				623
MX53_PAD_EIM_LBA__IPU_DI1_PIN17				624
MX53_PAD_EIM_LBA__SRC_BT_CFG1_0				625
MX53_PAD_EIM_EB0__EMI_WEIM_EB_0				626
MX53_PAD_EIM_EB0__GPIO2_28				627
MX53_PAD_EIM_EB0__IPU_DISP1_DAT_11			628
MX53_PAD_EIM_EB0__IPU_CSI1_D_11				629
MX53_PAD_EIM_EB0__GPC_PMIC_RDY				630
MX53_PAD_EIM_EB0__SRC_BT_CFG2_7				631
MX53_PAD_EIM_EB1__EMI_WEIM_EB_1				632
MX53_PAD_EIM_EB1__GPIO2_29				633
MX53_PAD_EIM_EB1__IPU_DISP1_DAT_10			634
MX53_PAD_EIM_EB1__IPU_CSI1_D_10				635
MX53_PAD_EIM_EB1__SRC_BT_CFG2_6				636
MX53_PAD_EIM_DA0__EMI_NAND_WEIM_DA_0			637
MX53_PAD_EIM_DA0__GPIO3_0				638
MX53_PAD_EIM_DA0__IPU_DISP1_DAT_9			639
MX53_PAD_EIM_DA0__IPU_CSI1_D_9				640
MX53_PAD_EIM_DA0__SRC_BT_CFG2_5				641
MX53_PAD_EIM_DA1__EMI_NAND_WEIM_DA_1			642
MX53_PAD_EIM_DA1__GPIO3_1				643
MX53_PAD_EIM_DA1__IPU_DISP1_DAT_8			644
MX53_PAD_EIM_DA1__IPU_CSI1_D_8				645
MX53_PAD_EIM_DA1__SRC_BT_CFG2_4				646
MX53_PAD_EIM_DA2__EMI_NAND_WEIM_DA_2			647
MX53_PAD_EIM_DA2__GPIO3_2				648
MX53_PAD_EIM_DA2__IPU_DISP1_DAT_7			649
MX53_PAD_EIM_DA2__IPU_CSI1_D_7				650
MX53_PAD_EIM_DA2__SRC_BT_CFG2_3				651
MX53_PAD_EIM_DA3__EMI_NAND_WEIM_DA_3			652
MX53_PAD_EIM_DA3__GPIO3_3				653
MX53_PAD_EIM_DA3__IPU_DISP1_DAT_6			654
MX53_PAD_EIM_DA3__IPU_CSI1_D_6				655
MX53_PAD_EIM_DA3__SRC_BT_CFG2_2				656
MX53_PAD_EIM_DA4__EMI_NAND_WEIM_DA_4			657
MX53_PAD_EIM_DA4__GPIO3_4				658
MX53_PAD_EIM_DA4__IPU_DISP1_DAT_5			659
MX53_PAD_EIM_DA4__IPU_CSI1_D_5				660
MX53_PAD_EIM_DA4__SRC_BT_CFG3_7				661
MX53_PAD_EIM_DA5__EMI_NAND_WEIM_DA_5			662
MX53_PAD_EIM_DA5__GPIO3_5				663
MX53_PAD_EIM_DA5__IPU_DISP1_DAT_4			664
MX53_PAD_EIM_DA5__IPU_CSI1_D_4				665
MX53_PAD_EIM_DA5__SRC_BT_CFG3_6				666
MX53_PAD_EIM_DA6__EMI_NAND_WEIM_DA_6			667
MX53_PAD_EIM_DA6__GPIO3_6				668
MX53_PAD_EIM_DA6__IPU_DISP1_DAT_3			669
MX53_PAD_EIM_DA6__IPU_CSI1_D_3				670
MX53_PAD_EIM_DA6__SRC_BT_CFG3_5				671
MX53_PAD_EIM_DA7__EMI_NAND_WEIM_DA_7			672
MX53_PAD_EIM_DA7__GPIO3_7				673
MX53_PAD_EIM_DA7__IPU_DISP1_DAT_2			674
MX53_PAD_EIM_DA7__IPU_CSI1_D_2				675
MX53_PAD_EIM_DA7__SRC_BT_CFG3_4				676
MX53_PAD_EIM_DA8__EMI_NAND_WEIM_DA_8			677
MX53_PAD_EIM_DA8__GPIO3_8				678
MX53_PAD_EIM_DA8__IPU_DISP1_DAT_1			679
MX53_PAD_EIM_DA8__IPU_CSI1_D_1				680
MX53_PAD_EIM_DA8__SRC_BT_CFG3_3				681
MX53_PAD_EIM_DA9__EMI_NAND_WEIM_DA_9			682
MX53_PAD_EIM_DA9__GPIO3_9				683
MX53_PAD_EIM_DA9__IPU_DISP1_DAT_0			684
MX53_PAD_EIM_DA9__IPU_CSI1_D_0				685
MX53_PAD_EIM_DA9__SRC_BT_CFG3_2				686
MX53_PAD_EIM_DA10__EMI_NAND_WEIM_DA_10			687
MX53_PAD_EIM_DA10__GPIO3_10				688
MX53_PAD_EIM_DA10__IPU_DI1_PIN15			689
MX53_PAD_EIM_DA10__IPU_CSI1_DATA_EN			690
MX53_PAD_EIM_DA10__SRC_BT_CFG3_1			691
MX53_PAD_EIM_DA11__EMI_NAND_WEIM_DA_11			692
MX53_PAD_EIM_DA11__GPIO3_11				693
MX53_PAD_EIM_DA11__IPU_DI1_PIN2				694
MX53_PAD_EIM_DA11__IPU_CSI1_HSYNC			695
MX53_PAD_EIM_DA12__EMI_NAND_WEIM_DA_12			696
MX53_PAD_EIM_DA12__GPIO3_12				697
MX53_PAD_EIM_DA12__IPU_DI1_PIN3				698
MX53_PAD_EIM_DA12__IPU_CSI1_VSYNC			699
MX53_PAD_EIM_DA13__EMI_NAND_WEIM_DA_13			700
MX53_PAD_EIM_DA13__GPIO3_13				701
MX53_PAD_EIM_DA13__IPU_DI1_D0_CS			702
MX53_PAD_EIM_DA13__CCM_DI1_EXT_CLK			703
MX53_PAD_EIM_DA14__EMI_NAND_WEIM_DA_14			704
MX53_PAD_EIM_DA14__GPIO3_14				705
MX53_PAD_EIM_DA14__IPU_DI1_D1_CS			706
MX53_PAD_EIM_DA14__CCM_DI0_EXT_CLK			707
MX53_PAD_EIM_DA15__EMI_NAND_WEIM_DA_15			708
MX53_PAD_EIM_DA15__GPIO3_15				709
MX53_PAD_EIM_DA15__IPU_DI1_PIN1				710
MX53_PAD_EIM_DA15__IPU_DI1_PIN4				711
MX53_PAD_NANDF_WE_B__EMI_NANDF_WE_B			712
MX53_PAD_NANDF_WE_B__GPIO6_12				713
MX53_PAD_NANDF_RE_B__EMI_NANDF_RE_B			714
MX53_PAD_NANDF_RE_B__GPIO6_13				715
MX53_PAD_EIM_WAIT__EMI_WEIM_WAIT			716
MX53_PAD_EIM_WAIT__GPIO5_0				717
MX53_PAD_EIM_WAIT__EMI_WEIM_DTACK_B			718
MX53_PAD_LVDS1_TX3_P__GPIO6_22				719
MX53_PAD_LVDS1_TX3_P__LDB_LVDS1_TX3			720
MX53_PAD_LVDS1_TX2_P__GPIO6_24				721
MX53_PAD_LVDS1_TX2_P__LDB_LVDS1_TX2			722
MX53_PAD_LVDS1_CLK_P__GPIO6_26				723
MX53_PAD_LVDS1_CLK_P__LDB_LVDS1_CLK			724
MX53_PAD_LVDS1_TX1_P__GPIO6_28				725
MX53_PAD_LVDS1_TX1_P__LDB_LVDS1_TX1			726
MX53_PAD_LVDS1_TX0_P__GPIO6_30				727
MX53_PAD_LVDS1_TX0_P__LDB_LVDS1_TX0			728
MX53_PAD_LVDS0_TX3_P__GPIO7_22				729
MX53_PAD_LVDS0_TX3_P__LDB_LVDS0_TX3			730
MX53_PAD_LVDS0_CLK_P__GPIO7_24				731
MX53_PAD_LVDS0_CLK_P__LDB_LVDS0_CLK			732
MX53_PAD_LVDS0_TX2_P__GPIO7_26				733
MX53_PAD_LVDS0_TX2_P__LDB_LVDS0_TX2			734
MX53_PAD_LVDS0_TX1_P__GPIO7_28				735
MX53_PAD_LVDS0_TX1_P__LDB_LVDS0_TX1			736
MX53_PAD_LVDS0_TX0_P__GPIO7_30				737
MX53_PAD_LVDS0_TX0_P__LDB_LVDS0_TX0			738
MX53_PAD_GPIO_10__GPIO4_0				739
MX53_PAD_GPIO_10__OSC32k_32K_OUT			740
MX53_PAD_GPIO_11__GPIO4_1				741
MX53_PAD_GPIO_12__GPIO4_2				742
MX53_PAD_GPIO_13__GPIO4_3				743
MX53_PAD_GPIO_14__GPIO4_4				744
MX53_PAD_NANDF_CLE__EMI_NANDF_CLE			745
MX53_PAD_NANDF_CLE__GPIO6_7				746
MX53_PAD_NANDF_CLE__USBPHY1_VSTATUS_0			747
MX53_PAD_NANDF_ALE__EMI_NANDF_ALE			748
MX53_PAD_NANDF_ALE__GPIO6_8				749
MX53_PAD_NANDF_ALE__USBPHY1_VSTATUS_1			750
MX53_PAD_NANDF_WP_B__EMI_NANDF_WP_B			751
MX53_PAD_NANDF_WP_B__GPIO6_9				752
MX53_PAD_NANDF_WP_B__USBPHY1_VSTATUS_2			753
MX53_PAD_NANDF_RB0__EMI_NANDF_RB_0			754
MX53_PAD_NANDF_RB0__GPIO6_10				755
MX53_PAD_NANDF_RB0__USBPHY1_VSTATUS_3			756
MX53_PAD_NANDF_CS0__EMI_NANDF_CS_0			757
MX53_PAD_NANDF_CS0__GPIO6_11				758
MX53_PAD_NANDF_CS0__USBPHY1_VSTATUS_4			759
MX53_PAD_NANDF_CS1__EMI_NANDF_CS_1			760
MX53_PAD_NANDF_CS1__GPIO6_14				761
MX53_PAD_NANDF_CS1__MLB_MLBCLK				762
MX53_PAD_NANDF_CS1__USBPHY1_VSTATUS_5			763
MX53_PAD_NANDF_CS2__EMI_NANDF_CS_2			764
MX53_PAD_NANDF_CS2__GPIO6_15				765
MX53_PAD_NANDF_CS2__IPU_SISG_0				766
MX53_PAD_NANDF_CS2__ESAI1_TX0				767
MX53_PAD_NANDF_CS2__EMI_WEIM_CRE			768
MX53_PAD_NANDF_CS2__CCM_CSI0_MCLK			769
MX53_PAD_NANDF_CS2__MLB_MLBSIG				770
MX53_PAD_NANDF_CS2__USBPHY1_VSTATUS_6			771
MX53_PAD_NANDF_CS3__EMI_NANDF_CS_3			772
MX53_PAD_NANDF_CS3__GPIO6_16				773
MX53_PAD_NANDF_CS3__IPU_SISG_1				774
MX53_PAD_NANDF_CS3__ESAI1_TX1				775
MX53_PAD_NANDF_CS3__EMI_WEIM_A_26			776
MX53_PAD_NANDF_CS3__MLB_MLBDAT				777
MX53_PAD_NANDF_CS3__USBPHY1_VSTATUS_7			778
MX53_PAD_FEC_MDIO__FEC_MDIO				779
MX53_PAD_FEC_MDIO__GPIO1_22				780
MX53_PAD_FEC_MDIO__ESAI1_SCKR				781
MX53_PAD_FEC_MDIO__FEC_COL				782
MX53_PAD_FEC_MDIO__RTC_CE_RTC_PS2			783
MX53_PAD_FEC_MDIO__SDMA_DEBUG_BUS_DEVICE_3		784
MX53_PAD_FEC_MDIO__EMI_EMI_DEBUG_49			785
MX53_PAD_FEC_REF_CLK__FEC_TX_CLK			786
MX53_PAD_FEC_REF_CLK__GPIO1_23				787
MX53_PAD_FEC_REF_CLK__ESAI1_FSR				788
MX53_PAD_FEC_REF_CLK__SDMA_DEBUG_BUS_DEVICE_4		789
MX53_PAD_FEC_REF_CLK__EMI_EMI_DEBUG_50			790
MX53_PAD_FEC_RX_ER__FEC_RX_ER				791
MX53_PAD_FEC_RX_ER__GPIO1_24				792
MX53_PAD_FEC_RX_ER__ESAI1_HCKR				793
MX53_PAD_FEC_RX_ER__FEC_RX_CLK				794
MX53_PAD_FEC_RX_ER__RTC_CE_RTC_PS3			795
MX53_PAD_FEC_CRS_DV__FEC_RX_DV				796
MX53_PAD_FEC_CRS_DV__GPIO1_25				797
MX53_PAD_FEC_CRS_DV__ESAI1_SCKT				798
MX53_PAD_FEC_RXD1__FEC_RDATA_1				799
MX53_PAD_FEC_RXD1__GPIO1_26				800
MX53_PAD_FEC_RXD1__ESAI1_FST				801
MX53_PAD_FEC_RXD1__MLB_MLBSIG				802
MX53_PAD_FEC_RXD1__RTC_CE_RTC_PS1			803
MX53_PAD_FEC_RXD0__FEC_RDATA_0				804
MX53_PAD_FEC_RXD0__GPIO1_27				805
MX53_PAD_FEC_RXD0__ESAI1_HCKT				806
MX53_PAD_FEC_RXD0__OSC32k_32K_OUT			807
MX53_PAD_FEC_TX_EN__FEC_TX_EN				808
MX53_PAD_FEC_TX_EN__GPIO1_28				809
MX53_PAD_FEC_TX_EN__ESAI1_TX3_RX2			810
MX53_PAD_FEC_TXD1__FEC_TDATA_1				811
MX53_PAD_FEC_TXD1__GPIO1_29				812
MX53_PAD_FEC_TXD1__ESAI1_TX2_RX3			813
MX53_PAD_FEC_TXD1__MLB_MLBCLK				814
MX53_PAD_FEC_TXD1__RTC_CE_RTC_PRSC_CLK			815
MX53_PAD_FEC_TXD0__FEC_TDATA_0				816
MX53_PAD_FEC_TXD0__GPIO1_30				817
MX53_PAD_FEC_TXD0__ESAI1_TX4_RX1			818
MX53_PAD_FEC_TXD0__USBPHY2_DATAOUT_0			819
MX53_PAD_FEC_MDC__FEC_MDC				820
MX53_PAD_FEC_MDC__GPIO1_31				821
MX53_PAD_FEC_MDC__ESAI1_TX5_RX0				822
MX53_PAD_FEC_MDC__MLB_MLBDAT				823
MX53_PAD_FEC_MDC__RTC_CE_RTC_ALARM1_TRIG		824
MX53_PAD_FEC_MDC__USBPHY2_DATAOUT_1			825
MX53_PAD_PATA_DIOW__PATA_DIOW				826
MX53_PAD_PATA_DIOW__GPIO6_17				827
MX53_PAD_PATA_DIOW__UART1_TXD_MUX			828
MX53_PAD_PATA_DIOW__USBPHY2_DATAOUT_2			829
MX53_PAD_PATA_DMACK__PATA_DMACK				830
MX53_PAD_PATA_DMACK__GPIO6_18				831
MX53_PAD_PATA_DMACK__UART1_RXD_MUX			832
MX53_PAD_PATA_DMACK__USBPHY2_DATAOUT_3			833
MX53_PAD_PATA_DMARQ__PATA_DMARQ				834
MX53_PAD_PATA_DMARQ__GPIO7_0				835
MX53_PAD_PATA_DMARQ__UART2_TXD_MUX			836
MX53_PAD_PATA_DMARQ__CCM_CCM_OUT_0			837
MX53_PAD_PATA_DMARQ__USBPHY2_DATAOUT_4			838
MX53_PAD_PATA_BUFFER_EN__PATA_BUFFER_EN			839
MX53_PAD_PATA_BUFFER_EN__GPIO7_1			840
MX53_PAD_PATA_BUFFER_EN__UART2_RXD_MUX			841
MX53_PAD_PATA_BUFFER_EN__CCM_CCM_OUT_1			842
MX53_PAD_PATA_BUFFER_EN__USBPHY2_DATAOUT_5		843
MX53_PAD_PATA_INTRQ__PATA_INTRQ				844
MX53_PAD_PATA_INTRQ__GPIO7_2				845
MX53_PAD_PATA_INTRQ__UART2_CTS				846
MX53_PAD_PATA_INTRQ__CAN1_TXCAN				847
MX53_PAD_PATA_INTRQ__CCM_CCM_OUT_2			848
MX53_PAD_PATA_INTRQ__USBPHY2_DATAOUT_6			849
MX53_PAD_PATA_DIOR__PATA_DIOR				850
MX53_PAD_PATA_DIOR__GPIO7_3				851
MX53_PAD_PATA_DIOR__UART2_RTS				852
MX53_PAD_PATA_DIOR__CAN1_RXCAN				853
MX53_PAD_PATA_DIOR__USBPHY2_DATAOUT_7			854
MX53_PAD_PATA_RESET_B__PATA_PATA_RESET_B		855
MX53_PAD_PATA_RESET_B__GPIO7_4				856
MX53_PAD_PATA_RESET_B__ESDHC3_CMD			857
MX53_PAD_PATA_RESET_B__UART1_CTS			858
MX53_PAD_PATA_RESET_B__CAN2_TXCAN			859
MX53_PAD_PATA_RESET_B__USBPHY1_DATAOUT_0		860
MX53_PAD_PATA_IORDY__PATA_IORDY				861
MX53_PAD_PATA_IORDY__GPIO7_5				862
MX53_PAD_PATA_IORDY__ESDHC3_CLK				863
MX53_PAD_PATA_IORDY__UART1_RTS				864
MX53_PAD_PATA_IORDY__CAN2_RXCAN				865
MX53_PAD_PATA_IORDY__USBPHY1_DATAOUT_1			866
MX53_PAD_PATA_DA_0__PATA_DA_0				867
MX53_PAD_PATA_DA_0__GPIO7_6				868
MX53_PAD_PATA_DA_0__ESDHC3_RST				869
MX53_PAD_PATA_DA_0__OWIRE_LINE				870
MX53_PAD_PATA_DA_0__USBPHY1_DATAOUT_2			871
MX53_PAD_PATA_DA_1__PATA_DA_1				872
MX53_PAD_PATA_DA_1__GPIO7_7				873
MX53_PAD_PATA_DA_1__ESDHC4_CMD				874
MX53_PAD_PATA_DA_1__UART3_CTS				875
MX53_PAD_PATA_DA_1__USBPHY1_DATAOUT_3			876
MX53_PAD_PATA_DA_2__PATA_DA_2				877
MX53_PAD_PATA_DA_2__GPIO7_8				878
MX53_PAD_PATA_DA_2__ESDHC4_CLK				879
MX53_PAD_PATA_DA_2__UART3_RTS				880
MX53_PAD_PATA_DA_2__USBPHY1_DATAOUT_4			881
MX53_PAD_PATA_CS_0__PATA_CS_0				882
MX53_PAD_PATA_CS_0__GPIO7_9				883
MX53_PAD_PATA_CS_0__UART3_TXD_MUX			884
MX53_PAD_PATA_CS_0__USBPHY1_DATAOUT_5			885
MX53_PAD_PATA_CS_1__PATA_CS_1				886
MX53_PAD_PATA_CS_1__GPIO7_10				887
MX53_PAD_PATA_CS_1__UART3_RXD_MUX			888
MX53_PAD_PATA_CS_1__USBPHY1_DATAOUT_6			889
MX53_PAD_PATA_DATA0__PATA_DATA_0			890
MX53_PAD_PATA_DATA0__GPIO2_0				891
MX53_PAD_PATA_DATA0__EMI_NANDF_D_0			892
MX53_PAD_PATA_DATA0__ESDHC3_DAT4			893
MX53_PAD_PATA_DATA0__GPU3d_GPU_DEBUG_OUT_0		894
MX53_PAD_PATA_DATA0__IPU_DIAG_BUS_0			895
MX53_PAD_PATA_DATA0__USBPHY1_DATAOUT_7			896
MX53_PAD_PATA_DATA1__PATA_DATA_1			897
MX53_PAD_PATA_DATA1__GPIO2_1				898
MX53_PAD_PATA_DATA1__EMI_NANDF_D_1			899
MX53_PAD_PATA_DATA1__ESDHC3_DAT5			900
MX53_PAD_PATA_DATA1__GPU3d_GPU_DEBUG_OUT_1		901
MX53_PAD_PATA_DATA1__IPU_DIAG_BUS_1			902
MX53_PAD_PATA_DATA2__PATA_DATA_2			903
MX53_PAD_PATA_DATA2__GPIO2_2				904
MX53_PAD_PATA_DATA2__EMI_NANDF_D_2			905
MX53_PAD_PATA_DATA2__ESDHC3_DAT6			906
MX53_PAD_PATA_DATA2__GPU3d_GPU_DEBUG_OUT_2		907
MX53_PAD_PATA_DATA2__IPU_DIAG_BUS_2			908
MX53_PAD_PATA_DATA3__PATA_DATA_3			909
MX53_PAD_PATA_DATA3__GPIO2_3				910
MX53_PAD_PATA_DATA3__EMI_NANDF_D_3			911
MX53_PAD_PATA_DATA3__ESDHC3_DAT7			912
MX53_PAD_PATA_DATA3__GPU3d_GPU_DEBUG_OUT_3		913
MX53_PAD_PATA_DATA3__IPU_DIAG_BUS_3			914
MX53_PAD_PATA_DATA4__PATA_DATA_4			915
MX53_PAD_PATA_DATA4__GPIO2_4				916
MX53_PAD_PATA_DATA4__EMI_NANDF_D_4			917
MX53_PAD_PATA_DATA4__ESDHC4_DAT4			918
MX53_PAD_PATA_DATA4__GPU3d_GPU_DEBUG_OUT_4		919
MX53_PAD_PATA_DATA4__IPU_DIAG_BUS_4			920
MX53_PAD_PATA_DATA5__PATA_DATA_5			921
MX53_PAD_PATA_DATA5__GPIO2_5				922
MX53_PAD_PATA_DATA5__EMI_NANDF_D_5			923
MX53_PAD_PATA_DATA5__ESDHC4_DAT5			924
MX53_PAD_PATA_DATA5__GPU3d_GPU_DEBUG_OUT_5		925
MX53_PAD_PATA_DATA5__IPU_DIAG_BUS_5			926
MX53_PAD_PATA_DATA6__PATA_DATA_6			927
MX53_PAD_PATA_DATA6__GPIO2_6				928
MX53_PAD_PATA_DATA6__EMI_NANDF_D_6			929
MX53_PAD_PATA_DATA6__ESDHC4_DAT6			930
MX53_PAD_PATA_DATA6__GPU3d_GPU_DEBUG_OUT_6		931
MX53_PAD_PATA_DATA6__IPU_DIAG_BUS_6			932
MX53_PAD_PATA_DATA7__PATA_DATA_7			933
MX53_PAD_PATA_DATA7__GPIO2_7				934
MX53_PAD_PATA_DATA7__EMI_NANDF_D_7			935
MX53_PAD_PATA_DATA7__ESDHC4_DAT7			936
MX53_PAD_PATA_DATA7__GPU3d_GPU_DEBUG_OUT_7		937
MX53_PAD_PATA_DATA7__IPU_DIAG_BUS_7			938
MX53_PAD_PATA_DATA8__PATA_DATA_8			939
MX53_PAD_PATA_DATA8__GPIO2_8				940
MX53_PAD_PATA_DATA8__ESDHC1_DAT4			941
MX53_PAD_PATA_DATA8__EMI_NANDF_D_8			942
MX53_PAD_PATA_DATA8__ESDHC3_DAT0			943
MX53_PAD_PATA_DATA8__GPU3d_GPU_DEBUG_OUT_8		944
MX53_PAD_PATA_DATA8__IPU_DIAG_BUS_8			945
MX53_PAD_PATA_DATA9__PATA_DATA_9			946
MX53_PAD_PATA_DATA9__GPIO2_9				947
MX53_PAD_PATA_DATA9__ESDHC1_DAT5			948
MX53_PAD_PATA_DATA9__EMI_NANDF_D_9			949
MX53_PAD_PATA_DATA9__ESDHC3_DAT1			950
MX53_PAD_PATA_DATA9__GPU3d_GPU_DEBUG_OUT_9		951
MX53_PAD_PATA_DATA9__IPU_DIAG_BUS_9			952
MX53_PAD_PATA_DATA10__PATA_DATA_10			953
MX53_PAD_PATA_DATA10__GPIO2_10				954
MX53_PAD_PATA_DATA10__ESDHC1_DAT6			955
MX53_PAD_PATA_DATA10__EMI_NANDF_D_10			956
MX53_PAD_PATA_DATA10__ESDHC3_DAT2			957
MX53_PAD_PATA_DATA10__GPU3d_GPU_DEBUG_OUT_10		958
MX53_PAD_PATA_DATA10__IPU_DIAG_BUS_10			959
MX53_PAD_PATA_DATA11__PATA_DATA_11			960
MX53_PAD_PATA_DATA11__GPIO2_11				961
MX53_PAD_PATA_DATA11__ESDHC1_DAT7			962
MX53_PAD_PATA_DATA11__EMI_NANDF_D_11			963
MX53_PAD_PATA_DATA11__ESDHC3_DAT3			964
MX53_PAD_PATA_DATA11__GPU3d_GPU_DEBUG_OUT_11		965
MX53_PAD_PATA_DATA11__IPU_DIAG_BUS_11			966
MX53_PAD_PATA_DATA12__PATA_DATA_12			967
MX53_PAD_PATA_DATA12__GPIO2_12				968
MX53_PAD_PATA_DATA12__ESDHC2_DAT4			969
MX53_PAD_PATA_DATA12__EMI_NANDF_D_12			970
MX53_PAD_PATA_DATA12__ESDHC4_DAT0			971
MX53_PAD_PATA_DATA12__GPU3d_GPU_DEBUG_OUT_12		972
MX53_PAD_PATA_DATA12__IPU_DIAG_BUS_12			973
MX53_PAD_PATA_DATA13__PATA_DATA_13			974
MX53_PAD_PATA_DATA13__GPIO2_13				975
MX53_PAD_PATA_DATA13__ESDHC2_DAT5			976
MX53_PAD_PATA_DATA13__EMI_NANDF_D_13			977
MX53_PAD_PATA_DATA13__ESDHC4_DAT1			978
MX53_PAD_PATA_DATA13__GPU3d_GPU_DEBUG_OUT_13		979
MX53_PAD_PATA_DATA13__IPU_DIAG_BUS_13			980
MX53_PAD_PATA_DATA14__PATA_DATA_14			981
MX53_PAD_PATA_DATA14__GPIO2_14				982
MX53_PAD_PATA_DATA14__ESDHC2_DAT6			983
MX53_PAD_PATA_DATA14__EMI_NANDF_D_14			984
MX53_PAD_PATA_DATA14__ESDHC4_DAT2			985
MX53_PAD_PATA_DATA14__GPU3d_GPU_DEBUG_OUT_14		986
MX53_PAD_PATA_DATA14__IPU_DIAG_BUS_14			987
MX53_PAD_PATA_DATA15__PATA_DATA_15			988
MX53_PAD_PATA_DATA15__GPIO2_15				989
MX53_PAD_PATA_DATA15__ESDHC2_DAT7			990
MX53_PAD_PATA_DATA15__EMI_NANDF_D_15			991
MX53_PAD_PATA_DATA15__ESDHC4_DAT3			992
MX53_PAD_PATA_DATA15__GPU3d_GPU_DEBUG_OUT_15		993
MX53_PAD_PATA_DATA15__IPU_DIAG_BUS_15			994
MX53_PAD_SD1_DATA0__ESDHC1_DAT0				995
MX53_PAD_SD1_DATA0__GPIO1_16				996
MX53_PAD_SD1_DATA0__GPT_CAPIN1				997
MX53_PAD_SD1_DATA0__CSPI_MISO				998
MX53_PAD_SD1_DATA0__CCM_PLL3_BYP			999
MX53_PAD_SD1_DATA1__ESDHC1_DAT1				1000
MX53_PAD_SD1_DATA1__GPIO1_17				1001
MX53_PAD_SD1_DATA1__GPT_CAPIN2				1002
MX53_PAD_SD1_DATA1__CSPI_SS0				1003
MX53_PAD_SD1_DATA1__CCM_PLL4_BYP			1004
MX53_PAD_SD1_CMD__ESDHC1_CMD				1005
MX53_PAD_SD1_CMD__GPIO1_18				1006
MX53_PAD_SD1_CMD__GPT_CMPOUT1				1007
MX53_PAD_SD1_CMD__CSPI_MOSI				1008
MX53_PAD_SD1_CMD__CCM_PLL1_BYP				1009
MX53_PAD_SD1_DATA2__ESDHC1_DAT2				1010
MX53_PAD_SD1_DATA2__GPIO1_19				1011
MX53_PAD_SD1_DATA2__GPT_CMPOUT2				1012
MX53_PAD_SD1_DATA2__PWM2_PWMO				1013
MX53_PAD_SD1_DATA2__WDOG1_WDOG_B			1014
MX53_PAD_SD1_DATA2__CSPI_SS1				1015
MX53_PAD_SD1_DATA2__WDOG1_WDOG_RST_B_DEB		1016
MX53_PAD_SD1_DATA2__CCM_PLL2_BYP			1017
MX53_PAD_SD1_CLK__ESDHC1_CLK				1018
MX53_PAD_SD1_CLK__GPIO1_20				1019
MX53_PAD_SD1_CLK__OSC32k_32K_OUT			1020
MX53_PAD_SD1_CLK__GPT_CLKIN				1021
MX53_PAD_SD1_CLK__CSPI_SCLK				1022
MX53_PAD_SD1_CLK__SATA_PHY_DTB_0			1023
MX53_PAD_SD1_DATA3__ESDHC1_DAT3				1024
MX53_PAD_SD1_DATA3__GPIO1_21				1025
MX53_PAD_SD1_DATA3__GPT_CMPOUT3				1026
MX53_PAD_SD1_DATA3__PWM1_PWMO				1027
MX53_PAD_SD1_DATA3__WDOG2_WDOG_B			1028
MX53_PAD_SD1_DATA3__CSPI_SS2				1029
MX53_PAD_SD1_DATA3__WDOG2_WDOG_RST_B_DEB		1030
MX53_PAD_SD1_DATA3__SATA_PHY_DTB_1			1031
MX53_PAD_SD2_CLK__ESDHC2_CLK				1032
MX53_PAD_SD2_CLK__GPIO1_10				1033
MX53_PAD_SD2_CLK__KPP_COL_5				1034
MX53_PAD_SD2_CLK__AUDMUX_AUD4_RXFS			1035
MX53_PAD_SD2_CLK__CSPI_SCLK				1036
MX53_PAD_SD2_CLK__SCC_RANDOM_V				1037
MX53_PAD_SD2_CMD__ESDHC2_CMD				1038
MX53_PAD_SD2_CMD__GPIO1_11				1039
MX53_PAD_SD2_CMD__KPP_ROW_5				1040
MX53_PAD_SD2_CMD__AUDMUX_AUD4_RXC			1041
MX53_PAD_SD2_CMD__CSPI_MOSI				1042
MX53_PAD_SD2_CMD__SCC_RANDOM				1043
MX53_PAD_SD2_DATA3__ESDHC2_DAT3				1044
MX53_PAD_SD2_DATA3__GPIO1_12				1045
MX53_PAD_SD2_DATA3__KPP_COL_6				1046
MX53_PAD_SD2_DATA3__AUDMUX_AUD4_TXC			1047
MX53_PAD_SD2_DATA3__CSPI_SS2				1048
MX53_PAD_SD2_DATA3__SJC_DONE				1049
MX53_PAD_SD2_DATA2__ESDHC2_DAT2				1050
MX53_PAD_SD2_DATA2__GPIO1_13				1051
MX53_PAD_SD2_DATA2__KPP_ROW_6				1052
MX53_PAD_SD2_DATA2__AUDMUX_AUD4_TXD			1053
MX53_PAD_SD2_DATA2__CSPI_SS1				1054
MX53_PAD_SD2_DATA2__SJC_FAIL				1055
MX53_PAD_SD2_DATA1__ESDHC2_DAT1				1056
MX53_PAD_SD2_DATA1__GPIO1_14				1057
MX53_PAD_SD2_DATA1__KPP_COL_7				1058
MX53_PAD_SD2_DATA1__AUDMUX_AUD4_TXFS			1059
MX53_PAD_SD2_DATA1__CSPI_SS0				1060
MX53_PAD_SD2_DATA1__RTIC_SEC_VIO			1061
MX53_PAD_SD2_DATA0__ESDHC2_DAT0				1062
MX53_PAD_SD2_DATA0__GPIO1_15				1063
MX53_PAD_SD2_DATA0__KPP_ROW_7				1064
MX53_PAD_SD2_DATA0__AUDMUX_AUD4_RXD			1065
MX53_PAD_SD2_DATA0__CSPI_MISO				1066
MX53_PAD_SD2_DATA0__RTIC_DONE_INT			1067
MX53_PAD_GPIO_0__CCM_CLKO				1068
MX53_PAD_GPIO_0__GPIO1_0				1069
MX53_PAD_GPIO_0__KPP_COL_5				1070
MX53_PAD_GPIO_0__CCM_SSI_EXT1_CLK			1071
MX53_PAD_GPIO_0__EPIT1_EPITO				1072
MX53_PAD_GPIO_0__SRTC_ALARM_DEB				1073
MX53_PAD_GPIO_0__USBOH3_USBH1_PWR			1074
MX53_PAD_GPIO_0__CSU_TD					1075
MX53_PAD_GPIO_1__ESAI1_SCKR				1076
MX53_PAD_GPIO_1__GPIO1_1				1077
MX53_PAD_GPIO_1__KPP_ROW_5				1078
MX53_PAD_GPIO_1__CCM_SSI_EXT2_CLK			1079
MX53_PAD_GPIO_1__PWM2_PWMO				1080
MX53_PAD_GPIO_1__WDOG2_WDOG_B				1081
MX53_PAD_GPIO_1__ESDHC1_CD				1082
MX53_PAD_GPIO_1__SRC_TESTER_ACK				1083
MX53_PAD_GPIO_9__ESAI1_FSR				1084
MX53_PAD_GPIO_9__GPIO1_9				1085
MX53_PAD_GPIO_9__KPP_COL_6				1086
MX53_PAD_GPIO_9__CCM_REF_EN_B				1087
MX53_PAD_GPIO_9__PWM1_PWMO				1088
MX53_PAD_GPIO_9__WDOG1_WDOG_B				1089
MX53_PAD_GPIO_9__ESDHC1_WP				1090
MX53_PAD_GPIO_9__SCC_FAIL_STATE				1091
MX53_PAD_GPIO_3__ESAI1_HCKR				1092
MX53_PAD_GPIO_3__GPIO1_3				1093
MX53_PAD_GPIO_3__I2C3_SCL				1094
MX53_PAD_GPIO_3__DPLLIP1_TOG_EN				1095
MX53_PAD_GPIO_3__CCM_CLKO2				1096
MX53_PAD_GPIO_3__OBSERVE_MUX_OBSRV_INT_OUT0		1097
MX53_PAD_GPIO_3__USBOH3_USBH1_OC			1098
MX53_PAD_GPIO_3__MLB_MLBCLK				1099
MX53_PAD_GPIO_6__ESAI1_SCKT				1100
MX53_PAD_GPIO_6__GPIO1_6				1101
MX53_PAD_GPIO_6__I2C3_SDA				1102
MX53_PAD_GPIO_6__CCM_CCM_OUT_0				1103
MX53_PAD_GPIO_6__CSU_CSU_INT_DEB			1104
MX53_PAD_GPIO_6__OBSERVE_MUX_OBSRV_INT_OUT1		1105
MX53_PAD_GPIO_6__ESDHC2_LCTL				1106
MX53_PAD_GPIO_6__MLB_MLBSIG				1107
MX53_PAD_GPIO_2__ESAI1_FST				1108
MX53_PAD_GPIO_2__GPIO1_2				1109
MX53_PAD_GPIO_2__KPP_ROW_6				1110
MX53_PAD_GPIO_2__CCM_CCM_OUT_1				1111
MX53_PAD_GPIO_2__CSU_CSU_ALARM_AUT_0			1112
MX53_PAD_GPIO_2__OBSERVE_MUX_OBSRV_INT_OUT2		1113
MX53_PAD_GPIO_2__ESDHC2_WP				1114
MX53_PAD_GPIO_2__MLB_MLBDAT				1115
MX53_PAD_GPIO_4__ESAI1_HCKT				1116
MX53_PAD_GPIO_4__GPIO1_4				1117
MX53_PAD_GPIO_4__KPP_COL_7				1118
MX53_PAD_GPIO_4__CCM_CCM_OUT_2				1119
MX53_PAD_GPIO_4__CSU_CSU_ALARM_AUT_1			1120
MX53_PAD_GPIO_4__OBSERVE_MUX_OBSRV_INT_OUT3		1121
MX53_PAD_GPIO_4__ESDHC2_CD				1122
MX53_PAD_GPIO_4__SCC_SEC_STATE				1123
MX53_PAD_GPIO_5__ESAI1_TX2_RX3				1124
MX53_PAD_GPIO_5__GPIO1_5				1125
MX53_PAD_GPIO_5__KPP_ROW_7				1126
MX53_PAD_GPIO_5__CCM_CLKO				1127
MX53_PAD_GPIO_5__CSU_CSU_ALARM_AUT_2			1128
MX53_PAD_GPIO_5__OBSERVE_MUX_OBSRV_INT_OUT4		1129
MX53_PAD_GPIO_5__I2C3_SCL				1130
MX53_PAD_GPIO_5__CCM_PLL1_BYP				1131
MX53_PAD_GPIO_7__ESAI1_TX4_RX1				1132
MX53_PAD_GPIO_7__GPIO1_7				1133
MX53_PAD_GPIO_7__EPIT1_EPITO				1134
MX53_PAD_GPIO_7__CAN1_TXCAN				1135
MX53_PAD_GPIO_7__UART2_TXD_MUX				1136
MX53_PAD_GPIO_7__FIRI_RXD				1137
MX53_PAD_GPIO_7__SPDIF_PLOCK				1138
MX53_PAD_GPIO_7__CCM_PLL2_BYP				1139
MX53_PAD_GPIO_8__ESAI1_TX5_RX0				1140
MX53_PAD_GPIO_8__GPIO1_8				1141
MX53_PAD_GPIO_8__EPIT2_EPITO				1142
MX53_PAD_GPIO_8__CAN1_RXCAN				1143
MX53_PAD_GPIO_8__UART2_RXD_MUX				1144
MX53_PAD_GPIO_8__FIRI_TXD				1145
MX53_PAD_GPIO_8__SPDIF_SRCLK				1146
MX53_PAD_GPIO_8__CCM_PLL3_BYP				1147
MX53_PAD_GPIO_16__ESAI1_TX3_RX2				1148
MX53_PAD_GPIO_16__GPIO7_11				1149
MX53_PAD_GPIO_16__TZIC_PWRFAIL_INT			1150
MX53_PAD_GPIO_16__RTC_CE_RTC_EXT_TRIG1			1151
MX53_PAD_GPIO_16__SPDIF_IN1				1152
MX53_PAD_GPIO_16__I2C3_SDA				1153
MX53_PAD_GPIO_16__SJC_DE_B				1154
MX53_PAD_GPIO_17__ESAI1_TX0				1155
MX53_PAD_GPIO_17__GPIO7_12				1156
MX53_PAD_GPIO_17__SDMA_EXT_EVENT_0			1157
MX53_PAD_GPIO_17__GPC_PMIC_RDY				1158
MX53_PAD_GPIO_17__RTC_CE_RTC_FSV_TRIG			1159
MX53_PAD_GPIO_17__SPDIF_OUT1				1160
MX53_PAD_GPIO_17__IPU_SNOOP2				1161
MX53_PAD_GPIO_17__SJC_JTAG_ACT				1162
MX53_PAD_GPIO_18__ESAI1_TX1				1163
MX53_PAD_GPIO_18__GPIO7_13				1164
MX53_PAD_GPIO_18__SDMA_EXT_EVENT_1			1165
MX53_PAD_GPIO_18__OWIRE_LINE				1166
MX53_PAD_GPIO_18__RTC_CE_RTC_ALARM2_TRIG		1167
MX53_PAD_GPIO_18__CCM_ASRC_EXT_CLK			1168
MX53_PAD_GPIO_18__ESDHC1_LCTL				1169
MX53_PAD_GPIO_18__SRC_SYSTEM_RST			1170
